SCOPE 40 ЛИ
Sofia, 15.05.2024

Ecoexpert 6 Ltd
Atmospheric air Testing laboratory

Management address: 9009 Varna, 1 Petko Staynov St., office 25
Laboratory address: 9009 Varna, 1 Petko Staynov St., office 27


To perform testing of:
	Type of the scope: flexible for a part of the scope

	№
	Tested products
	Type of test / characteristics
	Test methods
(standard/validated method)

	1
	2
	3
	4

	1.
	Stationary sourses emissions in atmospheric air / Gas streams
	1.1. Dust
	БДС ISO 9096
БДС EN 13284-1

	
	
	1.2. Velocity (average gas velocity
	ISO 10780
БДС ISO 9096

	
	
	1.3. Volume flow (quantity) of the gas
	

	
	
	1.4. Temperature (air temperature, stack gas temperature)
	

	
	
	1.5. Pressure (barometric pressure, stack gas pressure, stack gas subpressure)
	

	
	
	1.6. Carbon dioxide (CO2)
	VVLM 1/2015

	
	
	1.7. Carbon monoxide (CO)
	

	
	
	1.8. Nitrogen oxide (NO)
	

	
	
	1.9. Nitrogen dioxide (NO2)
	

	
	
	1.10. Nitrogen oxides (NOx) (expressed as nitrogen dioxide)
	

	
	
	1.11. Sulfur dioxide (SO2)
	

	
	
	1.12. Oxygen (O2)
	

	
	
	1.13. Methane (CH4)
	

	
	
	1.14. Hydrogen sulfide (H2S)
	

	
	
	1.15. Total hydrocarbons (CxHy) and volatile organic compounds (VOC);
	VVLM 2/2013

	
	
	1.16. Total Carbon (TOC)
	

	
	
	1.17. Ammonia (NH3)
	VVLM 3/2016

	
	
	1.18. Water vapor (moisture), relative humidity of the gas
	БДС EN 14790 
VVLM 1/2015

	2.
	Environmental noise
	Equivalent noise level, total sound power level
	БДС ISO 8297
БДС 15471
VVLM 4/2016




To perform sampling of:
	Type of the scope: Flexible

	№
	Product
	Sampling methods (standardized/validated)

	1
	2
	3

	1.
	Stationary sources emissions in atmospheric air / Gas streams
	БДС ISO 9096 
БДС EN 13284-1 
БДС EN 14790



Flexible scope: Implementing a new version of standards or standards replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.


Fixed scope references:
VVLM 1/2015 - Sampling and automatic determination of concentrations of stationary sources gas emissions - carbon monoxide, carbon dioxide, nitrogen oxide, nitrogen dioxide, nitrogen oxides (expressed as nitrogen dioxide), sulfur dioxide, oxygen, methane, hydrogen sulfide.
VVLM 2/2013 - Sampling and determination of total hydrocarbons and volatile organic compounds, expressed as total carbon in stationary sources emissions.
VVLM 3/2016 - Sampling and automatic determination of ammonia in emissions from stationary sources.
VVLM 4/2016 - Measurement of equivalent noise levels. Determination до the total sound power emitted into the environment by an industrial plant and the noise levels at the point of inpact.
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