
SCOPE 140 ЛИ
Sofia, 25.09.2024
REGIONAL HEALTH INSPECTORATE - STARA ZAGORA 
LABORATORY TESTING COMPLEX 

Management and laboratory address: 
6000 Stara Zagora, Stara Zagora Municipality, 10 Stefan Karadzha Str.

To perform testing of:
	Type of the scope: flexible for a part of the scope*

	№
	Tested Products
	Type of test/ Characteristic
	Testing methods
(standard/ validated method)

	1
	2
	3
	4

	1.
	Bottled natural, mineral (1), 
spring and table water (2);














	Total count of aerobic mesophilic and facultative anaerobic microorganisms at 22° and 37°C
	БДС EN ISO 6222 (1), (2)

	
	
	Coliform
	БДС EN ISO 9308-1/A1 (1), (2)

	
	
	Escherichia coli
	БДС EN ISO 9308-1/A1 (1), (2)

	
	
	Enterococcus (E. faecium)/ Faecalis Streptococcus
	БДС EN ISO 7899-2 (1), (2)

	
	
	Sulfite-reducing Clostridia/
Clostridium perfringens
	БДС EN 26461-2 (1), (2)
БДС EN ISO 14189 (1), (2)

	
	
	Pseudomonas aeruginosa
	БДС EN ISO 16266 (1), (2)

	
	
	pH
	БДС EN ISO 10523 (2)

	
	
	Aluminum
	БДС EN ISO 17294-2 (2)

	
	
	Ammonium ions
	БДС EN ISO 14911 (2)

	
	
	Antimony
	БДС ISO 17378-2 (1), (2)
БДС EN ISO 17294-2 (1), (2)

	
	
	Arsenic
	БДС ISO 17378-2 (1), (2)
БДС EN ISO 17294-2 (1), (2)

	
	
	Barium
	БДС EN ISO 17294-2 (1)

	
	
	Boron
	БДС EN ISO 17294-2 (1), (2)

	
	
	Bromates
	ISO 15061 (2)

	
	
	Electrical conductivity
	БДС EN 27888 (2)

	
	
	Iron
	БДС EN ISO 17294-2 (2)

	
	
	Mercury
	ВЛМ №1/2016 (1), (2)
БДС EN ISO 17294-2 (1), (2)

	
	
	Cadmium
	БДС EN ISO 15586 (1), (2) 
БДС EN ISO 17294-2 (1), (2)

	
	
	Calcium
	БДС ISO 6058 (2)

	
	
	Magnesium
	ВЛМ № 3/2024 (2)

	
	
	Manganese
	БДС ISO 6333 (1), (2)
БДС EN ISO 17294-2 (1), (2)

	
	
	Copper
	ISO 8288, A (1), (2)
БДС EN ISO 17294-2 (1), (2)

	
	
	Turbidity
	БДС EN ISO 7027-1 (2)

	
	
	Sodium
	БДС ISO 9964-3 (2)
БДС EN ISO 14911 (2)

	
	
	Nickel
	БДС EN ISO 15586 (1), (2)
БДС EN ISO 17294-2 (1), (2)

	
	
	Nitrates
	БДС ISO 7890-3 (1), (2)
БДС EN ISO 10304-1 (1), (2)

	
	
	Nitrites
	БДС EN 26777 (1), (2)
БДС EN ISO 10304-1 (1), (2)

	
	
	Total hardness
	БДС ISO 6059 (2)

	
	
	Lead
	БДС EN ISO 15586 (1), (2)
БДС EN ISO 17294-2 (1), (2)

	
	
	Permanganate oxidizability
	БДС EN ISO 8467 (2)

	
	
	Selenium
	ISO/TS 17379-2 (1), (2)
БДС EN ISO 17294-2 (1), (2)

	
	
	Sulfates
	БДС EN ISO 10304-1 (2)

	
	
	Uranium natural
	БДС EN ISO 17294-2 (2)

	
	
	Fluorides
	БДС EN ISO 10304-1 (1), (2)

	
	
	Phosphates
	БДС EN ISO 10304-1 (2)

	
	
	Chlorides
	ISO 9297 (2)
БДС EN ISO 10304-1 (2)

	
	
	Chromium
	БДС EN ISO 17294-2 (1), (2)

	
	
	Zinc
	ISO 8288, A (2)
БДС EN ISO 17294-2 (2)

	
	
	Trihalomethanes (total)*, 
as amount of: 
chloroform, bromoform, 
dibromochloromethane, bromodichloromethane
	БДС EN ISO 10301, cl. 3 (2)

	
	
	1,2-dichloroethane
	БДС EN ISO 10301, cl. 3 (2)

	
	
	Tetrachloroethylene and trichloroethylene (total)
	БДС EN ISO 10301, cl. 3 (2)

	
	
	Benzene
	БДС ISO 11423-1 (2)

	
	
	Pesticides:*
	БДС EN ISO 6468 (2)
БДС EN 12918 (2) Annex B

	
	
	Pesticides (total)*, as amount of concentrations of all individual pesticides
	БДС EN ISO 6468 (2)
БДС EN 12918 (2) Annex B

	2.
	Surfaces testing for determining hygiene status
	Total count of microorganisms
	БДС EN ISO 4833-1/A1

	
	
	Coliform
	ISO 4832

	
	
	Staphylococcus aureus
	БДС EN ISO 6888-1/A1

	
	
	Salmonella spp.
	БДС EN ISO 6579-1/A1

	
	
	Listeria monocytogenes
	БДС EN ISO 11290-1, cl. 9.5.2

	3.
	Water intended for drinking and household purposes
	Total count of microorganisms at 22°C and 37°C
	БДС EN ISO 6222

	
	
	Coliform
	БДС EN ISO 9308-1/A1;
БДС 17336, cl. 1.1

	
	
	Escherichia coli
	БДС EN ISO 9308-1/A1;
БДС 17336, cl. 1.3

	
	
	Enterococcus
	БДС EN ISO 7899-2; 
БДС 17335, cl. 1.4

	
	
	Legionella
	БДС EN ISO 11731

	
	
	Sulfite-reducing Clostridia / Clostridium perfringens
	БДС EN 26461-2
БДС EN ISO 14189

	
	
	Color
	БДС 8451

	
	
	Taste
	БДС 8451, cl. 3.3

	
	
	Odor
	БДС 8451, cl. 4.3.1

	
	
	Turbidity
	БДС EN ISO 7027-1

	
	
	Active reaction (pH)
	БДС EN ISO 10523

	
	
	Aluminum
	БДС ISO 10566
БДС EN ISO 17294-2

	
	
	Ammonium ions
	БДС ISO 7150-1
БДС EN ISO 14911

	
	
	Antimony
	БДС ISO 17378-2
БДС EN ISO 17294-2

	
	
	Arsenic
	БДС ISO 17378-2
БДС EN ISO 17294-2

	
	
	Boron
	БДС ISO 9390
БДС EN ISO 17294-2

	
	
	Bromates
	ISO 15061

	
	
	Electrical conductivity
	БДС EN 27888

	
	
	Iron
	БДС ISO 6332
БДС EN ISO 17294-2

	
	
	Mercury
	ВЛМ №1/2016
БДС EN ISO 17294-2

	
	
	Cadmium
	БДС EN ISO 15586
БДС EN ISO 17294-2

	
	
	Calcium
	БДС ISO 6058

	
	
	Magnesium
	ВЛМ № 3/2024

	
	
	Manganese
	БДС ISO 6333
БДС 3559
БДС EN ISO 17294-2

	
	
	Copper
	ISO 8288, A
БДС EN ISO 17294-2

	
	
	Sodium
	БДС ISO 9964-3
БДС EN ISO 14911

	
	
	Nickel
	БДС EN ISO 15586
БДС EN ISO 17294-2

	
	
	Nitrates
	БДС ISO 7890-3
БДС 3758
БДС EN ISO 10304-1

	
	
	Nitrites
	БДС EN 26777
БДС EN ISO 10304-1

	
	
	Total hardness
	БДС 3775
БДС ISO 6059

	
	
	Lead
	БДС EN ISO 15586
БДС EN ISO 17294-2

	
	
	Permanganate oxidizability
	БДС 3413 
БДС EN ISO 8467

	
	
	Selenium
	ISO/TS 17379-2
БДС EN ISO 17294-2

	
	
	Sulfates
	БДС 3588 cl. 5
БДС EN ISO 10304-1

	
	
	Dry residue
	БДС 3546

	
	
	Uranium natural
	БДС EN ISO 17294-2

	
	
	Fluorides
	БДС 16911 cl. 1
БДС EN ISO 10304-1

	
	
	Phosphates
	БДС EN ISO 6878, cl.4
БДС EN ISO 10304-1

	
	
	Chlorides
	БДС 3414
ISO 9297
БДС EN ISO 10304-1

	
	
	Chromium
	БДС 7212
БДС EN ISO 17294-2

	
	
	Cyanides
	БДС 7214;

	
	
	Zinc
	ISO 8288,
БДС EN ISO 17294-2

	
	
	Trihalomethanes (total)*, as amount of: chloroform, bromoform, dibromochloromethane, 
bromodichloromethane
	БДС EN ISO 10301, cl. 3

	
	
	1,2-dichloroethane
	БДС EN ISO 10301, cl. 3

	
	
	Tetrachloroethylene and trichloroethylene (total)
	БДС EN ISO 10301, cl.3

	
	
	Benzene
	БДС ISO 11423-1

	
	
	Pesticides:*
	БДС EN ISO 6468;
БДС EN 12918 Annex B

	
	
	Pesticides (total)*, as amount of concentrations of all individual pesticides
	БДС EN ISO 6468;
БДС EN 12918, Annex B

	4.
	Water from swimming pools
	Total count of microorganisms at 37°C
	БДС 17335

	
	
	Total Colli titer
	БДС 17335

	
	
	Escherichia colli titer
	БДС 17335

	
	
	Staphylococcus titer
	БДС 17335

	
	
	Enterococcus titer
	БДС 17335

	
	
	Active reaction (pH)
	БДС EN ISO 10523

	
	
	Ammonium ions
	БДС ISO 7150-1
БДС EN ISO 14911

	
	
	Iron
	БДС ISO 6332
БДС EN ISO 17294-2

	
	
	Manganese
	БДС ISO 6333
БДС EN ISO 17294-2

	
	
	Nitrites
	БДС EN 26777
БДС EN ISO 10304-1

	
	
	Permanganate oxidizability
	БДС EN ISO 8467

	5.
	Mineral water at water sources used for drinking and medicinal purposes
	Total count of aerobic mesophilic microorganisms
· at 20°C to 22°C for 72 hours
· at 37°C for 24 hours
	БДС EN ISO 6222

	
	
	Coliform at 37°C
	БДС EN ISO 9308-1/А1;
БДС 17336, cl. 1.1

	
	
	Escherichia colli
	БДС EN ISO 9308-1/А1;
БДС 17336, cl. 1.3

	
	
	Enterococcus
	БДС EN ISO 7899-2; 
БДС 17335, cl. 1.4

	
	
	Pseudomonas aeruginosa
	БДС EN ISO 16266; 
БДС 17335, cl. 1.7

	
	
	Sulfitc-rcducing Clostridia/
Clostridium perfringens
	БДС EN 26461-2;
БДС EN ISO 14189

	6.
	Ground water
	Active reaction (pH)
	БДС EN ISO 10523

	
	
	Aluminum
	БДС ISO 10566

	
	
	Ammonium ions
	БДС ISO 7150-1

	
	
	Arsenic
	БДС ISO 17378-2

	
	
	Boron
	БДС ISO 9390

	
	
	Electrical conductivity
	БДС EN 27888

	
	
	Iron
	БДС ISO 6332

	
	
	Cadmium
	БДС EN ISO 15586

	
	
	Calcium
	БДС ISO 6058

	
	
	Magnesium
	ВЛМ № 3/2024

	
	
	Manganese
	БДС ISO 6333

	
	
	Copper
	ISO 8288, A

	
	
	Nickel
	БДС EN ISO 15586

	
	
	Nitrates
	БДС ISO 7890-3

	
	
	Nitrites
	БДС EN 26777

	
	
	Total hardness
	БДС ISO 6059

	
	
	Lead
	БДС EN ISO 15586

	
	
	Permanganate oxidizability
	БДС EN ISO 8467

	
	
	Phosphates
	БДС EN ISO 6878, cl. 4

	
	
	Chlorides
	ISO 9297

	
	
	Zinc
	ISO 8288, A

	7.
	Cosmetic products
	Total count of heterotrophic mesophilic micro flora,
	БДС 3741, cl. 11;
БДС 10751, cl. 12;
БДС EN ISO 21149/A1

	
	
	Yeasts and moulds
	БДС EN ISO 16212/A1

	
	
	Escherichia coli
	БДС EN ISO 21150/A1

	
	
	Staphylococcus aureus
	БДС 10751, cl.3
БДС EN ISO 22718/A1

	
	
	Candida albicans
	БДС EN ISO 18416/A1

	
	
	Pseudomonas aeruginosa
	БДС EN ISO 22717/A1

	
	
	Active reaction pH
	БДС 3741, cl. 10;
БДС EN 1262

	
	
	Determination of lead content in cosmetic products
	Compendium of methods for hygiene researches of NCHMEN, 2002, vol. IV; 
СД ISO/TR 17276, Annex C

	
	
	Determination of cadmium content in cosmetic products
	Compendium of methods for hygiene researches of NCHMEN, 2002, vol. IV;
СД ISO/TR 17276, Annex C

	
	
	Determination of arsenic content in cosmetic products
	СД ISO/TR 17276, Annex C

	
	
	Moisture and volatile matter content
	БДС ISO 672;
БДС 3741, cl. 4

	
	
	Identification and determination of formaldehyde
	Ordinance № 14, SG № 68/ 2014, Annex №2, item XI

	
	
	Determination of ammonia
	Ordinance № 14, SG № 68/ 2014, Annex № 2, item XVI; БДС 10751, cl. 4.7

	8.
	Products intended to come into direct and prolonged contact with the skin
	Nickel content
	БДС EN 1811




To perform sampling of:
	Type of the scope: flexible

	№ 
	Product 
	Sampling method 
(standardized/ validated)

	1
	2
	3

	1.
	Water:
- Water intended for drinking and household purposes (1);
- Water from swimming pools (2);
- Mineral waters at water sources used for drinking and medicinal purposes (3);
- Bottled natural, mineral, spring and table water (4)
	
БДС EN ISO 19458 (1), (2), (3)
БДС 17335 (2),
БДС ISO 5667-5 (1),
БДС EN ISO 5667-14 (3), (4)



Flexible scope: Implementing a new version of standards/documents or standards/ documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by the CAB.

*Within the framework of its competence, the laboratory is authorised to determine the products marked with ”*" (column 2) by characteristics (column 3), according to the test methods (column 4 and an up-to- date list of standards with their dated versions), after carry ing out verification (or validation), provision of CRM/RM relevant characteristics and calibrated technical means. The laboratory maintains a detailed, dated list of products belonging to those mentioned in the scope of accreditation.


Flexible scope references:
1. Compendium of methods for hvgiene researches, Vol. IV Sofia 2002 (NCHMEN) - Compendium of methods for hygiene researches, Vol. IV, Sofia, 2002, National Center of Hygiene, Medical Ecology and Nutrition.	
2. Ordinance № 14, SG № 68/2014 - To determine detailed rules for presenting the information under Art 19, para. 4 of Regulation (EC) № 1223/2009 regarding cosmetic products, requirements for the effectiveness of sunscreen cosmetic products and chemical methods for verifying the composition of cosmetic products, Annex № 2, items XI and XVI.

 Fixed scope reference:
ВЛМ № 1/2016 - Determination of mercury in water. Method using hydride generation atomic absorption spectrometry (HG-AAS).
BJIM № 3/2024 - Water quality. Determination of magnesium by calculation method.
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