SCOPE 168 ЛИ
Sofia, 08.11.2024

ROAD LABORATORY 
at PATPERFEKT-T EAD
[bookmark: bookmark8]Management address: 7500 Silistra, 199 Makedoniya Blvd. 
Laboratory address: 7610 Zafirovo, Silistra Region, Asphalt Base 

To perform testing of: 
	Type of the scope: flexible

	№ 
	Tested products
	Type of test / characteristic
	Testing methods
(standard/ validated method)

	 1
	                   2
	                               3
	                 4

	I. 
	Rocky materials
	I.1. Grain metric composition. 

	БДС EN 933-1
БДС EN 1367-2

	
	
	I.3. Density in bulk.
	БДС EN 1097-3

	
	
	I.4. Water content. 
	БДС EN 1097-5

	
	
	I.5. Sand equivalent.
	БДС EN 933-8+A1

	
	
	I.6. Flat grain common index.
	БДС EN 933-3

	
	
	I.7. Form ratio (coefficient) 
	БДС EN 933-4

	
	
	I.8. Grain density Pa, Prd, Pssd and water absorption.
	БДС EN 1097-6


	II.
   
	Asphalt mixtures 
	II.1. Bulk density of asphalt test specimens. 
	БДС EN 12697-6

	
	
	II.2. Maximum density.
	БДС EN 12697-5

	
	
	II.3. Content of air pores in asphalt test specimens. 
	БДС EN 12697-8

	
	
	II.4. Marshall test
-stability
-proceeding
	БДС EN 12697-34

	
	
	II.5. Soluble binder content.
	БДС EN 12697-1

	
	
	II.6. Distribution of particles size 
(grain size composition). 
	БДС EN 12697-2+A1

	
	
	II.7. Asphalt mixture temperature.
	БДС EN 12697-13

	
	
	II.8. Asphalt pavement thickness.
	БДС EN12697-36 cl.6.1

	
	
	II.9. Degree of compaction.
	БДС EN 12697-9*

	III.
	Bitumen
	III.1. Needle penetration.  
	БДС EN 1426

	
	
	III.2. Softening temperature.
	БДС EN 1427

	IV.
	Construction soils
	IV.1. Water content. 
	БДС EN 1097-5

	
	
	IV.2. Maximum bulk density at optimal water content. 
	БДС EN 13286-2

	
	
	IV.3. Grain metric composition. 
	БДС EN 933-1

	
	
	IV.4. Soil density in place by sand cone method. 
	AASHTO T 191

	
	
	IV.5. Elastic Module. 
Deformation Modules, E1, E2, E3.
Relation of deformation modules E2/E1.
	БДС 15130



	V.
	Concrete. 
	V.1. Compressive strength.
	БДС EN 12390-3



  To perform sampling of:
	Type of the scope: fiexible

	№
	Product 
	Sampling methods
(standard / validated)

	1
	2
	3

	1.
	Rocky materials
	БДС EN 932-1, cl. 8.8.

	2.
	Asphalt mixtures
	БДС EN 12697-27, cl. 4.1, cl. 4.7

	3.
	Bitumen
	БДС EN 58, cl.  8.2.2

	4.
	Construction soils
	БДС 17146, cl. 5, 
БДС EN 13286-1



*Repealed but not replaced standard with regard to the testing method.

Flexible scope: Implementing a new version of standards/documents or standards / documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.
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