SCOPE 203 ЛИ
PATINZHENERING-M EAD
ROAD LABORATORY
Management address: 3400 Montana, 24 Graf Ignatiev Str.
Laboratory address: 3440 Vladimirovo, Boychinovtsi Municipality,
Land plot with Identifier: 11418.853.325

To perform testing of:
	Type of the scope: flexible

	№
	Tested Products
	Type of Test/Characteristic
	Testing methods
(standardized / validated methods)

	1
	2
	3
	4

	I.
	Rock materials
	1. Content of fine particles of                             size less than 0.063 mm
	БДС EN 933-1

	
	
	2. Grain structure composition
	БДС EN 933-1

	
	
	3. Index of flat grains
	БДС EN 933-3

	
	
	4. Form factor
	БДС EN 933-4

	
	
	5. Percentage of:
· partially broken grains
· fully crushed grains
· fully rounded grains
	БДС EN 933-5

	
	
	6. Shell content
	БДС EN 933-7

	
	
	7. Sand equivalent
	БДС EN 933-8+A 1

	
	
	8. Bulk bulk density
	БДС EN 1097-3

	
	
	9. Water content
	БДС EN 1097-5

	
	
	10. Absorption
	БДС EN 1097-6, 
cl. 7, cl. 8, cl. 9

	
	
	11. Grain density:
· apparent grain density
· dry grain density
· grain density in water- saturated
surface dry state
	БДС EN 1097-6, 
cl. 7, cl. 8, cl. 9

	
	
	
	

	
	
	12. Resistance in magnesium                           sulphate solution
	БДС EN 1367-2

	II.
	Bitumens and    bituminous binders
	1. Penetration
	БДС EN 1426

	
	
	2. Softening temperature
	БДС EN 1427

	
	
	3. Extensibility
	ST of Comecon 4542

	
	
	4. Adhesion
	БДС 11685

	
	
	5. Elastic recovery
	БДС EN 13398

	
	
	6. Density
	БДС EN 15326+A 1

	III.
	Asphalt mixtures
	1. Soluble binder content
	БДС EN 12697-1 
Annex   B, cl. B.2.1

	
	
	2. Particle size distribution 
	БДС EN 12697-2+A 1

	
	
	3. Maximum density 
	БДС EN 12697-5

	
	
	4. Bulk density of asphalt test                        bodies
	БДС EN 12697-6

	
	
	5. Content of air pores 
	БДС EN 12697-8

	
	
	6. Pore volume in the mineral                     part 
	БДС EN 12697-8

	
	
	7. Conditional comparative                    density
	БДС EN 12697-9*

	
	
	8. Sensitivity to water 
	БДС EN 12697-12

	
	
	9. Asphalt mixture temperature
	БДС EN 12697-13

	
	
	10. Marshall Stability 
	БДС EN 12697-34

	
	
	11. Marshall flow (Conditional     plasticity)
	БДС EN 12697-34

	
	
	12. Thickness of asphalt                pavements
	БДС EN 12697-36, 
cl. 6.1

	
	
	13. Asphalt Test Body Size
	БДС EN 12697-29

	
	
	14. Degree of compaction of             asphalt pavement
	БДС EN 12697-9*

	
	
	15. Indirect tensile strength
	БДС EN 12697-23

	IV.
	Construction soils
	1. Grain structure composition
	БДС EN 933-1

	
	
	2. Limit of flow.
Drainage limit. 
Plasticity index.
	AASHTO T 89
AASHTO T 90

	
	
	3. Density of soils in place by the        Sand-Cone Method
	AASHTO T 191

	
	
	4. Maximum bulk density at           optimum water content by Proctor                           method
	БДС EN 13286-2, cl. 7.1, cl. 7.2, cl. 7.4, cl. 7.5

	
	
	5. Elastic and deformation modulus.      Ratio of deformation                                      modules E2/E1
	БДС 15130

	
	
	6. Optimum water content
	БДС EN 13286-2

	V.
	Road structures
	1. Roughness of road structures
	БДС EN 13036-7

	
	
	2. Road surface roughness
	БДС 17143 cl. 5.7



To perform sampling of: 
	Type of the scope: flexible

	№
	Product
	Sampling methods
(standardized /validated)

	1
	2
	3

	1.
	Rock materials.
	БДС EN 932-1

	2.
	Mineral flour for asphalt concrete mixtures
	БДС EN 932-1

	3.
	Bitumens and bituminous binders
	БДС EN 58

	4.
	Asphalt mixtures
	БДС EN 12697-27

	5.
	Construction soils
	БДС EN 13286-1



Flexible scope: Implementing a new version of standards/documents or standards / documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by the laboratory.
Note: *Repealed but not replaced standards with regard to the testing method.

52 А “Dr. G. M. Dimitrov” Blvd. 1797 Sofia Bulgaria
phone: +359 2 9766 401; fax: +359 2 873 53 02
e-mail: office@nab-bas.bg; web: www.nab-bas.bg
EA BAS                                          10.12.2024                                    Page 42 of 43
