SCOPE 188 ЛИ
Sofia, 15.05.2026
BUILD LAB LTD.
ROAD CONSTRUCTION TESTING LABORATORY, MRAMOR

Management address: 1261, Mramor, 96, Vasil Levski Str.
Laboratory address: 1261, Mramor, 96, Vasil Levski Str.

To perform testing of:
	Type of the scope: flexible*

	№
	Tested Products
	Type of test/ Characteristic
	Testing methods
(standard/ validated method)

	1
	2
	3
	4

	1.
	Bituminous mixtures









	1.1. Soluble binder content
	БДС EN 12697-1, 
Annex В, cl. 1.7

	
	
	1.2. Particle size distribution 
	БДС EN 12697-2

	
	
	1.3. Maximum density
	БДС EN 12697-5, 
Procedure А

	
	
	1.4. Bulk density
	БДС EN12697-6, 
Procedures А, В, D

	
	
	1.5. Air void characteristics
	БДС EN 12697-8, cl. 4

	
	
	1.6. Degree of compaction 
	**БДС EN 12697-9

	
	
	1.7. Marshall test (strength; conditional plasticity)
	БДС EN 12697-34

	
	
	1.8. Dimensions of a bituminous specimen
	БДС EN 12697-29

	
	
	1.9. Affinity between aggregate and bitumen (degree of retention of the bituminous coating)
	БДС EN 12697-11, cl. 7

	2.
	Bitumen
	2.1. Penetration of the reminder at 25°С
	БДС EN 1426

	
	
	2.2. Softening point 
- Ring and Ball method
	БДС EN 1427

	3.









	Construction soils (1) 
/Rock materials (2) 
/Unbound and hydraulically bound mixtures (3)









	3.1. Particle size distribution
	БДС EN 933-1 (2) (3);
БДС EN ISO 17892-4, cl.5.2 (2), (3)

	
	
	3.2. Fine fraction (material passing through a sieve with openings 0,063 mm)
	БДС EN 933-1 (2), (3)

	
	
	3.3. Flakiness index
	БДС EN 933-3 (2), (3)

	
	
	3.4. Shape index
	БДС EN 933-4 (2), (3)

	
	
	3.5. Content of:
- completely crushed grains,
- crushed grains,
- totally rounded grains
	БДС EN 933-5 (2)

	
	
	3.6. Sand equivalent value

	БДС EN 933-8+А1 (2), (3)

	
	
	3.7. Methylene blue value
	БДС EN 933-9 (2), (3)

	
	
	3.8. Loose bulk density
	БДС EN 1097-З (2), (3)

	
	
	3.9. Water content
	БДС EN 1097-5 (2), (3);
БДС EN ISO 17892-1+А1 (1)

	
	
	3.10. Particle density:
- particle mass density,
- bulk density of particles in
dry condition,
- bulk density of particles in
saturated surface-dry condition,
- pre-dried particle mass density,
- bulk density of watersaturated
particles to a constant mass
	БДС EN 1097-6, (2) 
cl. 7, cl. 8, cl. 9, 
Annex А (2),
cl. А.З Annex А (2), 
cl. A.4 Annex В (2)

	
	
	3.11. Water absorption
	БДС EN 1097-6, 
cl. 7; cl. 8, cl. 9 
Annex В (2)

	
	
	3.12. Stability in Мg2SO4
solution
	БДС EN 1367-2 (2)

	
	
	3.13. Humus content

	БДС EN 1744-1+А1, cl. 15.1 (2)

	
	
	3.14. Determination of an elastic
modulus using a circular loading
plate
	БДС 15130 (1)

	
	
	3.15. Determination of an
deformation modulus using a
circular loading plate
	БДС 15130 (1)

	
	
	3.16. Ratio of the modules of
deformation Е2:Е1 using a
circular loading plate
	БДС 15130 (1)

	
	
	3.17. Maximum Dry Density
(Proctor)
	БДС EN 13286-2, cl. 7.1, 
cl. 7.2, cl. 7.4, cl. 7.5
(1), (2), (3)
БДС 17146, cl. 3.3.1, 
cl. 3.3.2 (1), (2), (3)

	
	
	3.18. Optimal moisture content
	БДС EN 13286-2, cl. 7.1, 
cl. 7.2, cl.7.4, cl. 7.5 
(1), (2), (3);
БДС 17146, cl.3.3.1, 
cl. 3.3.2 (1), (2), (3)

	
	
	3.19. Dry density determined by
the sand replacement method
	Annex № 18 to Art. 168, item 1 of Ordinance № РД-02-20-2, SG 79/2018 (1), (2), (3)

	
	
	3.20. Degree of compaction
	Annex № 18** to Art. 168, item 1 of Ordinance № РД-02-20-2, SG 79/2018 (1), (2), (3)

	
	
	3.21. Compressive strength
	БДС EN 13286-41 (3)

	
	
	3.22. Aggregate’s resistance to
fragmentation – Los Angeles
(LA) coefficient
	БДС EN 1097-2 (2)

	
	
	3.23. California Bearing Ratio
(CBR)
	БДС EN 13286-47 (1), (2), (3)

	
	
	3.24. Linear swelling
	БДС EN 13286-47 (1), (2), (3)

	
	
	3.25. Liquid limits 
	БДС EN 17892-12, 
Casagrande method (1), (2);
Annex № 15 to Art. 160, item 3 of Ordinance № РД-02-02-2, SG 79/2018 (1), (2)

	
	
	3.26. Plastic limits
	БДС EN 17892-12 (1), (2);
Annex № 16 to art. 160, item 3 of Ordinance № РД-02-02-2, SG 79/2018 (1), (2)

	
	
	3.27. Plasticity index
	БДС EN 17892-12 (1), (2);
Annex № 16 to Art. 160, item 3 of Ordinance № РД-02-02-2, SG 79/2018 (1), (2)

	4.




	Mineral filler (fine filler)
	4.1. Particle size distribution
	БДС EN 933-1

	
	
	4.2. Methylene blue value
	БДС EN 933-9

	
	
	4.3. Water content
	БДС EN 1097-5

	
	
	4.4. Particles density
	БДС EN 1097-7

	5.
	Grout for prestressing
tendons (elements)
	5.1. Compressive strength
	БДС EN 445, cl. 4.6; 
БДС EN 196-1

	6.
	Grouted anchors
	6.1. Load-bearing capacity of
anchors: elongation/
displacement at a given tensile
load
	БДС EN ISO 22477-5, cl. 10.4

	7.
	Waterproofing systems
	7.1. Tensile adhesion to concrete
substrate
	БДС EN 13596

	8.
	Road pavements
	8.1. Deflection (Benkelman beam
method)
	БДС EN 15131

	9.
	Concrete mixtures
	9.1. Slump-test
	БДС EN 12350-2

	10.
	Hardened concrete 
	10.1. Compressive strength
	БДС EN 12390-3

	
	
	10.2. Compressive strength of core specimens drilled from
concrete test cylinders
	БДС EN 12504-1

	11.
	Shotcrete
	11.1. Compressive strength
of early-age shotcrete
	БДС EN 14488-2, Method A: needle penetration



To perform sampling of:
	Type of the scope: flexible* 

	№
	Product
	Sampling methods
(standard/ validated method)

	1
	2
	3

	1.
	Bituminous mixtures
	БДС EN 12697-27, 
cl. 4.1, cl. 4.3, cl. 4.4, cl. 4.6, cl. 4.7

	2.
	Bitumen
	БДС EN 58, cl. 8.1, cl.  8.2.1

	3.
	Construction soils (1) 
/Rock materials (2) 
/Unbound and hydraulically bound mixtures (3)
	БДС EN 932-1 (1) (2), (3)

	4.
	Mineral filler (fine filler)
	БДС EN 932-1, cl. 8.3, cl. 8.4, cl. 8.5, cl. 8.7

	5.
	Concrete mixtures
	БДС EN 12350-1

	6.
	Hardened concrete
	БДС EN 12504-1



** БДС EN 12697-9 - Repealed but not replaced standard with regard to the testing method.

*Flexible scope: Implementing a new version of standards/documents or standards/ documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by the laboratory.

Reference:
Annex № 15 to Art. 160, item 3 of Ordinance № РД-02-20-2, SG 79/2018 - Method for determining the liquid limit of soil.

Annex № 16 to Art. 160, item 3 of Ordinance № РД-02-20-2, SG 79/2018 - Method for determining the plastic limit and plasticity index of soil.

Annex № 18 to Art. 160, item 1 of Ordinance № РД-02-20-2, SG 79/2018 - Method for determining the in-situ bulk density of construction soils using sand replacement method.
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