SCOPE 69 ЛИ
Sofia, 02.05.2025
VODOSNABDYAVANE I KANALIZATSIYA OOD, PERNIK 
TESTING LABORATORY COMPLEX
Management address: 2300 Pernik, 11, Sredets Str.
Laboratory addresses: Office 1 Pernik: 2308 Pernik, PSPV-Pernik
      Office 2 Batanovtsi: 2340 Batanovtsi, GPSOV

Office 1 PSPV-Pernik:
To perform testing of:
	Type of the Scope:  Flexible for part of the scope

	№ 
	Tested products
	Type of test / characteristic
	Testing methods
(standard / validated method)

	1
	2
	3
	4

	1.
	Potable Water (1)
Surface Water (2)
Underground Water (3)
	1.1  Color
	БДС 8451, clause 2 (1)                                

	
	
	1.2  Smell
	БДС 8451, cl. 4 (1)

	
	
	1.3  Taste
	БДС 8451, cl. 3 (1)

	
	
	1.4 Теmperature
	БДС 8451, cl. 5 (1)

	
	
	1.5 Specific Electrical 
       Conductivity 
	БДС EN 27888 (1,2,3)

	
	
	1.6  Total Hardness 
	БДС ISO 6059 (1,2,3)

	
	
	1.7  Аctive Reaction
	БДС 3424, cl. 1 (1)
БДС 17.1.4.27, cl. 1 (2,3)

	
	
	1.8 Permanganate  
      Oxidation
	БДС 3413 (1)
БДС 17.1.4.16 (2,3)

	
	
	1.9  Ammonium Ion 
	БДС 3587, Method 2 (1)
БДС 17.1.4.10, Method 2 (2,3)
VLM (Validated Laboratory Method) 001: 2012 (1,2,3)

	
	
	1.10  Nitrites 
	БДС  ЕN 26777 (1, 3)
VLM 003: 2012 (1, 3)

	
	
	1.11  Nitrates 
	БДС  ISO 7890-3 (1,2,3)
VLM 005: 2012 (1,2,3)

	
	
	1.12  Chlorides
	БДС 3414 (1)
БДС 17.1.4.24, cl. 1 (2,3)
VLM 007:2012 (1,2,3)

	
	
	1.13  Sulphates
	VLM 008: 2012 (1,2,3)

	
	
	1.14  Phosphates
	БДС EN ISO 6878, cl. 4 (1,2,3)
VLM 034:2012 (1,2,3)

	
	
	1.15  Маgnesium
	VLM 038:2022 (1,3)

	
	
	1.16  Calcium
	БДС ISO 6058 (1,3)

	
	
	1.17  Iron
	БДС ISO 6332 (1,2,3)

	
	
	1.18  Zink
	VLM 009:2012 (1,2,3)

	
	
	1.19  Copper
	VLM 011:2012 (1,2,3)

	
	
	1.20  Lead
	VLM 013:2012 (1,2,3)

	
	
	1.21  Manganese
	БДС ISO 6333 (1,2,3)

	
	
	1.22  Fluorides
	VLM 026:2012 (1,2,3)

	
	
	1.23  Cadmium
	VLM 017:2012 (1,2,3)

	
	
	1.24  Chrome, Total
	VLM 019:2012 (1,2,3)

	
	
	1.25  Free and Total Chlorine
	VLM 015:2012 (1)
VLM 016:2012 (1)

	
	
	1.26  Nickel
	VLM 022:2012 (1,2,3)

	
	
	1.27  Cyanides
	VLM 024:2012 (1,2,3)

	
	
	1.28  Aluminum
	БДС ISO 10566 (1,3)

	
	
	1.29 COD (Chemical Oxygen Demand)
	VLM 027:2012 (2) 

	
	
	1.30  Turbidity
	БДС EN ISO 7027-1 (1,2,3)

	
	
	1.31  Dissolved Oxygen
	БДС EN ISO 5814 (1,2,3)

	
	
	Microbiological  characteristics:

	
	
	1.32  Clostridium Perfringens 
	БДС EN ISO 14189 (1,3)

	
	
	1.33  Coliforms
	БДС EN ISO 9308-1/А1  (1,3)

	
	
	1.34  Еscherichia Coli
	БДС EN ISO 9308-1/А1  (1,3)

	
	
	1.35  Total Colonies of
Viable Microorganisms /
Microbial Count
	БДС EN ISO 6222  (1,3)


	
	
	1.36  Faecal Streptococci 
	БДС EN ISO 7899-2  (2)

	
	
	1.37  Enterococci 
	БДС EN ISO 7899-2  (1,3)

	
	
	1.38  Salmonella 
	БДС EN ISO 19250  (2)



Office 1 PSPV-Pernik:
To perform sampling of:
	Type of the scope:  Flexible

	№
	Product
	Sampling methods
(standard/validated method)

	1
	2
	3

	1.
	Potable Water  
	БДС ISO 5667-5
БДС EN ISO 19458

	2.
	Surface Water  
	БДС ISO 5667-4
БДС EN ISO 19458

	3.
	Underground Water
	БДС ISO 5667-11
БДС EN ISO 19458




Office 2 Batanovtsi, GPSOV:
To perform testing of: 
	Type of the scope:  Flexible for part of the scope

	№
	Tested products
	Type of test/characteristic
	Testing methods
(standard/validated method)

	1
	2
	3
	4

	1.
	Wastewater
	1.1   Аctive Reaction
	БДС 17.1.4.27, cl. 1

	
	
	1.2   Теmperature
	БДС 17.1.4.01, cl. 4

	
	
	1.3   COD (Chemical Oxygen Demand)
	VLM  027: 2012
VLM  028: 2012
VLM  029: 2012

	
	
	1.4   BOD5 (Biochemical
Oxygen Demand for 5 days)
	БДС EN ISO 5815-1                             БДС EN 1899-2 

	
	
	1.5   Ammonium Ion
	БДС 17.1.4.10, Method 2
VLM 002: 2012

	
	
	1.6   Nitrates
	БДС 17.1.4.12
VLM 006: 2012

	
	
	1.7   Chlorides
	БДС 17.1.4.24, cl. 1

	
	
	1.8   Nitrites
	БДС ЕN 26777
VLM 004: 2012

	
	
	1.9   Zink
	VLM 010: 2012

	
	
	1.10  Iron
	БДС ISO 6332
VLM 031: 2012

	
	
	1.11  Phosphorus / Total /
	БДС EN ISO 6878, cl. 7
VLM  036: 2012

	
	
	1.12  Phosphates
	БДС EN ISO 6878, cl. 4
VLM  035: 2012

	
	
	1.13  Total Nitrogen 
	VLM  030: 2012

	
	
	1.14  Undissolved Substances
	БДС 17.1.4.04, cl. 2

	
	
	1.15 Suspended Substances
/ Undissolved Substances
	БДС EN 872  

	
	
	1.16  Dissolved Oxygen
	БДС EN 25813

	
	
	1.17  Cyanides
	VLM  025: 2012

	
	
	1.18 Anionic Detergents
/ α-Synthetic Surfactants/
	VLM  033: 2012

	
	
	1.19  Phenols / Volatile /
	VLM  037: 2012

	
	
	1.20  Cadmium
	VLM  018: 2012

	
	
	1.21  Copper
	VLM  012: 2012

	
	
	1.22  Nickel
	VLM  023: 2012

	
	
	1.23  Chrome, Total
	VLM  020: 2012

	
	
	1.24  Sulphates
	БДС 17.1.4.03

	2.
	Surface Water 




	2.1  Undissolved Substances 
	БДС 17.1.4.04, cl. 2

	
	
	2.2 BOD5 (Biochemical 
       Oxygen Demand for 5 days) 
	БДС EN ISO 5815-1
БДС EN 1899-2

	
	
	2.3  Dissolved Oxygen
	БДС EN 25813



Office 2 Batanovtsi, GPSOV:
To perform sampling of:
	Type of the scope:  Flexible

	№
	Product 
	Sampling methods
(standard/validated method)

	1
	2
	3

	 1.
	Wastewater
	БДС ISO 5667-10



*Flexible Scope: Implementing a new version of standards/documents or standards / documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.

Fixed scope references:
1. VLM 001/2012 - Water quality. Spectrophotometric method for the determination of ammonium ions in water using a Nessler reagent.
2. VLM 002/2012 - Water quality. Spectrophotometric method for the determination of ammonium ions in wastewater with the formation of indophenol blue.
3. VLM 003 /2012 - Water quality. Spectrophotometric method for the determination of nitrites in water by using diazotization.
4. VLM 004/2012 - Water quality. Spectrophotometric method for the determination of nitrites in wastewater by using diazotization.
5. VLM 005/2012 - Water quality. Spectrophotometric method for the determination of nitrates in water by using 2,6-dimethylphenol.
6. VLM 006/2012 - Water quality. Spectrophotometric method for the determination of nitrates in wastewater by using 2,6-dimethylphenol.
7. VLM 007/2012 - Water quality. Spectrophotometric method for the determination of chlorides in water by using mercuric thiocyanate.
8. VLM 008/2012 - Water quality. Spectrophotometric method for the determination of sulphates in water by using a Sulfa Ver® 4 powder reagent.
9.  VLM 009/2012 - Water quality. Spectrophotometric method for the determination of zinc in water by using 4- (2-pyridylazo) -resorcinol.
10. VLM 010/2012 - Water quality. Spectrophotometric method for the determination of zinc in wastewater by using 4-(2-pyridylazo) -resorcinol.
11. VLM 011/2012 /2012 - Water quality. Spectrophotometric method for the determination of copper in water by using a CuVer®1 powder reagent.
12. VLM 012/2012 - Water quality. Spectrophotometric method for the determination of copper in wastewater by using a CuVer®1 powder reagent.
13. VLM 013/2012 - Water quality. Spectrophotometric method for the determination of lead in water by using rapid column extraction.
14. VLM 015/2012 - Water quality. Spectrophotometric method for the determination of free and total chlorine in water by using DPD.
15. VLM 016/2012 - Water quality. MERCK Spectroquant® photometric method for the determination of free and total chlorine / Picco /.
16. VLM 017/2012 - Water quality. Spectrophotometric method for the determination of cadmium in water by using a DithiVer powder reagent.
17. VLM 018/2012 - Water quality. Spectrophotometric method for the determination of cadmium in wastewater by using Cadion.
18. VLM 019/2012 - Water quality. Spectrophotometric method for the determination of chromium in water by using a ChromaVer® powder reagent.
19. VLM 020/2012 - Water quality. Spectrophotometric method for the determination of chromium (VI, III- valent and total) in wastewater by using 1,5-diphenylcarbazide.
20. VLM 022/2012 - Water quality. Spectrophotometric method for the determination of nickel in water by using 1-(2-pyridylazo) -2-naphthol.
21. VLM 023/2012 - Water quality. Spectrophotometric method for the determination of nickel in wastewater by using a Heptoxime powder reagent.
22. VLM 024/2012 - Water quality. Spectrophotometric method for the determination of cyanides in water by using pyridine-pyrazolone.
23. VLM 025/2012 - Water quality. Spectrophotometric method for the determination of cyanides in wastewater by using pyridine in the presence of barbituric acid.
24. VLM 026/2012 - Water quality. Spectrophotometric method for the determination of fluoride in water by using SPADNS reagent solution.
25. VLM 027/2012 - Water quality. Spectrophotometric method in the determination of COD /Chemical Oxygen Demand/ (5-60) mg O2/l in surface and waste water.
26. VLM 028/2012 - Water quality. Spectrophotometric method in the determination of COD (15-150) mg O2/l in wastewater.
27. VLM 029/2012 - Water quality. Spectrophotometric method in the determination of COD (150-1000) mgO2/l in wastewater.
28. VLM 030/2012 - Water quality. Spectrophotometric method for the determination of total nitrogen in wastewater.
29. VLM 031/2012 - Water quality. Spectrophotometric method for the determination of iron in wastewater by using 1,10-phenanthroline.
30. VLM 033/2012 - Water quality. Spectrophotometric method for the determination of anionic detergents (α-Synthetic Surfactants) in wastewater and surface water by using methylene blue.
31. VLM 034/2012 - Water quality. Spectrophotometric method for the determination of phosphates in water by using ammonium molybdate.
32. VLM 035/2012 - Water quality. Spectrophotometric method for the determination of phosphates in wastewater by using ammonium molybdate.
33. VLM 036/2012 - Water quality. Spectrophotometric method for the determination of total phosphorus in wastewater.
34. VLM 037/2012 - Water quality. Spectrophotometric method for the determination of phenols in wastewater by using 4-nitroaniline. 
35. VLM 038/2022 - Water quality. Determination of magnesium content in water.
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