SCOPE 17 ЛК

Meter Expert Ltd. 
Calibration laboratory 

Management address: 1040 Sofia, Sredets District, 2 Hristo Belchev Str, floor 4, office 3
Laboratory address: 1618 Sofia, Manastirski livadi, 59 B Ivan Susanin Str.

To perform calibrating of:

	Type of the scope: fixed

	№
	Measuring 
instrument
	Measured value,
unit of measure
	Measurement 
range
	Measurement
uncertainty
	Calibration Method 

	1
	2
	3
	4
	5
	6

	1
	Non-automatic electronic and mechanical scales, class:

Class I
	Mass,
(kg and his submultiples)
	to 300 g

	0,01 mg to 3,0 mg
	ПК 7.2-5
 (K): 2019 

	
	


Class II
	
	0,3 kg to 2,2 kg

2,2 kg to 20 kg

20 kg to 60 kg

60 kg to 80 kg
	3,0 mg to 6,6 mg

6,6 mg to 600 mg

600 mg to 1000 mg

1 g
	

	2.
	Non-automatic electronic and mechanical scales, class  III 
	Mass, 
(kg and his submultiples)
	2,0 kg to 20 kg
20 kg to 500 kg
500 kg to 2000 kg

	1,6 g to 6 g
6 g to 25 g
25 g to 200 g

	ПК 7.2-5
 (K): 2019 

	3.
	Weights, 
class F2
	Mass, 
(kg and his submultiples)
	10 g
	2,0.10-4 g
	ПК 7.2-4
 (K): 2019 

	
	
	
	20 g
	2,6.10-4 g
	

	
	
	
	50 g
	3,0.10-4 g
	

	
	
	
	100 g
	5,0.10-4 g
	

	
	
	
	200 g
	1,0.10-3 g
	

	
	
	
	500 g
	2,7.10-3 g
	

	
	
	
	1000 g
	5,0.10-3 g
	

	
	
	
	2000 g
	1,0.10-2 g
	

	
	
	
	5000 g
	2,7.10-2 g
	

	
	
	
	10000 g
	4,3.10-2 g
	

	
	
	
	20000 g
	7,0.10-2 g

	

	4.
	Weights, 
class М: 
М1, M1-2, М2, 
М2-3 and М3
	Mass, 
(kg and his submultiples)
	1 g
	2,0.10-4 g
	ПК 7.2-4
 (K): 2019 

	
	
	
	2 g
	2,6.10-4 g
	

	
	
	
	5 g
	3,2.10-4 g
	

	
	
	
	10 g
	4,0.10-4 g
	

	
	
	
	20 g
	5,0.10-4 g
	

	
	
	
	50 g
	6,0.10-4 g
	

	
	
	
	100 g
	1,0.10-3 g
	

	
	
	
	200 g
	2,5.10-3 g
	

	
	
	
	500 g
	8,0.10-3 g
	

	
	
	
	1000 g
	1,6.10-2 g
	

	
	
	
	2000 g
	3,0.10-2 g
	

	
	
	
	5000 g
	5,3.10-2 g
	

	
	
	
	10000 g
	7,7.10-2 g
	

	
	
	
	20000 g
	1,2.10-1 g
	

	5.
	Reference weights
	Mass, 
(kg and his submultiples)
	1 g to 20000 g
	2,0.10-4 g 
to 1,2.10-1 g
	ПК 7.2-4
 (K): 2019




Notes:
1. Calibration of the measuring instruments specified in item 1 is performed onsite, at the customer’s premises.
2. Calibration of the measuring instruments specified in item 2 performed in the laboratory   and onsite, at the customer’s premises.
3. Calibration of the measuring instruments specified in items 3, 4 and 5 is performed in the laboratory.

References:
ПК 7.2-5 (K):2019 - Method for calibration of non-automatic scales;
ПК 7.2-4 (K):2019 - Method for calibration of weights - direct comparison method;


гр. София 1797, бул. "Г.М.Димитров" № 52 А, ет.7
Тел: +3592 9766 401; Факс: +3592 9766 415 
e-mail: office@nab-bas.bg
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