SCOPE 94 ЛИ
Sofia, 26.08.2025
AMEES OOD
WATER TESTING LABORATORY
Management and laboratory address: 
6260 Radnevo, Stara Zagora Region, 3 Valentina Tereshkova Str.
To perform testing of:
	Type of the scope: Flexible for part of the scope*

	№
	Tested Products
	Type of Test/Characteristic
	Testing Methods
(standard/ validated Method)

	1
	2
	3
	4

	1.
	Surface water (1)
Groundwater (2)
Wastewater (3)	
	1.1. Active reaction - pH
	БДС EN ISO 10523 (1,2,3)

	
	
	1.2. Electrical conductivity
	БДС EN 27888 (1,2,3)

	
	
	1.3. Colour
	БДС EN ISO 7887 (1,2,3)

	
	
	1.4. Temperature
	БДС 17.1.4.01, cl. 4 (1,2,3)

	
	
	1.5. Chemical Oxygen Demand (COD)
	БДС ISO 15705 (1,2,3)

	
	
	1.6. Biochemical Oxygen Demand (BOD)5
	БДС EN ISO 5815-1
(1,2,3)

	
	
	1.7. Dissolved oxygen, Oxygen saturation
	БДС EN ISO 5814 (1,2,3)

	
	
	1.8. Permanganate oxidisability
	БДС 17.1.4.16 (1,2,3)

	
	
	1.9. Total dry matter,
Insoluble substances,
Soluble substances
	БДС 17.1.4.04 (1,2,3)

	
	
	1.10. Insoluble (suspended) substances	
	БДС EN 872 (3)

	
	
	1.11. Dissolved sulphides and
free hydrogen sulphide
	БДС 17.1.4.09 (1,2,3)

	
	
	1.12. Sulphides
	VLM 10/2012 (1,2,3)

	
	
	1.13. Alkalinity (total and
constituent), Carbonates,
Hydrogen carbonates
	БДС EN ISO 9963-1 (1,2,3)

	
	
	1.14. General hardness
	БДС ISO 6059 (1,2)

	
	
	1.15. Calcium
	БДС ISO 6058 (1,2)

	
	
	1.16. Magnesium
	VLM 19/2020 (1,2)

	
	
	1.17. Sulphate ions, Sulphates
	БДС 17.1.4.03 (1,2,3)
VLM 20/2024 (1,2,3) 

	
	
	1.18. Free Chlorine, Total Chlorine
	БДС EN ISO 7393-2 (1,2,3)
VLM 15/2015 (1,2,3)

	
	
	1.19. Chlorides
	БДС 17.1.4.24 (1,2,3)

	
	
	1.20. Phosphorus (total), Phosphates,
Orthophosphates,Phosphates (as P)
Phosphates (as P2O5)	
	БДС EN ISO 6878 (1,2,3)
VLM 16/2015 (1,2,3)

	
	
	1.21. Ammonium nitrogen
Ammonium ions, Ammonium
	БДС ISO 7150-1 (1,2,3)
БДС 17.1.4.10 (1,2,3)

	
	
	1.22. Nitrite nitrogen, Nitrites 
	БДС EN 26777 (1,2,3)

	
	
	1.23. Nitrate nitrogen, Nitrates
	БДС ISO 7890-3 (1,2,3)
БДС 17.1.4.12 (1,2,3)

	
	
	1.24. Nitrogen (total)
	VLM 01/2010 (1,2,3)

	
	
	1.25. Adsorbable Organic
Halides (AOH)
	VLM 11/2015 (1,2,3)

	
	
	1.26. Anionic detergents (a-PAHs)
	БДС EN 903 (1,2,3)

	
	
	1.27. Extractable lipids,
Petroleum products, 
Total extractable substances.
	VLM 02/2010(1,2,3)

	
	
	1.28. Iron (total), (dissolved)	
	БДС ISO 6332 (1,2,3)

	
	
	1.29. Chromium (total), (trivalent), (hexavalent)	
	БДС 17.1.4.17 (1,2,3)

	
	
	1.30. Copper
	БДС 17.1.4.19 (1,2,3)

	
	
	1.31. Nickel
	VLM 12/2015 (1,2,3)

	
	
	1.32. Manganese
	VLM 13/2015 (1,2,3)

	
	
	1.33. Arsenic
	VLM 14/2015 (1,2,3)

	
	
	1.34. Aluminium
	БДС ISO 10566 (1,2)

	
	
	1.35. Zinc
	VLM 03/2011 (1,2,3)

	
	
	1.36. Lead
	VLM 04/2011 (1,2,3)

	
	
	1.37. Cadmium
	VLM 05/2011 (1,2,3)

	
	
	1.38. Cobalt
	VLM 06/2011 (1,2,3)

	
	
	1.39. Fluorides
	VLM 07/2012 (1,2,3)

	
	
	1.40. Cyanides (total), (free)
	VLM 08/2012 (1,2,3)

	
	
	1.41. Phenols
	VLM 09/2012 (1,2,3)

	2.
	Calcium carbonate
(limestone),
Dolomite
	2.1. Calcium Carbonate content
	БДС EN ISO 3262-1, 
cl. 5.3

	
	
	2.2. Magnesium carbonate
content	
	БДС EN ISO 3262-1, 
cl. 5.3



To perform sampling of:
	Type of the scope: Flexible*

	№
	Product
	Sampling Method 
(standardized / internal validated)

	1
	2
	3

	1.
	Surface water
	БДС ISO 5667-4
БДС EN ISO 5667-6/A11

	2.
	Groundwater
	БДС ISO 5667-11

	3.
	Wastewater
	БДС ISO 5667-10



Flexible scope: Implementing a new version of standards/documents or standards / documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by the laboratory.

Fixed scope reference:
VLM 01/2010 Water quality. Determination of total nitrogen. Method employing oxidative decomposition with peroxydisulphate and photometric determination using 2,6-dimethylphenol.
VLM 02/2010 Water quality. Determination of total extractable substances, extractable lipids, vegetable oils, and petroleum products.
VLM 03/2011 Water quality. Determination of zinc.
VLM 04/2011 Water quality. Determination of lead.
VLM 05/2011 Water quality. Determination of cadmium.
VLM 06/2011 Water quality. Determination of cobalt.
VLM 07/2012 Water quality. Determination of fluorides.
VLM 08/2012 Water quality. Determination of cyanides.
VLM 09/2012 Water quality. Determination of phenols.
VLM 10/2012 Water quality. Determination of sulphides.
VLM 11/2015 Water quality. Photometric determination of Absorbable Organic Halides (AOH).
VLM 12/2015 Water quality. Photometric determination of nickel in water.
VLM 13/2015 Water quality. Photometric determination of manganese in water.
VLM 14/2015 Water quality. Photometric Determination of Total Arsenic in Water.
VLM 15/2015 Water quality. Determination of free chlorine and total chlorine in water.
VLM 16/2015 Water quality. Determination of total phosphorus and orthophosphates.
VLM 19/2020 Water quality. Determination of magnesium.
VLM 20/2024 Water quality. Spectrophotometric determination of sulphates.
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