SCOPE 167 ЛИ
Sofia, 30.09.2025
VODOSNABDYAVANE I KANALIZATSIYA DOBRICH AD
TESTING LABORATORY
Management address: 
9300 Dobrich, 59 Treti Mart Blvd, p.o. Box 203

Laboratory address:
Drinking, Surface and Groundwater Direction: 9300 Dobrich, 59 Treti Mart Blvd.
Wastewater Direction: 9345 Vrachantsi, Dobrich Region, Wastewater Treatment Plant

To perform testing of:
	Type of the scope: flexible for a part of the scope

	№
	Tested products
	Type of test / 
characteristic
	Testing methods
(standard / validated method)

	1
	2
	3
	4

	1.
	Drinking water (1), 
Surface water (2),
Groundwater (3)
	1.1 Color
	БДС 8451, (1)

	
	
	1.2 Active reaction (pH)
	БДС EN ISO 10523, (1), (2), (3)

	
	
	1.3 Electrical conductivity
	БДС EN 27888, (1), (2), (3)

	
	
	1.4 Turbidity
	БДС EN ISO 7027-1, (1), (2), (3)

	
	
	1.5 Ammonium ions
	БДС 3587, cl. 2, (1) 
IVLM 17:2024, (1), (2), (3)

	
	
	1.6 Nitrites
	БДС EN 26777, (1), (2), (3)
IVLM 18:2024, (1), (2), (3)

	
	
	1.7 Nitrates
	БДС 3758, cl. 1, (1)
IVLM 19:2024, (1), (2), (3)

	
	
	1.8 Chlorides
	БДС 3414, (1)
БДС 17.1.4.24, (2),(3)

	
	
	1.9 Phosphates
	IVLM-1-DW:2006, (1), (2), (3)

	
	
	1.10 Sulfates
	IVLM-2-DW:2005, (1), (2), (3)

	
	
	1.11 Magnesium
	IVLM-16-DW:2020, (1), (2), (3)

	
	
	1.12 Calcium
	БДС ISO 6058, (1), (2), (3)

	
	
	1.13 Sum of calcium and magnesium
	БДС ISO 6059, (1), (2), (3) 

	
	
	1.14 Iron
	БДС ISO 6332, cl. 7.1, (1), (2), (3)
IVLM-20:2024, (1), (2), (3)

	
	
	1.15 Copper
	IVLM-3-DW:2005, (1), (2), (3)

	
	
	1.16 Zinc
	IVLM-4–DW:2005, (1), (2), (3)

	
	
	1.17 Chrome
	IVLM-5-DW:2005, (1), (2), (3)

	
	
	1.18 Manganese
	IVLM-6-DW:2005, (1), (2), (3)
БДС ISO 6333, (1), (2), (3)

	
	
	1.19 Cyanides
	IVLM-7-DW:2005, (1), (2), (3)

	
	
	1.20 Fluorides
	IVLM-8-DW:2005, (1), (2), (3)

	
	
	1.21 Residual chlorine
	БДС 3560, cl. 5, (1)

	
	
	1.22 Oxidation (permanganate)
	БДС 3413, (1)
БДС 17.1.4 .16, (2),(3)

	
	
	1.23 Dissolved oxygen
	БДС 17.1.4.08, (2), (3)

	
	
	1.24 Aluminum
	IVLM-9-DW:2006, (1), (2), (3)

	
	
	1.25 Nickel
	IVLM-10-DW:2007, (1), (2), (3)

	
	
	1.26 Boron
	IVLM-11-DW:2012, (1), (2), (3)

	
	
	1.27 Lead
	IVLM-12–DW:2012, (1), (2), (3)

	
	
	1.28 Cadmium
	IVLM-13–DW:2012, (1), (2), (3)

	
	
	1.29 Arsenic
	IVLM-14-DW:2012, (1), (2), (3)

	
	
	1.30 Sodium
	IVLM-15-DW:2012, (1), (2), (3)

	
	
	1.31 Solids
	БДС 3546, (1)
БДС 17.1.4.04, (2), (3)

	
	
	1.32 Coliform bacteria
	БДС EN ISO 9308-1, (1),

	
	
	1.33 Escherichia coli
	БДС EN ISO 9308-1, (1)

	
	
	1.34 Intestinal Enterococci
	БДС EN ISO 7899-2, (1), (3)

	
	
	1.35 Viable microbial count (microbial count at 22oC and 36oC)
	БДС EN ISO 6222, (1), (3)





 II. Wastewater Laboratory – Wastewater Treatment Plant, village of Vrachantsi, municipality of Dobrich, region of Dobrich

	Type of the scope: flexible for part of the scope

	№
	Tested products
	Type of test/characteristic
	Testing methods
(standard / validated method)

	1
	2
	3
	4

	1
	Wastewater



	1.1 Active reaction (pH)
	БДС EN ISO 10523

	
	
	1.2 Undissolved substances
	БДС 17.1.4.04, cl. 2

	
	
	1.3 Dissolved oxygen
	БДС 17.1.4.08

	
	
	1.4 COD (bichromate oxidation)
	IVLM-1-WW:2006

	
	
	1.5 Nitrogen (total)
	IVLM–2-WW:2006

	
	
	1.6 Phosphorus (total), phosphorus (phosphate) and phosphates
	IVLM-3-WW:2005

	
	
	1.7 Cyanides
	IVLM-4-WW:2005

	
	
	1.8 Anionic active detergents (a-surfactants) 
	IVLM-5-WW:2006

	
	
	1.9 Phenols
	БДС 17.1.4.13

	
	
	1.10 Iron (total)
	IVLM-6-WW:2006

	
	
	1.11 Cadmium
	IVLM-7-WW:2006

	
	
	1.12 Manganese
	IVLM-8-WW:2005

	
	
	1.13 Copper
	IVLM-9-WW:2005

	
	
	1.14 Nickel
	IVLM-10-WW:2005

	
	
	1.15 Arsenic
	IVLM-11-WW:2006

	
	
	1.16 Lead
	IVLM-12-WW:2005

	
	
	1.17 Chromium (hexavalent),
 Chromium (trivalent),
 Chromium (total) 
	IVLM– 13-WW:2005

	
	
	1.18 Zinc
	IVLM-14-WW:2006

	
	
	1.19 Biochemical oxygen demand (BODn)
	БДС ISO 5815-1

	
	
	1.20 Extractable substances 
	IVLM-15-WW:2006, item 1

	
	
	1.21 Petroleum products
	IVLM-15-WW:2006, item 2

	
	
	1.22 Sulfates
	IVLM-16-WW:2008

	
	
	1.23 Nitrates, 
Nitrate nitrogen
	IVLM-17-WW:2013



To perform sampling of:
	Type of the scope: flexible

	№
	Product
	Samplting methods
(standard/validated method)

	1
	2
	3

	1.
	Water: 
Drinking water (1),
Groundwater (2),
Wastewater (3).
	БДС ISO 5667-5, (1)
БДС ISO EN 19458, (1), (2)
БДС ISO 5667-11, cl. 5.3.2.2.  (2)
БДС ISO 5667-10, (3)



Flexible scope: Implementing a new version of standards/documents or standards/ documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.

Fixed scope references:
IVLM-1-DW:2006 Spectrophotometric method for determination of phosphates content.
IVLM-2-DW:2005 Spectrophotometric method for the determination of sulphates content.
IVLM-3-DW:2005 Spectrophotometric method for the determination of copper content.
IVLM-4-DW:2005 Spectrophotometric method for the determination of zinc content.
IVLM-5-DW:2005 Spectrophotometric method for the determination of chrome content.
IVLM-6-DW:2005 Spectrophotometric method for the determination of manganese content.
IVLM-7-DW:2005 Spectrophotometric method for the determination of cyanides content.
IVLM-8-DW:2005 Spectrophotometric method for the determination of fluorides content.
IVLM-9-DW:2006 Spectrophotometric method for the determination of aluminum content.
IVLM-10-DW:2007 Spectrophotometric method for the determination of nickel content.
IVLM-11-DW:2012 Spectrophotometric method for the determination of boron content.
IVLM-12-DW:2012 Spectrophotometric method for the determination of lead content.
IVLM-13-DW:2012 Spectrophotometric method for the determination of cadmium content.
IVLM-14-DW:2012 Spectrophotometric method for the determination of arsenic content.
IVLM-15-DW:2012 Spectrophotometric method for the determination of sodium content.
IVLM-16-DW:2020 Method for determination of magnesium in water.
IVLM-17:2024 Spectrophotometric method for the determination of ammonium content.
IVLM-18:2024 Spectrophotometric method for the determination of nitrites content.
IVLM-19:2024 Spectrophotometric method for the determination of nitrates content.
IVLM-20:2024 Spectrophotometric method for the determination of iron content.

IVLM-1-WW:2006 Spectrophotometric method for determination of COD content /dichromate oxidizability.
IVLM-2-WW:2006 Spectrophotometric method for determination of nitrogen content (total).
IVLM-3-WW:2005 Spectrophotometric method for determination of phosphorus (total), phosphorus (phosphate) and phosphates content.
IVLM-4-WW:2005 Spectrophotometric method for determination of cyanides content.
IVLM-5-WW:2006 Spectrophotometric method for determination of anionic active detergents (a-surfactants) content.
IVLM-6-WW:2006 Spectrophotometric method for determination of iron /total) content.
IVLM-7-WW:2006 Spectrophotometric method for determination of cadmium content.
IVLM-8-WW:2005 Spectrophotometric method for determination of manganese content.
IVLM-9-WW:2005 Spectrophotometric method for determination of copper content.
IVLM-10-WW:2005 Spectrophotometric method for determination of nickel content.
IVLM-11-WW:2006 Spectrophotometric method for determination of arsenic content.
IVLM-12-WW:2005 Spectrophotometric method for determination of lead content.
IVLM-13-WW:2005 Spectrophotometric method for determination of chromium content (hexavalent, trivalent and total).
IVLM-14-WW:2006 Spectrophotometric method for determination of zinc content.
IVLM-15-WW:2006 Methods for determination of extractable substances and petroleum products.
IVLM-16–WW:2008 Spectrophotometric method for determination of sulfates content.
IVLM-17–WW:2013 Spectrophotometric method for determination of nitrates / nitrate nitrogen.
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