SCOPE 323 ЛИ
Sofia, 01.12.2025
RESEARCH AND CERTIFICATION CENTRE 
FOR BUILDING MATERIALS LTD (ISZSM LTD)
TESTING LABORATORY

Management address: Sofia, Manastirski Livadi, 86 Ralevitsa Str, 
Laboratory address: Sofia, Druzhba 1, 14 Asen Yordanov Blvd.

To perform testing of:
	Type of the scope: fixed

	№
	Tested products
	Type of test/ characteristic
	Testing methods
(standard/ validated method)

	1
	2
	3
	4

	1.
	Plastic piping and connecting parts 
	Appearance
	БДС EN 12201-2:2024, 
БДС EN 13476-3:2018+А1:2020 
БДС EN 1451-1:2018

	
	
	Sizes
	БДС EN ISO 3126:2005

	
	
	Melt index
	БДС EN ISO 1133-1:2022

	
	
	Tensile elongation at break
	БДС EN ISO 6259-1:2015
БДС EN ISO 6259-3:2015

	
	
	Oxidation induction time (OIT)
	БДС EN ISO 11357-6:2025

	
	
	Resistance to internal hydrostatic pressure
	БДС EN ISO 1167-1:2006
БДС EN ISO 1167-2:2006

	
	
	Longitudinal shrinkage
	БДС EN ISO 2505:2023

	2.
	Products for decorative coatings
	Adhesion
	БДС EN ISO 4624:2023

	
	
	Wet friction resistance
	БДС EN ISO 11998:2006

	
	
	Film gloss
	БДС EN ISO 2813:2015

	
	
	Water vapor transmission rate (WVTR)
	БДС EN 1062-3:2008

	
	
	Water vapor transmission properties:
- water vapor transmission rate;
- equivalent layer thickness
air under diffusion conditions
	БДС EN ISO 7783:2019 
Wet plate method

	3.
	Construction mortars, including: Masonry mortars; Floor screed mortars
	Adhesion strength
	БДС EN 13892-8:2003

	
	
	Wear resistance VCA method
	БДС EN 13892-4:2003

	
	
	Bulk density of fresh mortar
	БДС EN 1015-6:2001/А1:2007

	4.
	Products and systems                 for the protection and restoration of concrete structures
	Adhesion under tensile load
	БДС EN 1542:2002

	
	
	Water permeability coefficient
	БДС EN 1062-3:2008

	
	
	Crack resistance
	БДС EN 1062-7:2006
Method A Uniform Crack Growth
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