SCOPE 89 ЛИ
Sofia, 04.03.2026
KCM AD
ENVIRONMENTAL LABORATORY

Management address: 4009 Plovdiv, Asenovgradsko Shose Str.
Laboratory address: 4009 Plovdiv, Asenovgradsko Shose Str.

To perform testing of:
	Type of the scope: flexible for a part of the scope*

	№
	Tested products
	Type of test/ characteristic
	Testing methods
(standard/ validated method)

	1
	2
	3
	4

	1.
	Emissions of harmful substances released into the air from facilities with stationary sources
	1.1. Dust
	БДС EN 13284-1 
БДС ISO 9096

	
	
	1.2. Sulfur dioxide/SO2
	БДС 17.2.4.04 
VILM 1-1:2003

	
	
	1.3. Carbon oxide/CO 
	VILM 1-1:2003
БДС EN 15058

	
	
	1.4. Nitrogen oxides –/NOx (NO + NO2)
	VILM 1-1:2003
БДС EN 14792

	
	
	1.5. Oxygen/O2
	VILM 1-1:2003
БДС EN 14789

	
	
	1.6. Moisture
	БДС EN 14790

	
	
	1.7. Zinc
	VILM 1-2:2003

	
	
	1.8. Cadmium
	VILM 1-2:2003
БДС EN 14385

	
	
	1.9.  Lead
	VILM 1-2:2003
БДС EN 14385

	
	
	1.10. Chrome
	БДС EN 14385

	
	
	1.11. Nickel
	БДС EN 14385

	
	
	1.12. Gas flow rate, speed, temperature, pressure/ vacuum, barometric pressure
	БДС EN ISO 16911-1

	
	
	1.13. Sulfur trioxide / SO3
	БДС 17.2.4.09

	2.
	Immissions of harmful substances into the air
	2.1. Total dust / Particulate matter 10/ PM 10
	БДС 17.2.4.20

	
	
	2.2. Lead
	VILM 1-3:2003

	
	
	2.3. Cadmium
	VILM 1-3:2003

	3.
	Water:
(1) industrial,
(2) running surface,
(3) waste,
(4) drinking,
(5) groundwater,
(6) infiltrates
	3.1. pH
	БДС 17.1.4.27, cl. 1
(1,2,3,5,6)
БДС 3424, pt. 1 (4)

	
	
	3.2. Dissolved substances
	БДС 17.1.4.04, cl. 3 (1,2,3,5,6)

	
	
	3.3. Undissolved substances
	БДС 17.1.4.04, cl. 2 (1,2,3,4,5,6)
БДС EN 872  (1,2,3,4,5,6)

	
	
	3.4. Biochemical oxygen demand for 5 days/ BOD5
	БДС EN 1899-2 (1,2,3,4,5,6)
БДС EN ISO 5815-1 (1,2,3,4,5,6)

	
	
	3.5. Lead
	ISO 8288 (1,2,3,5,6)
БДС 16777 (4)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.6. Zinc
	ISO 8288 (1,2,3,5,6)
БДС 16777 (4)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.7. Cadmium
	ISO 8288 (1,2,3,5,6)
БДС 16777 (4)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.8. Copper
	ISO 8288 (1,2,3,5,6)
БДС 16777 (4)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.9. Iron (total)
	БДС 3425, pt. 2 (1,2,3,5,6)
БДС 16777 (4)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.10. Manganese
	БДС 16777 (1,2,3,4,5,6)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.11. Cobalt
	ISO 8288 (1,2,3,4,5,6)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.12. Nickel
	ISO 8288 (1,2,3,4,5,6)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.13. Chrome (total)
	БДС EN 1233, cl. 3, cl.4 (1,3,6)
БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.14. Cyanides (total)
	БДС ISO 6703-1, Section 2 (1,2,3,4,5,6)

	
	
	3.15. Cyanides (free readily degradable)
	БДС 17.1.4.14 (1,2,3,4,5,6)
БДС 7214 (4)

	
	
	3.16. Cyanides total/ free readily degradable
	VILM 1-5:2008 (1,2,3,4,5,6)

	
	
	3.17. Sulfates
	БДС 3588 (4)
БДС 17.1.4.03 (1,2,3,5,6)

	
	
	3.18. Chlorides
	БДС 3414 (4)
БДС 17.1.4.24, cl.1 (1,2,3,5,6)

	
	
	3.19. Nitrates/ nitrate nitrogen
	БДС 3758 (4)
БДС 17.1.4.12 (1,2,3,5,6)
БДС ISO 7890-3 (1,2,3,4,5,6)

	
	
	3.20. Nitrites/ nitrite nitrogen
	БДС EN 26777 (1,2,3,4,5,6)

	
	
	3.21. Total phosphorus/ orthophosphates
	БДС EN ISO 6878 (1,2,3,4,5,6)

	
	
	3.22. Ammonia/ ammonium/ ammonium nitrogen
	БДС ISO 7150-1 (1,2,3,4,5,6)

	
	
	3.23. Electrical conductivity
	БДС EN 27888 (1,2,3,4,5,6)

	
	
	3.24. Total dry residue
	БДС 17.1.4.04, cl.1 (1,2,3,5,6)
БДС 3546 (4)

	
	
	3.25. Chemical oxygen demand/ COD
	БДС 17.1.4.02 (1,2,3,4,5,6)
ISO 6060 (1,2,3,4,5,6)

	
	
	3.26. Permanganate oxidation (Permanganate index)
	БДС EN ISO 8467 (4)
БДС 17.1.4.16 (1,2,3,5,6)
БДС 3413 (4)

	
	
	3.27. Arsenic
	БДС ISO 17378-2, Method B (1,2,3,4,5,6)

	
	
	3.28. Sodium
	БДС ISO 9964-3 (4,5)

	
	
	3.29. Potassium
	БДС ISO 9964-3 (4,5)

	
	
	3.30. Calcium
	БДС EN ISO 7980 (4,5)

	
	
	3.31. Magnesium
	БДС EN ISO 7980 (4,5)

	
	
	3.32. Total hardness (sum of calcium and magnesium)/ Calcium carbonate hardness
	БДС ISO 6059 (2,4,5)

	
	
	3.33. Dissolved oxygen
	БДС EN 25813 (2,3,4,5)

	
	
	3.34. Aluminum
	БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.35. Antimony
	БДС EN ISO 17294-2 (1,2,3,4,5,6)

	
	
	3.36. Selenium
	БДС EN ISO 17294-2 (1,2,3,4,5,6)

	4.
	Soils
	4.1. pH (H2O)
       pH (CaCl2)
       pH (KCl)
	БДС EN ISO 10390

	
	
	4.2. Lead
	ISO 11047, Method A

	
	
	4.3. Zinc
	

	
	
	4.4. Cadmium
	

	
	
	4.5. Copper
	

	
	
	4.6. Chrome
	

	
	
	4.7. Cobalt
	

	
	
	4.8. Manganese
	

	
	
	4.9. Nickel
	

	
	
	4.10. Arsenic
	ISO 20280, Method B

	5.
	Industrial noise
	5.1. Noise level
	БДС ISO 8297
VILM 1-6:2008

	
	
	5.2. Equivalent noise level
	

	
	
	5.3. Average noise level on the measuring circuit
	

	
	
	5.4. Total sound power level
	

	
	
	5.5. Noise level at the impact site
	VILM 1-6:2008



To perform sampling of:
	Type of the scope: flexible *

	№
	Product
	Sampling method (standard/ validated methods)

	1
	2
	3

	1.
	Emissions of harmful substances released into the air from facilities with stationary sources
	БДС EN 13284-1, 
БДС ISO 9096,
БДС EN 14790, 
БДС 17.2.4.04, 
БДС 17.2.4.09

	2.
	Immissions 
	БДС 17.2.5.01, 
БДС 17.2.4.20,
БДС EN 14902, cl. 8

	3.
	Water:
(1) industrial,
(2) running surface,
(3) waste,
(4) drinking,
(5) groundwater,
infiltrates
	БДС ISO 5667-5 (4),
БДС EN ISO 5667-6 (2),
БДС ISO 5667-10 (1,3,6),
БДС ISO 5667-11 (5)

	4.
	Soils
	БДС ISO 18400-102, 
БДС ISO 18400-104



*Flexible scope: The introduction of a new version of the standard/document or standards/documents, which replace them, is permitted. The laboratory keeps an updated list of the standards and their dated versions.

Fixed scope reference:
1. VILM 1-1 Determination of the content of sulfur dioxide, carbon oxide, nitrogen oxides-total and oxygen in gas streams.
2. VILM 1-2 Determination of the content of lead, zinc and cadmium in gas streams.
3. VILM 1-3 Determination of the content of lead, zinc and cadmium in the air.
4. VILM 1-5 Determination of cyanide content in water samples.
5. VILM 1-6 Determination of total sound power released in the environment from industrial plant and determination of noise level at the impact site.
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