
SCOPE 24 ЛК
Sofia, 15.07.2026
VRS CONTROL LTD
CALIBRATION LABORATORY
Management address:
1517, Sofia, Poduyane, 26 Vasil Kanchev Str, Block Section B, Entr. G, Floor 5, Office 23
Laboratory address:
1298, Sofia, Trebich, 139 Rozhen Blvd.
To perform calibration of:
	Type of the scope: fixed
	

	№
	Measuring instrument
	Measured value,
unit of measure
	Measurement Range
	Measurement uncertainty
	Calibration method

	1
	2
	3
	4
	5
	6

	1.
	Tanks:
-horizontal made of metal and non-metal, mounted stationary and on mobile platforms;
- with different geometric shape;
- vertical or cylindrical
	Volume, 
m3
	from 2,5 m3 
to 60 m3
	0,20%
	МК 7-2.1/2026
(based on 
ISO 4269:2001 -volumetric method)


	2.
	Tanks:
-horizontal, cylindrical, made of metal and non-metal, mounted stationary and on mobile platforms
	Volume, 
m3
	form 5 m3 
to 100 m3
	0,30%
	МК 7-2.2/2026
(based on 
ISO 12917-1:2017, 
ISO 7507-1:2003 -geometrical method, strapping method)

	3.
	Tanks:
-vertical, cylindrical, made of metal and non-metal.
Mounted stationary and on mobile platforms;
	Volume, 
m3
	form 5 m3 
to 100 m3
	0,30%
	МК 7-2.3/2026
(based on 
ISO 7507-1:2003 – strapping method)


Note: Calibration is performed at the customer's site.
Reference:
1. МК 7-2.1/2026 Method for calibration of tanks for liquids other than water by volumetric method (based on ISO 4269:2001 Petroleum and liquid petroleum products - Calibration of tanks by measuring the liquid - Incremental method using volume measuring instruments).

2. MK 7-2.2/2026 Method for calibration of horizontal tanks for liquids by geometric method (based on ISO 12917-1:2017 Petroleum and liquid petroleum products — Calibration of horizontal cylindrical tanks – Part 1: Manual methods, ISO 7507-1:2003 Petroleum and liquid petroleum products — Calibration of vertical cylindrical tanks – Part 1: Strapping method) (introduced with БДС ISO 7507-1:2016 Petroleum and liquid petroleum products. Calibration of vertical cylindrical tanks. Part 1: Strapping method). 

3. MK 7-2.3/2026 Method for calibration of vertical tanks by geometric method (based on ISO 7507-1:2003 Petroleum and liquid petroleum products — Calibration of vertical cylindrical tanks – Part 1: Strapping method) (introduced with БДС ISO 7507-1:2016 Petroleum and liquid petroleum products — Calibration of vertical cylindrical tanks – Part 1: Strapping method).
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