SCOPE 252 ЛИ
Sofia, 20.07.2026
CENTER FOR TESTING AND EUROPEAN CERTIFICATION LTD
CONSTRUCTION PRODUCTS TESTING LABORATORY 
Management and  laboratory address: 
6006 Stara Zagora, Industrial Quarter, 2 Industrialna Str.

[bookmark: _Hlk236296074]To perform testing of:
	Type of the scope: flexible*

	№ 
	Tested products
	Type of test / characteristic
	Testing methods
(standard/ validated method)

	1
	2
	
	3
	4

	1.
	Building lime 
	1.1
	Maintaining a constant volume/slaked/
	БДС EN 459-2

	
	
	1.2
	Extraction of lime slurry
	БДС EN 459-2

	
	
	1.3
	Subtlety of grinding
	БДС EN 459-2, cl.7.1

	
	
	1.4
	Connection time
	БДС EN 459-2

	
	
	1.5
	Spreading diameter
	БДС EN 459-2

	
	
	1.6
	Ability to retain water
	БДС EN 459-2

	
	
	1.7
	Air content 
	БДС EN 459-2

	
	
	1.8
	Bulk density
	БДС EN 459-2

	
	
	1.9
	Free water
	БДС EN 459-2

	
	
	1.10
	Reactivity
	БДС EN 459-2

	
	
	1.11
	CaO+MgO content
	БДС EN 459-2

	
	
	1.12
	Active MgO content
	БДС EN 459-2

	
	
	1.13
	SO3 content
	БДС EN 459-2

	
	
	1.14
	CO2 content
	БДС EN 459-2, cl. 6.6

	
	
	1.15
	Loss ignition
	БДС EN 459-2

	
	
	1.16
	Content of available lime
	БДС EN 459-2 

	2.
	Gypsum binders and gypsum plasters (1) 

and gypsum-based construction products (2)
	2.1
	Particle size distribution
	БДС EN 13279-2 (1)

	
	
	2.2
	Content of CaSO4
	БДС EN 13279-2 (1)

	
	
	2.3
	Ratio of water / plaster 
	БДС EN 13279-2 (1)

	
	
	2.4
	Beginning connection
	БДС EN 13279-2, cl. 4.4.1 (1)

	
	
	2.5
	Bending strength
	БДС EN 13279-2 (1)

	
	
	2.6
	Compressive strength
	БДС EN 13279-2 (1)

	
	
	2.7
	SO3 content  
	БДС EN 13279-2 (1)

	
	
	2.8
	Hardness
	БДС EN 13279-2 (1)

	
	
	2.9
	Presence of cracks
	БДС EN 13963 (1)

	
	
	2.10
	Strength of adhesion
	БДС EN 13279-2 (1)

	
	
	2.11
	Dimensions / thickness, height, length /
	БДС EN 520+A1 (2);
БДС EN 12859 (2); 
БДС EN 15283-1+A1 (2);
БДС EN 15283-2+A1 (2)

	
	
	2.12
	Density 
	БДС EN 520+A1 (2);
БДС EN 12859 (2); 
БДС EN 15283-2+A1 (2)

	
	
	2.13
	Flatness
	БДС EN 12859 (2)

	
	
	2.14
	Mass
	БДС EN 12859 (2)

	
	
	2.15
	Bending strength-breaking load
	БДС EN 520+A1 (2);
БДС EN 12859 (2);
БДС EN 15283-1+A1 (2)

	
	
	2.16
	Tensile strength in bending
	БДС EN 15283-2+A1 (2);
БДС EN 14353 (2)

	
	
	2.17
	рН value
	БДС EN 12859 (2);
БДС EN 12860 (1)

	
	
	2.18
	Moisture content
	БДС EN 12859 (2)

	
	
	2.19
	Water absorption
	БДС EN 12859 (2)

	
	
	2.20
	Total water absorption
	БДС EN 520+A1 (2); 
БДС EN 15283-1+A1 (2);
БДС EN 15283-2+A1 (2)

	
	
	2.21
	Surface hardness
	БДС EN 520+A1 (2);
БДС EN 15283-1+A1 (2);
БДС EN 15283-2+A1 (2)

	
	
	2.22
	Shear strength
	БДС EN 520+A1 (2);
БДС EN 15283-2+A1 (2)

	
	
	2.23
	Thermal resistance/ thermal conductivity
	БДС EN 13815, Annex В (2);
БДС EN ISO 6946, cl. 5.1 (2)

	3.
	Steel for reinforcement of concrete. Weldable
 reinforcing steels
	3.1
	Extension
	БДС EN ISO 15630-1

	
	
	3.2
	Nominal diameter
	БДС EN ISO 15630-1

	
	
	3.3
	Nominal cross section area
	БДС EN ISO 15630-1

	
	
	3.4
	Nominal linear mass
	БДС EN ISO 15630-1

	
	
	3.5
	Cohesion
	БДС EN ISO 15630-1

	
	
	3.6
	Terms of voltage (maximum strength / flow limit and tensile)
	БДС EN ISO 15630-1

	
	
	3.7
	Limit of yield strength under tensile
	БДС EN ISO 15630-1

	
	
	3.8
	Tensile strength
	БДС EN ISO 15630-1

	4.
	Aggregates (1) / 
rock materials (2)
	4.1
	Particle size distribution
	БДС EN 933-1 (1,2);
БДС EN 13383-2 (2)

	
	
	4.2
	Fine particle content, passing through a 0.063 mm sieve
	БДС EN 933-1(1)

	
	
	4.3
	Particle density 

Particle density:
- apparent particle density;
- oven-dried particle density;
- saturated and surface-dried particle density;
- pre-dried particle density
	БДС EN 13383-2 (2);

БДС EN 1097-6 (1)

	
	
	4.4
	Water absorption
	БДС EN 1097-6 (1);
БДС EN 13383-2 (2)

	
	
	4.5
	Flakiness index
	БДС EN 933-3 (1)

	
	
	4.6
	Shape index
	БДС EN 933-4 (1)

	
	
	4.7
	Shell content
	БДС EN 933-7 (1)

	
	
	4.8
	Sand equivalent
	БДС EN 933-8+A1 (1)

	
	
	4.9
	Resistance to fragmentation (Los Angeles)
	БДС EN 1097-2, cl. 5 (1,2)

	
	
	4.10
	Resistance to wear (micro-Deval)
	БДС EN 1097-1 (1,2)

	
	
	4.11
	Resistance to freezing and thawing
	БДС EN 1367-1 (1,2)

	
	
	4.12
	Weathering resistance with MgSO4
	БДС EN 1367-2 (1,2)

	
	
	4.13
	Bulk density
	БДС EN 1097-3 (1,2)

	
	
	4.14
	Resistance to fragmentation
	БДС EN 206+A2/NA (Annex NА.Q.) (1)

	
	
	4.15
	Adhesion with bitumen
	БДС EN 12697-11, cl. 6 (1, 2)

	
	
	4.16
	Assessment of fines with methylene blue (fines/methylene blue value)
	БДС EN 933-9 (1, 2)

	
	
	4.17
	Determination of percentage of:
- crushed particles,
- totally crushed particles,
- totally rounded particles
	БДС EN 933-5+A1 (1, 2)

	
	
	4.18
	Chlorides content
	БДС EN 1744-1+A1 (1, 2)

	
	
	4.19
	Acid soluble sulphates content
	БДС EN 1744-1+A1 (1, 2)

	
	
	4.20
	Water soluble sulphates
	БДС EN 1744-1+A1, 
cl. 10.1 (1, 2)

	
	
	4.21
	Sulphur SO3 content  
	БДС EN 1744-1+A1, 
cl. 11.1 (1, 2)

	
	
	4.22
	Contaminations with low weight
	БДС EN 1744-1+A1 (1, 2)

	
	
	4.23
	Availability of organic components - humus
	БДС EN 1744-1+A1, 
cl. 15.1 (1, 2)

	
	
	4.24
	Resistance to alkali-silicon reaction (determination of silicon)
	БДС 14851, cl. 8 (1)

	
	
	4.25
	Water content
	БДС EN 1097-5 (1, 2)

	
	
	4.26
	Water-soluble salts content
	БДС 11301 (1, 2)

	
	
	4.27
	Content of fines passing through a 0.5 mm sieve
	БДС EN 933-1 (2)

	
	
	4.28
	Content of particles with length ≥100mm
	БДС EN 13450 (2)

	
	
	4.29
	Resistance to freezing and thawing - direct freezing 25 cycles
	БДС EN 13383-2 (2)

	
	
	4.30
	Compressive strength
	БДС EN 1926 (2)

	
	
	4.31
	Particles shape
	БДС EN 13383-2 (2)

	
	
	4.32
	Calcium carbonate content
	БДС EN ISO 3262-1 (1, 2)

	
	
	4.33
	Magnesium carbonate content
	БДС EN ISO 3262-1 (1, 2)

	
	
	4.34
	Polished stone value
	БДС EN 1097-8

	5.
	Construction mortars
	5.1
	Consistence
	БДС EN 1015-3+A1+A2;
БДС EN 1015-4 

	
	
	5.2
	Bulk density
	БДС EN 1015-6+A1

	
	
	5.3
	Air content of fresh mortar
	БДС EN 1015-7, cl. 7

	
	
	5.4
	Compressive strength of hardened mortar
	БДС EN 1015-11 

	
	
	5.5
	Flexural strength of hardened mortar
	БДС EN 1015-11 

	
	
	5.6
	Chloride content
	БДС EN 1015-17+A1

	
	
	5.7
	Dry bulk density
	БДС EN 1015-10+A1

	
	
	5.8
	Particle size distribution
	БДС EN 1015-1+A1

	6.
	Hardened concrete
	6.1
	Compressive strength
	БДС EN 12390-3 

	
	
	6.2
	Density
	БДС EN 12390-7 

	
	
	6.3
	Freeze/thaw resistance:
- loss of mass, 
- loss of compressive, strength
	БДС EN 206+A2/NA 
(Annex NА.О.1)

	
	
	6.4
	Water impermeability, Maximum penetration of water
	БДС EN 206+A2/NA 
(Annex NА.N);
БДС EN 12390-8

	
	
	6.5
	Rebound number 
	БДС EN 12504-2

	
	
	6.6
	Compressive strength of cored specimens
	БДС EN 12504-1

	
	
	6.7
	Flexural strength
	БДС EN 12390-5, 
Annex A

	7.
	Fresh concrete


	7.1
	Slump-test
	БДС EN 12350-2 

	
	
	7.2
	Density
	БДС EN 12350-6

	
	
	7.3
	Air content 
	БДС EN 12350-7

	
	
	7.4
	Consistency - slump-flow diameter
	БДС EN 12350-8

	
	
	7.5
	 V-funnel flow time
	БДС EN 12350-9

	
	
	7.6
	Passing ability ratio - L box test
	БДС EN 12350-10

	
	
	7.7
	Sieve segregation
	БДС EN 12350-11

	
	
	7.8
	J-ring test:
- passing ability (PJ),
- slump-flow diameter (SFJ),
- flow time (t500J)
	БДС EN 12350-12

	8.
	Concrete kerb units
	8.1
	Geometric dimensions: 
- length, 
- width, 
- height
	БДС EN 1340

	
	
	8.2
	Straightness/bow
	БДС EN 1340

	
	
	8.3
	Draw (Rake angle)
	БДС EN 1340

	
	
	8.4
	Bending strength
	БДС EN 1340

	
	
	8.5
	Abrasion resistance 
	БДС EN 1340

	
	
	8.6
	Water absorption
	БДС EN 1340

	
	
	8.7
	Freeze/thaw resistance - mass loss
	БДС EN 1340

	
	
	8.8
	Visual aspects:
-presence of defects in appearance, 
-presence of defects in texture,
-presence of defects in color
	БДС EN 1340

	
	
	8.9
	Slip resistance
	БДС EN 1340

	9.
	Concrete flags for tile lining on road water gang
	9.1
	Geometric dimensions: 
- length, 
- width, 
- thickness, 
- difference in the diagonals
	БДС 11482

	
	
	9.2
	Distortions in planes: 
- side planes,
- upper and lower plane
	БДС 11482

	
	
	9.3
	Bending strength
	БДС 11482

	
	
	9.4
	Water absorption
	БДС 11482

	
	
	9.5
	Freeze/thaw resistance: 
- reduce the mass,
- reduce the tensile strength in bending
	БДС 11482

	10.
	Concrete paving flags
	10.1
	Geometric dimensions:
 - length, 
- width, 
- height, 
- diagonals
	БДС EN 1339

	
	
	10.2
	Flatness/bow
	БДС EN 1339

	
	
	10.3
	Water absorption
	БДС EN 1339

	
	
	10.4
	Freeze/thaw resistance
mass loss
	БДС EN 1339

	
	
	10.5
	Bending strength
	БДС EN 1339

	
	
	10.6
	Breaking load
	БДС EN 1339

	
	
	10.7
	Abrasion resistance 
	БДС EN 1339

	
	
	10.8
	Visual aspects: 
-presence of defects in appearance,
 -presence of defects in texture,
-presence of defects in color
	БДС EN 1339

	
	
	10.9
	Slip resistance
	БДС EN 1339

	11.
	Concrete roofing tiles
	11.1
	Hanging length
	БДС EN 491

	
	
	11.2
	Cover width
	БДС EN 491

	
	
	11.3
	Flatness
	БДС EN 491

	
	
	11.4
	Mass
	БДС EN 491

	
	
	11.5
	Mechanical resistance (transverse strength)
	БДС EN 491

	
	
	11.6
	Water impermeability - appearance of falling water drops
	БДС EN 491

	
	
	11.7
	Mechanical resistance (transverse strength) after freeze-thaw resistance
	БДС EN 491

	
	
	11.8
	Water impermeability - appearance of falling water drops after freeze-thaw resistance
	БДС EN 491

	12.
	Concrete chute for unwater on road water gang
	12.1
	Geometric dimensions:
- length, 
- width, 
- height
	БДС 11483

	
	
	12.2
	Availability on cracks
	БДС 11483

	
	
	12.3
	Break off the edges: 
- number, 
- depth, 
- length
	БДС 11483

	
	
	12.4
	Availability on roughness: 
- number, 
- height, 
- width, 
- length
	БДС 11483

	
	
	12.5
	Pores on the front surface:
- number, 
- depth, 
- area
	БДС 11483

	
	
	12.6
	Freeze/thaw resistance: 
- loss of mass, 
- loss of strength
	БДС EN 206+A2/NA – (Annex NA.O.1)

	13.
	Concrete paving blocks
	13.1
	Geometric dimensions:
- length, 
- width, 
- thickness, 
- diagonals
	БДС EN 1338

	
	
	13.2
	Flatness/bow
	БДС EN 1338

	
	
	13.3
	Visual aspects: 
- presence of defects in appearance, 
- presence of defects in texture, 
- presence of defects in color
	БДС EN 1338

	
	
	13.4
	Tensile splitting strength:
- average, 
- single
	БДС EN 1338

	
	
	13.5
	Breaking load
	БДС EN 1338

	
	
	13.6
	Abrasive wear
	БДС EN 1338

	
	
	13.7
	Water absorption 
	БДС EN 1338

	
	
	13.8
	Freeze/thaw resistance 
	БДС EN 1338

	
	
	13.9
	Slip resistance 
	БДС EN 1338

	14.
	 Clay roofing tiles
	14.1
	Single dimensions:
- length, 
- width 
	БДС EN 1024 

	
	
	14.2
	Size of overlap: 
- Average length of overlap, 
- Maximum length of overlap, 
- Average width of overlap, 
- Maximum width of overlap
	БДС EN 1024

	
	
	14.3
	Distortion 
	БДС EN 1024

	
	
	14.4
	Construction characteristics: 
- break, 
- structural crack, 
- loss of nib
	БДС EN 1304

	
	
	14.5
	Impermeability
	БДС EN 539-1, cl. 6

	
	
	14.6
	Flexural strength 
	БДС EN 538

	
	
	14.7
	Frost resistance 
	БДС EN 539-2

	
	
	14.8
	Mass
	БДС EN 1024

	15.
	 Ceramic tiles
	15.1
	Geometric dimensions:
- length, 
- width, 
- thickness 
	БДС EN ISO 10545-2

	
	
	15.2
	Straightness 
	БДС EN ISO 10545-2

	
	
	15.3
	Squareness 
	БДС EN ISO 10545-2

	
	
	15.4
	Flatness 
	БДС EN ISO 10545-2

	
	
	15.5
	- Surface Defects, 
- Decorative defects 
	БДС EN ISO 10545-2

	
	
	15.6
	Water absorption
	БДС EN ISO 10545-3

	
	
	15.7
	Bending strength 
	БДС EN ISO 10545-4

	
	
	15.8
	Resistance to shock: 
- Coefficient of reciprocating motion, 
- Presence of chipped or cracking
	БДС EN ISO 10545-5

	
	
	15.9
	Resistance to surface abrasion: 
- number of revolutions without visible wear, 
- loss of mass
	БДС EN ISO 10545-7

	
	
	15.10
	Thermal resistance - number of specimens with visible defects 
	БДС EN ISO 10545-9

	
	
	15.11
	Moisture extension 
	БДС EN ISO 10545-10

	
	
	15.12
	Cold resistance - number of damaged specimens after 100 cycles 
	БДС EN ISO 10545-12

	16.
	 Masonry units

	16.1
	Geometric dimensions:
- length, 
- width, 
- height 
	БДС EN 772-16 

	
	
	16.2
	Length of the diagonal 
Flatness of based 
	БДС EN 772-20+A1

	
	
	16.3
	Thickness of exposed walls 
	БДС EN 772-16 

	
	
	16.4
	Thickness of partition walls 
	БДС EN 772-16 

	
	
	16.5
	Density: 
- Net density, 
- gross density 
	БДС EN 772-13

	
	
	16.6
	Compressive strength
	БДС EN 772-1+А1

	
	
	16.7
	Content of the active soluble salts -magnesium ions 
	БДС EN 772-5, cl. 10

	
	
	16.8
	Water absorption
	БДС EN 772-11

	
	
	16.9
	Freeze-thaw resistance
	БДС EN 772-18

	
	
	16.10
	Net volume 
Percentage of voids
	БДС EN 772-2+A1;
БДС EN 772-3

	
	
	16.11
	Equivalent thermal conductivity
	БДС EN 1745;
БДС EN 12664

	17.
	Waterproofing products
 
	17.1
	Geometric dimensions: 
- length, 
- width, 
- straightness
	БДС EN 1848-1

	
	
	17.2
	Flexibility at low temperatures – presence of cracks
	БДС EN 1109

	
	
	17.3
	Mass per unit area
	БДС EN 1849-1 

	
	
	17.4
	Relatively extension
	БДС EN 12311-1

	
	
	17.5
	Water impermeability - visible crossing the water
	БДС EN 1928;
БДС EN 15820

	
	
	17.6
	Resistance to tearing (nail shank)
	БДС EN 12310-1

	
	
	17.7
	Shear resistance of joints
	БДС EN 12317-1

	
	
	17.8
	Peel resistance of joints
	БДС EN 12316-1

	
	
	17.9
	Tensile strength:
- in longitudinal direction,
- in transverse direction
	БДС EN 12311-1

	
	
	17.10
	Thickness
	БДС EN 1849-1 

	
	
	17.11
	Resistance to water penetration
	БДС EN 13111

	18.
	Thermal insulating products 
	18.1
	Length
	БДС EN ISO 29465

	
	
	18.2
	Width
	БДС EN ISO 29465

	
	
	18.3
	Thickness
	БДС EN ISO 29466

	
	
	18.4
	Flatness
	БДС EN ISO 29468

	
	
	18.5
	Squareness
	БДС EN 824

	
	
	18.6
	Apparent density
	БДС EN ISO 29470

	
	
	18.7
	Compressive stress at 10 % relative deformation
	БДС EN ISO 29469

	
	
	18.8
	Bending strength
	БДС EN 12089 

	
	
	18.9
	Long term water absorption by immersion
	БДС EN ISO 16535

	
	
	18.10
	Deformation under specified compressive load and temperature conditions
	БДС EN 1605

	
	
	18.11
	Tensile strength perpendicular to faces
	БДС EN 1607

	
	
	18.12
	Organic content
	БДС EN 13820

	
	
	18.13
	Thermal conductivity coefficient/ Thermal resistance
	БДС EN 12667;
БДС EN 12939

	19.
	Building soils
	19.1
	Water content
	    БДС 644**;
БДС EN 1097-5;
БДС EN ISO 17892-1+A1

	
	
	19.2
	Specific density
	    БДС 646**

	
	
	19.3
	Sieve analysis
	БДС EN ISO 17892-4

	
	
	19.4
	Volume density „substitute sand” Compacting factor
	AASHTO T 191

	
	
	19.5
	Organic carbon content
	БДС 11302

	
	
	19.6
	Humic substances
	БДС 11302

	
	
	19.7
	Water-soluble salts content
	БДС 11301

	
	
	19.8
	Uniformity coefficient
	    БДС 2761**

	
	
	19.9
	Plastic limit
	    БДС 648**

	
	
	19.10
	Liquid limit
	    БДС 648**

	
	
	19.11
	Plasticity index (consistency)
	    БДС 2761**

	
	
	19.12
	Standard density:
- maximum density,
- optimum moisture content
	БДС EN 13286-2

	
	
	19.13
	California Bearing Ratio (CBR)
	БДС EN 13286-47

	
	
	19.14
	Moisture content
	БДС EN 13286-46

	
	
	19.15
	Elastic modulus
	БДС 15130

	
	
	19.16
	Ratio of deformation modules
	БДС 15130

	
	
	19.17
	Bulk density
	БДС EN ISO 17892-2

	
	
	19.18
	Particle density
	БДС EN ISO 17892-3, 
cl. 5.1

	
	
	19.19
	Undrained shear strength
	БДС EN ISO 17892-6

	
	
	19.20
	- liquid limit, Wl,
- Plastic limit, Wp,
- Plasticity index, Ip
	БДС EN ISO 17892-12 +A1+A2

	20.
	Sinks (1) / Wash basins (2)



	20.1
	Draining of water - drained to waste outlet hole
	БДС EN 13310+A1 (1);
БДС EN 14688+A1 (2)

	
	
	20.2
	Resistance to dry heat – presence of changes of appearance of the surface
	БДС EN 13310+A1 (1);
БДС EN 14688+A1 (2)

	
	
	20.3
	Resistance to chemicals and staining agents - presence of permanent surface changes
	БДС EN 13310+A1 (1);
БДС EN 14688+A1 (2)

	21.
	Screed material and floor screeds
	21.1
	Compressive strength
	БДС EN 13892-2 

	
	
	21.2
	Bending strength
	БДС EN 13892-2 

	
	
	21.3
	Wear resistance-Bohme
	БДС EN 13892-3 

	
	
	21.4
	Surface hardness
	БДС EN 13892-6 

	
	
	21.5
	Bond strength
	БДС EN 13892-8

	
	
	21.6
	Release of aggressive substances - pH value
	БДС EN 13454-2

	22.
	 Adhesives for tiles
	22.1
	Initial tensile adhesion strength
	БДС EN 12004-2 

	
	
	22.2
	Tensile adhesion strength after water immersion 
	БДС EN 12004-2 

	
	
	22.3
	Tensile adhesion strength after heat aging
	БДС EN 12004-2 

	
	
	22.4
	Tensile adhesion strength after freeze-thaw cycle 
	БДС EN 12004-2 

	
	
	22.5 
	Open time
	БДС EN 12004-2 

	
	
	22.6
	Slip
	БДС EN 12004-2 

	
	
	22.7
	Transverse deformation
	БДС EN 12004-2 

	
	
	22.8
	Shear adhesion strength
	БДС EN 12004-2 

	23.
	 Bituminous mixtures
	23.1
	Volume density
	БДС EN 12697-6,
 Procedure D

	
	
	23.2
	Thickness of a bituminous pavement/core
	БДС EN 12697-36, cl. 6.1

	
	
	23.3
	Void content
	БДС EN 12697-8

	
	
	23.4
	Temperature
	БДС EN 12697-13

	
	
	23.5
	Maximum density
	БДС EN 12697-5,
Procedure В

	24.
	Mixing water for concrete
	24.1
	Determination of pH
	БДС ISO 4316

	
	
	24.2
	Oils and fats
	БДС EN 1008 

	
	
	24.3
	Detergents
	БДС EN 1008 

	
	
	24.4
	Color
	БДС EN 1008 

	
	
	24.5
	Suspended matter
	БДС EN 1008 

	
	
	24.6
	Odor
	БДС EN 1008 

	
	
	24.7
	Presence of hydrogen sulphide odor
	БДС EN 1008 

	
	
	24.8
	Humic matter
	БДС EN 1008

	
	
	24.9
	Determination of chloride
	БДС EN 196-2 

	
	
	24.10
	Determination of sulphate
	БДС EN 196-2 

	25.
	Siliceous fly ash
	25.1
	Chloride content
	БДС EN 196-2 

	
	
	25.2
	Sulphate content (as SO3)
	БДС EN 196-2 

	
	
	25.3
	Loss on ignition
	БДС EN 196-2 

	26.
	Admixtures for concrete, mortar and grout
	26.1
	Homogeneity
	БДС EN 934-1

	
	
	26.2
	Color
	БДС EN 934-1

	
	
	26.3
	pH value (for liquid admixtures only)
	БДС ISO 4316

	
	
	26.4
	Water soluble chloride
	БДС EN 480-10

	27.
	Construction products, products and components


	27.1
	Non-combustibility: 
- Mass loss,
- Duration of sustained flaming,
- Temperature rise
	БДС EN ISO 1182

	
	
	27.2
	Gross heat of combustion (calorific value)
	БДС EN ISO 1716

	
	
	27.3
	Single-flame source test:
- Ignition,
- Flame tip reaches 150 mm,
- Time at which flame tip reaches 150 mm,
- Ignition of the filter paper,
- Physical behavior of the test specimen
	БДС EN ISO 11925-2

	
	
	27.4
	Thermal attack by a single burning item:
- Heat release,
- Fire growth rate index,
- Presence of lateral flame spread,
- Smoke growth rate index,
- Total smoke production within 600 s,
- Production of flaming droplets and particles
	БДС EN 13823+A1

	
	
	27.5
	Determination of the burning behavior using a radiant heat source:
- CHF or HF-30,
- Flame spread,
- Time for flame spread,
- Duration on testing,
- Smoke measurement
	БДС EN ISO 9239-1

	28.
	 Ladders

	28.1
	Functional sizes
	БДС EN 131-1+A2

	
	
	28.2
	Permanent deformation after strength test 
	БДС EN 131-2+A3

	
	
	28.3
	Deformation after bending test
	БДС EN 131-2+A3

	
	
	28.4
	Deformation after lateral deflection test
	БДС EN 131-2+A3

	
	
	28.5
	Permanent deformation after bottom stile ends test
	БДС EN 131-2+A3

	
	
	28.6
	Permanent deformation after vertical load on steps and platforms
	БДС EN 131-2+A3

	29.
	Wood-based panels. Wood flooring and parquet 
	29.1
	Bending strength
	БДС EN 310

	
	
	29.2
	Modulus of elasticity
	БДС EN 310

	
	
	29.3
	Tensile strength perpendicular to the plane of the surface layer
	БДС EN 311

	
	
	29.4
	Resistance to
axial withdrawal of screws
	БДС EN 320

	
	
	29.5
	Swelling in thickness after immersion in water
	БДС EN 317

	
	
	29.6
	Tensile strength perpendicular to the plane of the board
	БДС EN 319

	
	
	29.7
	Moisture content
	БДС EN 322

	
	
	29.8
	Density
	БДС EN 323

	
	
	29.9
	Dimensions: thickness, width, 
length
	БДС EN 324-1

	
	
	29.10
	Moisture resistance under cyclic test conditions:
- Swelling in thickness;
- Bending strength;
- Tensile strength perpendicular to the plane of the board
	БДС EN 321

	
	
	29.11
	Bending strength
	БДС EN 1533

	
	
	29.12
	Slip
	СД CEN/TS 15676

	
	
	29.13
	Thermal conductivity
	БДС EN 14342 

	30.
	Products from natural rock materials (1) / 
 Agglomerated rock materials (2)
	30.1
	Water absorption coefficient by capillarity
	БДС EN 1925 (1)

	
	
	30.2
	Flexural strength
	БДС EN 12372 (1)

	
	
	30.3
	Compressive strength
	БДС EN 1926 (1)

	
	
	30.4
	Slip resistance
	БДС EN 14231 (1, 2)

	
	
	30.5
	Water absorption
	БДС EN 13755 (1)
БДС EN 14617-1 (2)

	
	
	30.6
	Frost resistance
	БДС EN 12371 (1)

	
	
	30.7
	Apparent density
	БДС EN 14617-1 (2)

	
	
	30.8
	Flexural strength
	БДС EN 14617-2 (2)

	
	
	30.9
	Tactility
	БДС EN 15285, cl. 4.2.12 (2)

	31.
	Gully tops and manhole tops for vehicular and pedestrian areas
	31.1
	Load bearing capacity:
load bearing capacity,
permanent deformation
	
БДС EN 124-1
БДС EN 124-1

	32.
	Drainage channels
	32.1
	Water tightness - jointing of drainage channel units
	БДС EN 1433+A1 

	
	
	32.2
	Maximum load bearing capacity
	БДС EN 1433+A1 

	
	
	32.3
	Deformation under load - permanent load
	БДС EN 1433+A1 

	
	
	32.4
	Durability:
- compressive strength,
- water absorption,
- freeze/ thaw
	БДС EN 1433+A1


	33.
	Cement
	33.1
	Compressive strength
	БДС EN 196-1

	
	
	33.2
	Flexural strength
	БДС EN 196-1

	
	
	33.3
	Setting times:
-initial setting time,
-final setting time
	БДС EN 196-3

	
	
	33.4
	Soundness 
- expansion
	БДС EN 196-3

	
	
	33.5
	SO3 content
	БДС EN 196-2

	
	
	33.6
	Residue insoluble:
- in hydrochloric acid and sodium carbonate,
- in hydrochloric acid and potassium hydroxide
	БДС EN 196-2

	
	
	33.7
	Loss of ignition
	БДС EN 196-2

	
	
	33.8
	Chloride content
	БДС EN 196-2

	34.
	Grout
	34.1
	Fluidity
	БДС EN 445, cl. 4.3.1;
БДС EN 14117

	
	
	34.2
	Wick-induced - bleeding
	БДС EN 445 

	
	
	34.3
	Wick-induced - volume change
	БДС EN 445 

	
	
	34.4
	Compressive strength
	БДС EN 445 

	
	
	34.5
	Density
	БДС EN 445 



To perform sampling of:
	Type of the scope: flexible*

	№ 
	Products
	Sampling methods
(standard/validated method)

	1
	2
	3

	1.
	Building lime
	БДС EN 459-2, cl. 3

	2.
	Gypsum binders and gypsum plasters
	БДС EN 13279-2, cl. 3.2.

	3.
	Steel for the reinforcement and prestressing of concrete
	БДС EN ISO 15630-1

	4.
	Aggregates
	БДС EN 932-1 

	5.
	Mortar for masonry
	БДС EN 1015-2+A1, cl. 5

	6.
	Hardened concrete
	БДС EN 12504-1

	7.
	Fresh concrete
	БДС EN 12350-1

	8.
	Concrete kerb units
	БДС EN 1340, cl. 6.2.3

	9.
	Concrete flags for tile lining on road water gang 
	БДС 11482, cl. 2

	10.
	Concrete paving flags
	БДС EN 1339, cl. 6.2.3

	11.
	Concrete roofing tiles
	БДС EN 490+A1, cl. 7

	12.
	Aggregate concrete masonry units
	БДС EN 771-3+A1, Annex А

	13.
	Concrete paving blocks
	БДС EN 1338, cl. 6.2.3

	14.
	Clay roofing tiles
	БДС EN 1304, cl. 6.4

	15.
	Ceramic tiles
	БДС EN 10545-1, cl. 6

	16.
	Clay masonry units
	БДС EN 771-1+A1, Annex А

	17.
	Flexible Bitumen sheets for waterproofing
	БДС EN 13416, cl. 5

	18.
	Building soils
	БДС EN 13286-1, Annex А

	19.
	Screed materials
	БДС EN 13892-1, cl. 3

	20.
	Cementitious adhesives
	БДС EN 1067

	21.
	Bituminous mixtures
	БДС EN 12697-27, cl. 4.1, cl. 4.7



*Flexible scope: Implementing a new version of standards/documents or standards/ documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by the CAB.

** Repealed but not replaced standard with regard to the testing method.
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