SCOPE 322 ЛИ 

CENTER FOR TESTING AND EUROPEAN CERTIFICATION LTD
LABORATORY FOR PERSONAL PROTECTIVE EQUIPMENT TESTING
Management and  laboratory address: 
6006, Stara Zagora, Industrial Quarter, 2 Industrialna Str.

To perform testing of:
	Type of the scope: flexible*

	№
	Tested products
	Type of test / characteristics
	Test methods
(standard/ validated method)

	1
	2
	3
	5

	1.
	Respiratory protective devices. Filtering half masks to protect against particles.
	1.1
	Leakage
(Total inward leakage)
	БДС EN 149:A1

	
	
	1.2
	Flammability
	БДС EN 149+A1

	
	
	1.3
	Strength of attachment of exhalation valve housing
	БДС EN 149:A1


	
	
	1.4
	Breathing Resistance
	БДС EN 149:A1

	
	
	1.5
	Flow impact of the exhalation valve
	БДС EN 149:A1


	
	
	1.6
	 Filter penetration
	БДС EN 149:A1;
БДС EN 13274-7

	
	
	1.7
	 Carbon dioxide content of the inhalation air
	БДС EN 149:A1


	
	
	1.8
	 Clogging
	БДС EN 149:A1

	2.
	Respiratory protective
devices. Particle
filters.
	2.1
	Mass
	БДС EN 143

	
	
	2.2
	Filter penetration
	БДС EN 143;
БДС EN 13274-7

	
	
	2.3
	Breathing Resistance
	БДС EN 143;
БДС EN 13274-3

	3.
	Respiratory protective
devices. Full face masks.
	3.1
	Carbon dioxide content of the inhalation air
	БДС EN 136

	
	
	3.2
	Breathing Resistance
	БДС EN 136

	
	
	3.3
	Leakage
(Total inward leakage)
	БДС EN 136

	4.
	Respiratory protective
devices. Half masks and quarter masks.
	4.1
	Flammability
	БДС EN 140;
БДС EN 140+AC

	
	
	4.2
	Carbon dioxide content of the inhalation air
	БДС EN 140;
БДС EN 140+AC 

	
	
	4.3
	Breathing Resistance
	БДС EN 140;
БДС EN 140+AC

	5.
	Respiratory protective devices. Half masks without inhalation valves and with separable filters to protect against gases or gases and particles or particles only.
	5.1
	Flammability
	БДС ЕN 1827+А1

	
	
	5.2
	Exhalation valve. Flow test
	БДС ЕN 1827+А1

	
	
	5.3
	Tensile test. Exhalation valve.
	БДС ЕN 1827+А1

	
	
	5.4
	Particle filter penetration 
	БДС EN 1827+A1;
БДС EN 13274-7

	
	
	5.5
	Clogging
	БДС ЕN 1827+А1;
БДС EN 149:A1

	
	
	5.6
	Carbon dioxide content of the inhalation air
	БДС ЕN 1827+А1

	
	
	5.7
	Breathing Resistance
	БДС ЕN 1827+А1

	6.
	Respiratory protective devices. Gas filter(s) and combined filter(s). 
	6.1
	Mass
	БДС EN 14387

	
	
	6.2
	Breathing Resistance
	БДС EN 14387;
БДС EN 13274-3

	
	
	6.3
	Filter penetration
	БДС EN 14387;
БДС EN 13274-7

	7.
	Textile products. Protective clothing for use against solid
Particulates.
	7
	Inward leakage 
into suit
	БДС EN 13982-2

	8.
	Textile products. Protective clothing for use against airborne solid particles including radioactive contamination.
	8
	Inward leakage 
into suit

	БДС EN 13982-2

	9.
	Community face coverings.
	9.1
	Head harness strength
	СД CEN/TS 17553

	
	
	9.2
	Material filtration efficiency
	БДС EN 13274-7

	
	
	9.3
	Breathing resistance
	БДС EN 13274-3

	10.
	Eye protective devices.
	10.1
	Resistance to mechanical impact
	БДС EN ISO 18526-3

	
	
	10.2
	Resistance to thermal exposure
	БДС EN ISO 18526-3

	
	
	10.3
	Resistance to corrosion
	БДС EN ISO 18526-3



*Flexible scope: Implementing a new version of standards/documents or standards/ documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.
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