SCOPE 12 ЛК
Sofia, 30.07.2026
SGS BULGARIA LTD.
CALIBRATION LABORATORY SGS BULGARIA

Management address:
1784, Sofia, Mladost District, 115G Tsarigradsko Shose Blvd.,
Megapark Business Center, Office C
Laboratory address:
8000, Burgas, Transportna Str., Condosco Business Center, Office 4

To perform calibration of:
	Type of the scope: fixed

	№
	Type of measuring instrument
	Measured quantity,
unit of measurement
	Measurement range
	Measurement uncertainty
	Calibration method

	1
	2
	3
	4
	5
	6

	1.
	Tanks of different shapes
	Volume, 
m³
	from 1 m³
to 75 m³
	0,20 %
	ISO 4269:2001,
Volumetric method

	2.
	Horizontal tanks
	Volume, 
m³
	from 1 m³
to 300 m³
	0,20 %
	ISO 12917-1:2017/ 
Amd 1:2025,
Tape method

	3.

	Vertical, cylindrical tanks
	Volume, 
m³
	from 10 m³
to 50,000 m³
	0,15 %
	ВЛМК 1:2015/
Edition 2 of 12.06.2023,
Electro-optical method

	
	
	Volume, 
m³
	from 100 m³
to 50,000 m³

	0,15 %
	БДС ISO 7507-4: 2016, Electro-optical method


Note: Calibration is performed on site at the customer.

References: ВЛМК 1:2015/Edition 2 of 12.06.2023. Method for calibration of vertical cylindrical tanks by geometric method through electro-optical measurement.
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