
SCOPE 176 ОКС
TYPE C INSPECTION BODY 

 CORTEX-5 LTD, CITY OF SOFIA
Registered office:
1434 city of Sofia, Simeonovo resid. quarter, 18 Krayrechna Str.

Office address:
1618 Sofia, Ovcha Kupel resid. quarter, 46, Ljubljana Str., Corpus A, office 1110

To execute inspection with the following scope:

	Scope type: flexible*

	No.
	Field of Inspection
	Type of Inspection
	Inspected parameter / characteristics
	Methods of testing / measurement used in the inspection
	Statutory instruments, standards, specifications, schemes

	1
	2
	3
	4
	5
	6

	1.
	Optical cable lines
	new and/or operating sites/facilities
	non-homogeneity insertion loss
	БДС EN 60793-1-40, PR 7.2.2
	Methodology for OCL measurement, 2002;

ICOCL – 2004;

TS

	2.
	Optical cable lines
	new and/or operating sites/facilities
	total attenuation
	БДС EN 61280-4-1

BDS EN 61280-4-2

(Annex A, B, C and D)

БДС EN 60793-1-22, PR 7.2.3
	Methodology for OCL measurement, 2002;

ICOCL – 2004;

TS


	No.
	Field of Inspection
	Type of Inspection
	Inspected parameter / characteristics
	Methods of testing / measurement used in the inspection
	Statutory instruments, standards, specifications, schemes

	1
	2
	3
	4
	5
	6

	3.
	Optical cable lines
	New and/or operating sites/facilities
	return loss
	БДС EN 61300-3-6, PR 7.2.4
	Methodology for OCL measurement, 2002;

ICOCL – 2004;

TS


* Introduction of new versions of standards/documents or of standards/documents, which supersede them, is allowed. A current list of the standards/documents with their dated versions is available from CIB.

Legend:

Methodology for OCL measurement, 2002 - Methodology for optical cable line measurement (BTC-SRIC [Scientific Research Institute for Communications], Sofia 2002);

ICOCL – 2004 – Instruction for the construction of optical cable lines (BTC-SRIC, 2004);

TS – Technical specification of the client.
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