**ORDER**

**№ A 533**

**Sofia, 31.08.2022**

**Inspection Body of Type A**

**at DEDAL – ATTESTATION AND CERTIFICATION LTD, NESEBAR**

**Management address**: 8230 Neseber, Mladost, bl. 50, Parter

**Office address:** 1574 Sofia, Slatina, 132, Geo Milev Str.

**To perform inspection of:**

| Type of the scope: Flexible\* | | | | | |
| --- | --- | --- | --- | --- | --- |
| **№** | **Field of Inspection** | **Type of Inspection** | **Parameter of Inspection / Characteristic** | **Test and Measurement Methods Used During Inspection, Inspection Procedure** | **Regulations, Standards, Specifications, Schemes** |
| 1 | 2 | **3** | 4 | 5 | 6 |
| 1**.** | Playgrounds, located indoor and / or outdoor | New and/or in use/ operation sites and facilities | Organisation and safety of playgrounds through complex inspection of documents, visual inspection and measurement / testing | Ordinance №1, SG №10/2009  БДС EN 1176-1  Documental – cl. 4.1, cl. 4.2, cl. 4.2.2, cl. 4.2.14, cl. 4.2.15, cl. 4.2.16, cl. 6  Visual inspection and measurement – cl. 4.2.3, cl. 4.2.4, cl. 4.2.5, cl. 4.2.6, cl. 4.2.7, cl. 4.2.8, cl. 4.2.9, cl. 4.2.10, cl. 4.2.11, cl. 4.2.12, cl. 4.2.13, cl. 4.2.16, cl. 7  БДС EN 1176-2 + AC  Documental – cl. 4.6, cl. 4.7, cl. 4.8, cl. 5.1, cl. 5.2, cl. 5.3  Visual inspection and measurement – cl. 4.2, cl. 4.3, cl. 4.4, cl. 4.5, cl. 4.9, cl. 4.10, cl. 7  БДС EN 1176-3  Documental – cl. 4.3.1, cl. 4.4.1,  Visual inspection and measurement – cl. 4.2, cl. 4.3., cl. 4.4, cl. 4.5, cl. 4.6, cl. 4.7, cl. 4.8, cl. 4.9, cl. 6  БДС EN 1176-4 + AC  Documental – cl. 4.2, cl. 4.3, cl. 4.4, cl. 4.9, cl. 4.10, cl. 6  Visual inspection and measurement – cl. 4.5, cl. 4.6, cl. 4.7, cl. 4.8, cl. 4.11, cl. 4.12, cl. 4.13, cl. 4.14, cl. 7  БДС EN 1176-5  Documental – cl. 4.6, cl. 5.1, cl. 5.3.2  Visual inspection and measurement – cl. 4.2 cl. 4.3, cl. 4.4, cl. 4.5, cl. 5.1, cl. 5.2, cl. 5.3.1, cl. 5.4, cl. 5.5, cl. 5.6, cl. 5.7, cl. 7  БДС EN 1176-6 + AC  Documental – cl. 4.3, cl. 5.1, cl. 5.2  Visual inspection and measurement – cl. 4.2, cl. 4.3, cl. 4.5, cl. 4.6, cl. 4.7, cl. 4.8, cl. 4.9, cl. 4.10, cl. 5.3, cl. 5.4, cl. 7  БДС EN 1176-7  Documental – cl. 4.2, cl. 5, cl. 5.1, cl. 5.2, cl. 6, cl. 7, cl. 8, cl. 8.2  БДС EN 1176-10  Documental – cl. 4.2.1, cl. 4.2.2.7, cl. 4.3.1, cl. 4.4.4.1, cl. 5 /1-5/  Visual inspection and measurement – cl. 4.2.2.1,  cl. 4.2.2.2, cl. 4.2.2.3, cl. 4.2.2.4, cl. 4.2.2.5, cl. 4.2.2.6, cl. 4.3.2.1, cl. 4.3.2.2, cl. 4.3.3, cl. 4.3.4, cl. 4.3.5, cl. 4.3.6, cl. 4.3.7, cl. 4.3.8, cl. 4.3.9, cl. 4.4.1, cl. 4.4.2, cl. 4.4.3, cl. 4.4.4.2  БДС EN 1176-11  Visual inspection and measurement – cl. 4.1, cl. 4.2, cl. 4.3, cl. 4.4, cl. 6  БДС EN 1177 + AC  Documental | Ordinance № 1, SG №10/2009 |

***\*Flexible scope:*** *Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.*