SCOPE 10 ЛИ
of SID 1 Ltd.
Fuel Testing laboratory
Management address: 

1756 Sofia, Darvenitsa, bl. 28, Entr. А, Apt. 5

Laboratory Address: 

1280 Novi Iskar, Kurilo District, 1 Kremenitsa Str, Petroleum Base Saxa

To perform testing of:
	Type of the scope: flexible for part of the scope*

	№


	Tested products
	Type of test / characteristic
	Testing methods
(standard / validated method)

	1
	2
	3
	4

	1.
	Automotive gasoline
	Appearance
	БДС EN 228+A1/NA, Table 1

	
	
	Vapor Lock Index
	БДС EN 228+A1/NA, cl. 5.5.2

	
	
	Benzene content
	БДС EN 238+A1

	
	
	Copper strip corrosion
	БДС EN ISO 2160

	
	
	Distillation characteristics
	БДС EN ISO 3405

	
	
	Density
	БДС EN ISO 3675

	
	
	Density
	БДС EN ISO 12185

	
	
	Vapour pressure (VP)
	БДС EN 13016-1

	
	
	Sulphur content
	БДС EN ISO 20846

	
	
	Oxygenates content - methanol, ethanol, ethers with 5 or more С atoms: MTBE, ETBE, TAME
	БДС EN 1601

	
	
	Oxygen content
	БДС EN 1601

	
	
	Bio component content
	VLMI № 007/2019

	2.
	Diesel engine fuel
	Cold filter plugging point (CFPP)
	БДС EN 116,

БДС EN 116/Amendment 1

	
	
	Copper strip corrosion
	БДС EN ISO 2160

	
	
	Flash point in closed cup
	БДС EN ISO 2719

	
	
	Kinematic viscosity
	БДС EN ISO 3104, Procedure A

	
	
	Distillation characteristics
	БДС EN ISO 3405

	
	
	Density
	БДС EN ISO 3675

	
	
	Density
	БДС EN ISO 12185

	
	
	Cetane index
	БДС EN ISO 4264

	
	
	Ash content
	БДС EN ISO 6245

	
	
	Total contamination
	БДС EN 12662

	
	
	Water content
	БДС EN ISO 12937

	
	
	Fatty acid methyl esters (FAME) content
	БДС EN 14078

Scope B

	
	
	Sulphur content
	БДС EN ISO 20846

	
	
	Cloud point
	БДС EN ISO 3015

	3.
	Biodiesel - fatty acid methyl esters
	Cold filter plugging point (CFPP)
	БДС EN 116,

БДС EN 116/Amendment 1

	
	
	Cloud point
	БДС EN ISO 3015

	
	
	Copper strip corrosion
	БДС EN ISO 2160

	
	
	Kinematic viscosity
	БДС EN ISO 3104, 

Procedure A

	
	
	Density
	БДС EN ISO 3675


	
	
	Density
	БДС EN ISO 12185

	
	
	Flash point in closed cup
	БДС EN ISO 2719

	
	
	Total contamination
	БДС EN 12662

	
	
	Water content
	БДС EN ISO 12937

	
	
	Sulphur content
	БДС EN ISO 20846

	
	
	Acid value
	БДС EN 14104

	
	
	Iodine value
	БДС EN 14111

	4.
	Gasoil for industrial and domestic purposes
	Freezing point
	БДС 1751

	
	
	Flash point in closed cup
	БДС EN ISO 2719

	
	
	Kinematic viscosity
	БДС EN ISO 3104, 

Procedure A

	
	
	Distillation characteristics
	БДС EN ISO 3405

	
	
	Density
	БДС EN ISO 3675

	
	
	Density
	БДС EN ISO 12185

	
	
	Water content
	БДС ISO 3733

	
	
	Ash content
	БДС EN ISO 6245

	
	
	Carbon residue
	БДС ISO 6615

	
	
	Total contamination
	БДС EN 12662

	
	
	Sulphur content
	БДС EN ISO 20846

	5.
	Fuel oils
	Freezing point
	БДС 1751

	
	
	Flash point in opened cup
	БДС EN ISO 2592

	
	
	Density
	БДС EN ISO 3675

	
	
	Density
	БДС EN ISO 12185

	
	
	Water soluble acids and bases
	БДС 5252

	
	
	Ash content
	БДС EN ISO 6245

	
	
	Water and sediments
	БДС ISO 3734

	
	
	Sulphur content
	БДС EN ISO 20846


To perform sampling of:
	Type of the scope: flexible*

	№
	Product
	Sampling methods
(standard / validated method)

	1
	2
	3

	1.
	Liquid fuels (automotive gasoline, diesel engine fuel, biodiesel, gas oil for industrial and domestic purposes, fuel oils)
	БДС EN ISO 3170


Flexible scope: Implementing a new version of standards/documents or standards / documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.

Fixed scope references:
	VLMI  № 007/2019 -
	Light petroleum products. Liquid fuels. Lead-free automotive gasolines. Determination of the contents of bio-components
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