SCOPE 1ЛИ
Sofia, 26.04.2024
ELLATZITE-MED AD
TESTING LABORATORY

Management address: 2086 Mirkovo, Mirkovo Municipality, Sofia-Region
Laboratory address: 2086 Mirkovo, Mirkovo Municipality, Sofia-Region

To perform testing of:
	Type of the scope: flexible for a part of the scope

	№
	Tested Products
	Type of Test/Characteristic
	Testing methods
(standard / validated method)

	1
	2
	3
	4

	I.
	Copper concentrates, copper ores, copper steriles
	I.1. Gold - Au g/t
	ВЛМ № 1:2005
ВЛМ № 2:2005

	
	
	I.2. Copper - Сu %
	ВЛМ № 3:2005
ВЛМ № 19:2011

	
	
	I.3. Molybdenum - Мо %
	ВЛМ № 4:2005

	
	
	I.4. Iron - Fe %
	ВЛМ № 5:2005

	
	
	1.5. Silver -Ag g/t
	ВЛМ № 6:2005

	II.
	Water-Underground
	II.1. Active reaction (pH)
	БДС 17.1.4.27

	
	
	II.2. Conductiveness
	БДС EN 27888

	
	
	II.3. Nitrates/ Nitrate Nitrogen (N-N03-)
	ВЛМ № 10:2005

	
	
	II.4. Nitrites/Nitrite Nitrogen (N-NO2-)
	ВЛМ № 9:2005

	
	
	II.5. Ammonium ions/ Ammonium Nitrogen (N-NH4+)
	ВЛМ № 11:2005

	
	
	II.6. Chlorides/ Chloride ions
	ВЛМ № 8:2005

	
	
	II.7. Sulphates/ Sulphate ions
	ВЛМ № 7:2005

	
	
	II.8. Arsenic
	БДС 17.1.4.22

	
	
	II.9. Aluminium; potassium; cadmium; chromium; copper; iron; manganese; nickel; tin; selenium; zinc;
	БДС EN ISO 11885

	
	
	II.10. Cyanides (all)
	ВЛМ № 21:2011

	
	
	II.11. Fluorides
	ВЛМ № 22:2011

	
	
	II.12. Dissolved Oxygen
	БДС EN 25813

	III.
	Water - surface
	III.1. Active reaction (pH)
	БДС 17.1.4.27

	
	
	III.2. Dissolved substances
	БДС 17.1.4.04 cl.З

	
	
	III.3. Undissolved substances
	БДС 17.1.4.04 cl.2

	
	
	III.4. Electrical conductivity
	БДС EN 27888

	
	
	III.5. Nitrates/ Nitrate Nitrogen (N-NO3-)
	ВЛМ № 10:2005

	
	
	III.6. Nitrites/Nitrite Nitrogen (N-NO2-)
	ВЛМ № 9:2005

	
	
	III.7. Ammonium ions/ Ammonium Nitrogen (N-NH4+)
	ВЛМ № 11:2005

	
	
	III.8. Chlorides/ Chloride ions
	ВЛМ № 8:2005

	
	
	III.9. Sulphates/ Sulphate ions
	ВЛМ № 7:2005

	
	
	III.10. Arsenic
	БДС 17.1.4.22

	
	
	III.11. Aluminium; cadmium; copper; iron; manganese; nickel; tin; zinc
	БДС EN ISO 11885

	
	
	III.12. Biochemical oxygen demand after 5 days (BOD5)
	ВЛМ № 12:2005

	
	
	III.13. Chemical oxygen demand (COD)
	ВЛМ № 13:005

	
	
	III.14. Cyanides (free); Free cyanide
	ВЛМ № 21:2011

	
	
	III.15. Dissolved oxygen
	БДС EN 25813

	
	
	III. 16. General hardness.
Calcium carbonate hardness
	БДС ISO 6059

	
	
	III.17. Chrome (hexavalent)
	ВЛМ 14:2015

	
	
	III.18. Phosphates such as phosphorus
	ВЛМ № 20:2018

	IV.
	Water - waste.
	IV.1. Active reaction (pH)
	БДС 17.1.4.27

	
	
	IV.2. Undissolved substances
	БДС 17.1.4.04 cl.2

	
	
	IV.3. Arsenic
	БДС 17.1.4.22

	
	
	IV.4. Cadmium; copper; iron; manganese; nickel; tin; zinc
	БДС EN ISO 11885

	
	
	IV.5. Cyanides (free);
	ВЛМ № 21:2011

	
	
	IV.6. Cyanides (all)
	ВЛМ № 21:2011

	
	
	IV.7. Chemical oxygen demand (COD)
	ВЛМ № 13:2005

	
	
	IV.8. Chrome (hexavalent)
	ВЛМ 14:2015



  To perform sampling of:
	Type of the scope: flexible 

	№
	Products
	Sampling method (standardized/validated)

	1
	2
	3

	1.
	Ground water
	БДС ISO 5667-11

	2.
	Surface water
	БДС ISO 5667-6

	3.
	Waste water
	БДС ISO 5667-10


Flexible scope: Implementing a new version of standards/documents or standards/ documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by the laboratory.

   Fixed scope references:
1. ВЛМ № 1/2005 Determination of gold content in copper and molybdenum concentrates by extraction.
2. ВЛМ № 2/2005 Determination of gold content in copper ores and sterols by extraction. 
3. ВЛМ № 3/2005 Determination of copper content in copper ores and sterols by atomic absorption.
4. ВЛМ № 4/2005 Determination of molybdenum content in copper concentrates, ores and sterols.
5. ВЛМ № 5/2005 Determination of iron content in copper concentrates, ores and sterols.
6. ВЛМ № 6/2005 Determination of silver content in copper concentrates, ores, sterols and molybdenum concentrates.
7. ВЛМ № 7/2005 Water quality. Determination of sulphate ion content. Photometric method with "Spectroquant" test.
8. ВЛМ № 8/2005 Water quality. Determination of chloride ion content. Photometric method with "Spectroquant" test.
9. ВЛМ № 9/2005 Water quality. Determination of nitrite/nitrite nitrogen content. Photometric method with "Spectroquant" test.
10. ВЛМ № 10/2005 Water quality. Photometric method with "Spectroquant" test.
11. ВЛМ №. 11/2005 Water quality. Determination of ammonium ion/ammonium nitrogen content. Photometric method with "Spectroquant" test.
12. ВЛМ № 12/2005 Water quality. Determination of BOD/5/. Photometric method with "Spectroquant" test
13. ВЛМ № 13/2005 Water quality. Determination of COD. Photometric method with "Spectroquant" test.
14. ВЛМ № 14/2015 Water quality. Determination of hexavalent chromium content. Photometric method with "Spectroquant" test
15. ВЛМ № 19/2011 Determination of copper content in copper and molybdenum concentrates. Iodide method.
16. ВЛМ № 20/2011 Water quality. Determination of phosphate content. Photometric method with Spectroquant test.
17. ВЛМ № 21/2011 Water quality. Determination of cyanide (free) cyanide content (total).
18. ВЛМ № 22/2011 Water quality. Determination of fluoride content. Photometric method with "Spectroquant" test.
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