ORDER

№ A 129
Sofia, 01.04.2024
Inspection Body “Nadezhda” of TYPE С
 at " Nadya 2005” Ltd.,Sofia
Management address: 1612 Sofia, Lagera housing estate, bl. 80 B, ap. 36
             Office address: 1000 Sofia, Oborishte Neighbourhood, 16 Stara Planina str.

To perform inspection according to the following scope:

	Type of scope: flexible*

	№
	Field of inspection
	Type of inspection
	Parameter of Inspection/ Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	PHYSICAL FACTORS IN WORKING AND HOUSEHOLD ENVIRONMENT:

	1.1
	Artificial illumination in working and household environment.
	Of new and/or in use/ operation sites/ facilities
	Illumination
	Methodical instructions for measurement and evaluation of artificial lighting in buildings 40-85, Standardization Publishing House 1985.;
ПК 1
	Ordinance No. 49, 

(SG, No. 7/1976);

Ordinance No. 9, 

(SG, No. 46/1994);

Ordinance No. 24, 

(SG, No. 95/2003);

Ordinance No. 2, 

(SG, No.15/2007);

БДС EN 12464-1

TS

	1.2
	Working and household environment microclimate
	Of new and/or in use/ operation sites/ facilities
	- Air temperature;

- Relative air humidity;

- Air velocity
	БДС 16686;

Ordinance No. РД-07-3

(SG, No. 63/2014)

ПК 2
	Ordinance No. 9, 

(SG, No. 46/1994);

Ordinance No. 2, 

(SG, No. 15/2007);

Ordinance No. 24, 

(SG, No. 95/2003);

Ordinance 

No. РД-07-3 

(SG, No. 63/2014);

БДС 14776;

TS

	1.3
	NOISE

	1.3.1
	Noise in working environment
	Of new and/or in use/ operation sites/ facilities
	-Daily noise exposure level,

-Average weekly noise exposure level;

-Peak sound pressure level
	БДС EN ISO 9612 (БДС ISO 1999); 

ПК 3
	Ordinance No. 6, 

(SG, No. 70/2005.) TS

	1.3.2
	Noise in territories and development zones in urban areas and outside them
	Of new and/or in use/ operation sites/ facilities
	-Equivalent noise level
	БДС 15471; 

ПК 3
	Ordinance No. 6, SG, No. 58/2006– 

(Annex No. 2, tab. 2);

TS

	1.3.3
	Noise in residential and public buildings premises
	Of new and/or in use/ operation sites/ facilities
	-Noise level;

-Equivalent noise level
	БДС 15471;
ПК 3
	Ordinance No. 2 

(SG, No. 15/2007); Ordinance No. 6 

(SG, No. 58/2006 (Annex No. 2, tab. 1); 

Ordinance No. 9 

(SG, No. 46/1994);

Ordinance No. 24 

(SG, No. 95/2003); 

TS

	2.
	ELECTRIC ASSEMBLIES AND FACILITIES UP TO 1000 V:

	2.1
	Electric assemblies and facilities up to 1000 V
	Of new and/or in use/ operation sites/ facilities
	-Insulation resistance
	БДС 1986 item 3.3, (а), (б), (д) and (е); 

ПК 5
	Ordinance No. 3, 

SG, No. 90.91/2004; 

Ordinance No. 16-116 

SG, No. 26/2008; 

Ordinance No. 9, 

SG, No. 72/2004; 

TS

	2.2
	Electric assemblies and facilities up to 1000 V
	Of new and/or in use/ operation sites/ facilities
	-Impedance of the “phase – protective conductor circuit”
	ПК 6
	Ordinance No. 3, 

SG, No. 90.91/2004.;

Ordinance No. 16-116 

SG, No. 26/2008; 

TS

	2.3
	Electric assemblies and facilities up to 1000 V
	Of new and/or in use/ operation sites/ facilities
	Safety fuse breakers:

-Trigger current

-Protective earthing resistor;

-Contact voltage
	ПК 7
	Ordinance No. 3, 

SG, No. 90.91/2004.;

Ordinance No. 16- 116 

SG, No. 26/2008; 

TS


	2.4
	Electric assemblies and facilities up to 1000 V
	Of new and/or in use/ operation sites/ facilities
	-Safety grounding systems resistance
	ПК 8
	Ordinance No. 3, 

SG, No. 90.91/2004.;

Ordinance No. 16-116 

SG, No. 26/2008; 

TS

	2.5
	Electric assemblies and facilities up to 1000 V
	Of new and/or in use/ operation sites/ facilities
	-Resistance of lightning protection earthing systems
	ПК 9
	Ordinance No. 4, 

(SG, No. 6/2011); 

Ordinance No. 3, 

SG, No. 90,91/2004.;

Ordinance No. 16-116 

SG, No. 26/2008; 

TS

	3.
	VENTILATION INSTALLATIONS:

	3.1
	Ventilation installations
	Of new and/or in use/ operation sites/ facilities
	-Airflow velocity;

-Airflow rate
	БДС 12.3.018; 

ПК 10
	Ordinance No. 15, 

SG, No. 78/2005; 

TS


* The introduction of a new version of standards / documents or standards/documents that replace them is allowed. An up-to-date list of standards/documents with their dated versions is provided by the CAB
Ordinance No. 2 on the health requirements to the computer and internet halls for public use (SG No. 15/2007).
Ordinance No. 3 on the structure of electrical installations and power lines (SG, No. 90/2004, SG, No. 91/2004).
Ordinance No. 4 on lightning protection of buildings, exterior facilities and open spaces (SG, No. 6/2011).
Ordinance No. 6 on the minimum requirements for ensuring the health and safety of workers in case of risks related to noise exposure (SG No. 70/2005)
Ordinance No. 6 on the noise indicators in the environment taking into account the degree of discomfort during different parts of the day, limit values of noise indicators in the environment, in the premises of residential and public buildings, in areas and territories intended for residential construction, recreational areas and territories and mixed-use areas, methods for assessing the values of noise indicators and the harmful effects of noise on the health of the population (SG, No. 58 /2006)
Ordinance No. 9 on the health and hygiene requirements for the use of personal computers in the education and extracurricular activities of students (SG No. 46/1994)
Ordinance No. 9 on the technical operation of power plants and networks (SG, issue 72/2004)
Ordinance No. 15 on technical rules and regulations for the design, construction and operation of the sites and facilities for the production, transmission and distribution of thermal energy (SG, No. 68/2005)
Ordinance No. 24 on the sanitary and hygienic requirements to the discotheques (SG No. 95/2003) 
Ordinance No. 49 on artificial lighting of buildings (SG No. 7/1976)
Ordinance РД-07-3 on the minimum requirements for the microclimate of workplaces (SG, No. 63/2014) 

Ordinance No. 16-116 on the technical operation of the energy equipment (SG, No. 26/2008)

TS – Technical specification.
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