SCOPE 107 ЛИ

Sofia, 10.07.2024

TOPLOFIKATSIA RUSE JSC 
FUELS AND OILS TESTING LABORATORY
Management and laboratory address: 
7009 Ruse, 1 TEC-Iztok Str. 

To perform testing of:
	Type of the scope: flexible for a part of the scope

	№ 
	Tested products
	Type of test / characteristic
	Testing methods
(standard / validated method)

	1
	2
	3
	4

	1. 
	Solid mineral fuels 
- Black and anthracite coal (1) 
- Brown and lignite coal (2) 
- Coke (3) 
	1.1. Moisture content:
· total
- in the analysis sample
	БДС ISO 589 (1), 
БДС ISO 5068-1 (2), 
БДС ISO 579 (3), 
БДС ISO 11722 (1), 
БДС ISO 5068-2 (2), 
БДС ISO 687 (3)

	
	
	1.2. Ash content:
- in dry state 
- as received
	БДС ISO 1171,
БДС ISO 1170 (1), (2), (3)

	
	
	1.3. Extraction of volatile substances:
· in dry state
· as received
- in dry ash-free slate
	БДС ISO 562
БДС ISO 1170 (1), (3);
БДС ISO 5071-1,
БДС ISO 1170 (2)

	
	
	1.4. Sulfur content: 
- in dry state 
- as received
	БДС ISO 19579,
БДС ISO 1170 (1), (2), (3)

	
	
	1.5. Carbon content:
· in dry state
- as received
	БДС ISO 29541, 
БДС ISO 1170 (1), (2), (3)

	
	
	1.6. Calorific value
- gross (in dry state and as received)
- net (in dry state and as received)
	БДС ISO 1928 (1), (2), (3)

	2.
	Solid biofuels: 
biomass (1) 
pellets (2) 
briquettes (3) 
wood shavings (4)
	2.1. Moisture content:
- total
- in the analysis sample
	БДС EN ISO 18134-2 (1), (2), (3), (4)
БДС EN ISO 18134-3 (1), (2), (3), (4) 		

	
	
	2.2. Ash content: 
- in dry state 
- as received
	БДС EN ISO 18122, 
БДС EN ISO 16993 (1), (2), (3), (4)

	
	
	2.3. Extraction of volatile substances:
· in dry state
· as received
- in dry ash-free state
	БДС EN ISO 18123, 
БДС EN ISO 16993 (1), (2), (3), (4)

	
	
	2.4. Sulfur content: - in dry state - as received
	ВЛМ 7.2-2,
БДС EN ISO 16993 (1), (2),
(3), (4)

	
	
	2.5. Carbon content: 
- in dry state 
- as received
	ВЛМ 7.2-3,
БДС EN ISO 16993 (1), (2), (3), (4) 		

	
	
	1.6. Calorific value
- gross (in dry state and as received)
- net (in dry state and as received)
	БДС EN ISO 18125 (1), (2), (3), (4)


Flexible scope: Implementing a new version of standards/documents or standards / documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.

Fixed scope references:
1. ВЛМ 7.2-2/05.07.2023 An intralaboratory method for determining the sulfur content in solid biofuels through a device for infrared spectrometry ELTRA CS 530;
2. ВЛМ 7.2-3/05.07.2023 An intralaboratory method for determining the carbon content in solid biofuels.
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