



ORDER 
No. A 206
Sofia, 29.05.2024

INSPECTION BODY OF TYPE C

at “FACTOR 2010” LTD., City of Varna


Management address: 9023, city of Varna, quarter “Vladislav Varnenchik", bl. 302, entr. 6, floor 2, apt. 78
Office address: 9000, city of Varna, 281, “Vladislav Varnenchik", Blvd

To perform inspection of:
	Scope type: flexible*

	№

	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1
	Electrical installations and facilities

	1.1










	Electrical installations and facilities up to 1000V
	On new and/or in use/operation sites / facilities








	Impedance of the "phase-protective conductor" circuit
	ПК  01
	Ordinance No 16-116, SG issue No 26/2008;
Ordinance No 3, SG issue No 90, 91/2004;
TS 

	
	
	
	Circuit breakers 
- actuating current;
- contact voltage.
	ПК 02
	 Ordinance No 16-116, SG issue No 26/2008;
Ordinance No 3, SG issue No 90, 91/2004;
TS 

	
	
	
	Insulation resistance
	ПК 03
	Ordinance No 16-116, SG issue No 26/2008;
Ordinance No 3, SG issue No 90, 91/2004;
TS



	1.2
	Electrical installations and facilities up to and above 1000V



	On new and/or in use/operation sites / facilities
	Resistance of protective earthing systems
	ПК 04
	Ordinance No 16-116, SG issue No 26/2008;
Ordinance No 3, SG issue No 90, 91/2004;
TS 

	
	
	
	Resistance of lightning protection earthing systems


	ПК 05
	Ordinance No 4, SG issue No 6/2011. 
TS 

	2
	Physical factors

	2.1
	Microclimate in working environment, residential and public buildings
	On new and/or in use/operation sites / facilities
	-air temperature;
-relative air humidity;
-speed of air movement
	БДС 16686;
Ordinance No РД- 07-3, SG issue No 63 /2014
ПК 06
	БДС 14776;
Ordinance No 9,
SG issue No 46/1994; Ordinance No 24,
SG issue No 95/2003; Ordinance No 3, 
SG issue No 15 /2007; Ordinance No 2,
SG issue No 15 /2007; Ordinance No 26,
SG issue No 03/ 2008;
Ordinance No РД-07-3, SG issue No 63/2014; 
TS 

	2.2
	Noise in work environment
	On new and/or in use/operation sites / facilities
	- daily noise exposure level;
- average weekly noise exposure level;
- peak sound pressure level,
	БДС EN ISO 9612 (БДС ISO 1999);
ПК 07
	Ordinance No 6,
SG issue No 70/2005;
TS 

	2.3
	Environmental noise
	On new and/or in use/operation sites / facilities
	- equivalent noise level
	БДС 15471;
ПК 08
	Ordinance No 6,
SG issue No58/2006, Appendix No2, Table 2;
TS 

	2.4
	Noise in the premises of residential and public buildings
	On new and/or in use/operation sites / facilities
	- noise level;
- equivalent noise level,
	БДС 15471; 
ПК 09
	Ordinance No 6,
SG issue No 58/2006,- Appendix No2,Table 1;
Ordinance No 9,
SG issue No 46/1994; Ordinance No 24,
SG issue No 95/2003;
Ordinance No 2,
SG issue No 15/2007; Ordinance No 26,
SG issue No 103/2008
TS

	2.5
	Artificial lighting in work environment, residential and public buildings
	On new and/or in use/operation sites / facilities
	- illumination
	Methodical guideline 40-85 - Methods for measuring and evaluating artificial lighting, issue 
Standardization 1985;
ПК 10
	БДС EN 12464-1;
Ordinance No 49,
SG issue No 7/1976;
Ordinance No 9,
SG issue No 46/1994;
Ordinance No 24,
SG issue No 95/2003;
Ordinance No 3,
SG issue No 15/2007, Ordinance No 2,
SG issue No15/2007;
Ordinance No 26,
SG issue No103/ 2008;
TS 

	3.
	Ventilation systems
	On new and/or in use/operation sites / facilities
	- air flow velocity;
- air flow rate
	БДС 12.3.018;
ПК 11
	Ordinance No 15,
SG issue No 68/2005 Ordinance No 24,
SG issue No 95/2003; TS



[bookmark: _GoBack]*The introduction of a new version of standards/documents or standards/documents that replace them is allowed. An up-to-date list of standards/documents with their dated versions is provided by Conformity assessment bodies (CAB).
Ordinance No 3 (prom. SG issue No 90 and issue No 91/2004) on the structure of electrical installations and power lines;
Ordinance No 16-116 (prom. SG, issue No 26/2008) on technical operation of energy equipment;
Ordinance No 4 (SG issue No 6 of 18.01.2011) on the lightning protection of buildings, external facilities and open spaces;
Ordinance №24 (prom. SG, issue No 95/2003, amended SG issue No 100/2003) on sanitary-and- hygienic requirements for discos;
Ordinance №9 (SG, issue No 46/1994) on the health and hygiene requirements for the use of personal computers in the education and extracurricular activities of pupils;
Ordinance No 2 (prom. SG issue No 15/2007) on the health requirements to the computer and internet halls for public use;
Ordinance No 3 (prom. SG, issue No 15/2007) on the health requirements for kindergartens;
Ordinance No 26 (SG, issue No 103/2008) on the structure and activity of nurseries and children's kitchens and the health requirements to them;
Ordinance № РД-07-3 (SG issue No 63/2014);14г.) on the minimum requirements for the microclimate of workplaces;
Ordinance №6 (SG, issue No 70/2005) on the minimum requirements for ensuring the health and safety of workers at risks related to noise exposure; 
Ordinance №6 (prom. SG, issue No 58/2006) on environmental noise indicators, taking into account the degree of discomfort during different parts of the day, the limit values of environmental noise indicators, in the premises of residential and public buildings, in zones and territories intended for residential construction, recreational zones and territories and zones with mixed purpose, the methods for assessing the values of noise indicators and the harmful effects of noise on public health;
Ordinance №49 (SG, issue No 7/1976, amended and supplemented, issue No 64/1976) on artificial lighting of buildings;
Methodical guidelines for measurement and evaluation of artificial lighting in buildings 40-85, issue Standardization, 1985;
Ordinance №15 (SG issue No 68/2005) on technical rules and norms for design, construction and operation of sites and facilities for production, transmission and distribution of heat energy.
TS- TECHNICAL SPECIFICATION.
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