SCOPE 312 ЛИ
Sofia, 30.08.2024
TECHNICAL UNIVERSITY OF SOFIA
VIBRO-ACOUSTIC LABORATORY
Management laboratory address: 1000 Sofia, Darvenitsa, 8 Sv. Kliment Ohridski Blvd.

To perform testing of:
	Type of the scope: fixed

	№
	Tested products
	Type of test/ characteristic
	Testing methods
(standard/ validated method)

	1
	2
	3
	4

	1.
	Sound insulation 
of partition walls 
from airborne noise
	1.1. Index of actual insulation of partition walls/floors from airborne noise
1.2. Weighted index of the actual insulation of the partition walls from airborne noise
	[bookmark: _Hlk159743240]БДС EN ISO 16283-1:2014
БДС EN ISO 16283-1:2014/ 
А1: 2018
БДС EN ISO 10140-2:2021
БДС EN ISO 10052:2021 
[bookmark: _Hlk125282310]БДС EN ISO 717-1:2021

	2.
	Sound insulation 
of floors from impact noise
	2.1. Index of actual sound insulation from impact noise
2.2. Weighted index of the actual sound insulation from impact noise
	[bookmark: _Hlk159743266]БДС EN ISO 16283-2:2020
[bookmark: _Hlk159743279]БДС EN ISO 10140-3:2021
БДС EN ISO 16205:2020
БДС EN ISO 10052:2021
БДС EN ISO 717-2:2021

	3.
	Sound insulation 
of building facades
	3.1. Index of actual insulation of facades from airborne noise
3.2. Weighted index of the actual insulation of facades from airborne noise
	[bookmark: _Hlk158971439][bookmark: _Hlk159743295]БДС EN ISO 16283-3:2016
БДС EN ISO 10052:2021 
БДС EN ISO 717-1:2021


	4.
	Acoustic output 
of machinery and equipment
	4.1. Acoustic output level 
	[bookmark: _Hlk159743310]БДС EN ISO 3741:2010
БДС EN ISO 3744:2010 /class 2/
БДС EN ISO 3745:2012 /class 1/
БДС EN ISO 3745:2012/A1:2017
БДС EN ISO 3746:2010 /class 3/
БДС EN ISO 9295:2015

	5.
	Sound absorption of materials
	5.1. Sound absorption index
	[bookmark: _Hlk159743343]БДС EN ISO 354:2003
БДС EN ISO 11654:2004

	6.
	Environmental noise, in the premises of residential and public buildings
	6.1. Equivalent noise level
6.2. Maximum A - weighted noise level
	[bookmark: _Hlk159743356]БДС ISO 1996-2:2017
БДС 15471:1982


	7.
	Vibrations in buildings, premises and work environment
	7.1. RMS values of vibration displacement
7.2. RMS values of vibration speed
7.3. RMS values of vibration acceleration
	[bookmark: _Hlk159743377]ISO 4866:2010 
DIN 45669-1:2020 
DIN 45669-2:2005 

	8.
	Vibrations transmitted from human hands to upper arm
	8.1. Daily value of vibration exposure
	[bookmark: _Hlk159743398]БДС ISO 5349-1:2002
БДС EN ISO 5349-2:2002
БДС EN ISO 5349-2:2001/
A1:2015

	9.
	Vibration of machinery and equipment
	9.1. RMS values of vibration displacement
9.2. RMS values of vibration speed
9.3. RMS values of vibration acceleration

	[bookmark: _Hlk159743412]БДС ISO-20816-1:2018
БДС ISO-20816-2:2019
БДС ISO-20816-3:2022
БДС ISO-20816-4:2019
БДС ISO-20816-5:2019
БДС ISO-20816-8:2019
БДС ISO-20816-9:2021;
БДС ISO-10816-6:2002
БДС ISO 10816-6:1995/
 Amd 1:2019
БДС ISO-10816-7:2014;

	10.
	Vibration and impact testing of machines and facilities with an electrodynamic vibrator
	10.1. RMS values of vibration displacement
10.2. RMS values of vibration speed
10.3. RMS values of vibration acceleration
	[bookmark: _Hlk159743429]БДС EN 60068-2-6:2008 
БДС EN 60068-2-27:2009 
БДС EN 60068-2-64:2008 
БДС EN 60068-2-64:2008/ 
A1:2020

	11.
	Measurement of outside noise emitted by railway vehicles
	11.1. Equivalent noise level
11.2. Maximum noise level /for stationary/rolling stock/
11.3. Transit level of sound exposition
11.5. Equivalent noise level /for stationary/rolling stock/
	[bookmark: _Hlk159743445]БДС EN ISO 3095:2013
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