
ORDER

№ А 355
Sofia, 30.09.2024
Inspection Body of type C
 at NEK JSC, Enterprise Hydroelectric Power Plants, town of Plovdiv

Management and office address: 4003 Plovdiv, 244 Vasil Levski Blvd.

To perform inspection of:
	Type of scope: flexible*

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Electrical systems and equipment of up to and more than 1000 V
	New and operated equipment
	Resistance of protective grounding systems
	РП-1


	Regulation № 3/2004, 

State Gazette, issue 90/2004,

Regulation № 16-116/2008,

State Gazette, issue 26/ 07.03.2008, TS  

	
	
	
	Resistance of lightning protection grounding systems
	РП-1


	Regulation № 3/2004, 

State Gazette, issue 90 and 91/2004,

Regulation № 16-116/2008,

State Gazette, issue 26/ 07.03.2008, 

Regulation № 4/2010, 

State Gazette, issue 6/ 18.01.2011, TS

	2. 
	Electrical systems and equipment of up to 1000 V 
	New and operated equipment
	Impedance of the edge “phase – protective conductor” 

	РП-2 


	Regulation № 3/2004, 

State Gazette, issue 90 and 91/2004,

Regulation № 16-116/2008,

State Gazette, issue 26/ 07.03.2008, 

TS

	3. 
	Electrical protective equipment 
	Operated products


	
	Regulation № 22/2006, 

State Gazette, issue 45/02.06.2006

РП-3
	Regulation № 22/2006, State Gazette, issue 45/ 02.06.2006

TS 

	3.1.
	Insulating rods of all types; Insulating pliers; Current-measuring pliers; Insulating rods for portable grounding devices; Dielectric carpets and strips of carpet 
	
	Electrical strength of insulation through inspection with increased voltage, with industrial frequency    
	
	

	3.2.
	Voltage indicators 
	
	Electrical strength of insulation through inspection with increased voltage, with industrial frequency; Threshold of voltage indication (voltage threshold) 
	
	

	3.3.
	Dielectric gloves; boots; overshoes
	
	Electrical strength of insulation through inspection with increased voltage, with industrial frequency, current of leakage
	
	


* The introduction of a new version of standards/documents or standards/documents that replace them is allowed. An up-to-date list of standards/documents with their dated versions is provided by the Conformity assessment bodies (CAB).

Regulation № 4 on Lightning Protection of Buildings, External Equipment and Open Spaces (State Gazette, issue 6/2001);

Regulation № 3 on Construction of Electrical Systems and Еlectroconductive Lines (State Gazette, issue 90 and 91/2004);

Regulation № 16-116 on Technical Operation of Electrical Equipment (State Gazette, issue 26/2008);

Regulation № 22 on Testing Operated Electrical Protective Equipment (State Gazette, issue 45/02.06.2006);

TS – Technical specification.
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