		


ORDER

№ A 249

Sofia, 01.07.2024


„EMU“ AD, TARGOVISHTE
EMU CONTROL, INSPECTION BODY OF TYPE C

Management address: 7700, Targovishte, Razboyna District, p.o. box 174
Office address: 7700, Targovishte, 12 Pirin Str.

To perform inspection of:
	Type of scope: Flexible*

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Electrical installations 
up to and including 
750 kV
	New and/or currently operated  installations and facilities
	Resistance of protective earthing systems
	
Technical policy – Electric substations and power lines – 
Electric Rower System
Operator  
ПК 1
	Ordinance № 16-116 
(SG № 26/2008)
Ordinance № 3 
(SG № 90 and 91/2004); TS

	
	
	
	Resistance of lightning protection earthing systems
	ПК 2

	Ordinance № 16-116 
(SG № 26/2008)
Ordinance № 4 
(SG № 6/2011); TS

	
	
	
	Earthed equipent’s connection to the earthing facility
	
Technical policy – Electric substations and power lines – 
Electric Rower System
Operator  
ПК3
	Technical policy – Electric substations and power lines – 
Electric Rower System
Operator/ 12.04.2022;TS

	
	
	
	Tangential and foot voltage
	
Technical policy – Electric substations and power lines – 
Electric Rower System
Operator  
ПК 4

	
БДС EN 50522
Technical policy – Electric substations and power lines – 
Electric Rower System
Operator/ 12.04.2022;TS

	2.
	Electrical installations 
up to and including 
1000 V
	New and/or currently operated  installations and facilities
	Impedance of the "phase-protective conductor" circuit
	           ПК 5

	Ordinance № 16-116 
(SG № 26/2008)
Ordinance № 3 
(SG № 90 and 91/2004); TS

	
	
	
	Zero sequence circuit breakers:
- tangential voltage;
- trigger current;
- shutdown time;
- resistance of protective earthing
	ПК 6

	Ordinance № 16-116 
(SG № 26/2008)
Ordinance № 3 
(SG № 90 and 91/2004); TS

	3.
	Cables and cable lines up to 35 kV
	New and/or currently operated  installations and facilities
	Insulation resistance
	БДС 1986,
items 3.3.a,b,е, f;
НИЕМС;
ПК 7

	Ordinance № 16-116 
(SG № 26/2008)
Ordinance № 3 
(SG № 90 and 91/2004); НИЕМС-1995; TS

	4.
	Cables and cable lines up to 20 kV
	New and/or currently operated  installations and facilities
	Electrical strength with increased DC voltage
	БДС 2406,
ПК 8

	Ordinance № 16-116 
(SG № 26/2008);
НИЕМC-1995; TS

	5.
	Overhead power lines, open and closed distribution systems up to and including 750 Kv

	New and/or currently operated  installations and facilities
	Transient resistance in tension terminals, screw and bolt joints
	НИЕМС;
ПК 9

	Ordinance № 16-116 
(SG № 26/2008);
НИЕМС -1995; TS

	6.
	Electrical insulating oil

	New and/or currently operated  installations and facilities
	Breakthrough
voltage

	БДС EN 60156;
ПК 10

	Ordinance № 16-116 
(SG № 26/2008);
НИЕМС -1995; TS

	7.
	Optical cables, optical cable lines
	New and/or currently operated  installations and facilities
	Imported attenuation from inhomogeneity; total attenuation; loss of reverse reflection
	БДС EN 60793-1-22; 
БДС EN 60793-140; 
БДС EN 61280-4-2;
              ПК 11
	Bulgarian Telecommunication Company’s instruction for the construction of optical cable lines – 2004; ТS

	8.
	Artificial lighting in work and living environment
	New and/or currently operated  installations and facilities
	Illumination
	Methodical guidelines on the measurement and evaluation of artificial lighting-85, publishing house "Standardization" -1985;
            ПК 12
	Ordinance № 49
(SG № 7/1976);
БДС EN 12464-1; 
ТS



*The introduction of a new version of standards/documents or standards/documents that replace them is allowed. An up-to-date list of standards/documents with their dated versions is provided by the CAB.


[bookmark: _GoBack]References:

Ordinance № 16-116 on energy equipment’s technical operation (as published in SG № 26/2008;
Ordinance № 3 on the structure of electrical installations and power lines (published in SG № 90/2004, and SG № 91/2004;
Ordinance № 4 on the lightning protection of buildings, external facilities and open spaces (SG № 45/2006);
Ordinance № 49 on buildings’ artificial lighting (SG № 7/1976, amended in SG № 64/1976);
NIEMS-1995 - Standards for electrical machinery and equipment testing – 1995 issued by the Energy Commission;
Methodological guidelines for measurement and assessment of artificial lighting in buildings 40-85, Compendium of methods NCHMEH, volume IV, ed. Standardization, 1985;
Technical policy - electrical substations and power lines - ESO/12.04.2022;
Instruction for construction of optical cable lines - БTК ЕАД „БTK - НИИС" - 2004.
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