



ORDER

№ A 336

Sofia, 30.08.2024


 Inspection Body of type A
at Regional Health Inspectorate, Sofia Region,
Sofia


Management and office address: 
1612 Sofia, 15 Acad. Ivan Geshov Blvd., level 3



To perform inspection of:
	Type of the scope: flexible for part of the scope*

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection, 
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	I. Physical factors of the work and natural environment

	1.1.1
	Noise in work environment
	New sites and/or sites in operation
	Daily level of noise exposure, 
Average weekly noise exposure level, Peak sound pressure, 
	ПР-СУК-01-1
БДС ISO 1999 
БДС EN ISO 9612
	Ordinance № 6
/SG № 70/2005; TС

	1.1.2
	Noise in the environmental in different territories and development zones in the urbanized territories and outside them
	New sites and/or sites in operation
	Noise level, Equivalent noise level, 
	ПР-СУК-01-2
 БДС 15471
	Ordinance № 6
/SG № 58/2006 Annex № 2, 
Table 2; TС

	1.1.3
	Noise in premises in residential and public buildings
	New sites and/or sites in operation
	Noise level, Equivalent noise level, 
	ПР-СУК-01-3
БДС 15471
	Ordinance № 7
/SG № 88/1999;
Ordinance № 2
/SG № 15/2007; Ordinance № 24
/ SG № 95/2003;
Ordinance № 9
/SG № 46/1994; Ordinance № 6
/SG № 58/2006 Annex № 2, 
Table 1 
Ordinance № 26
/ SG № 103/2008; TC

	1.2
	Microclimate in a work and domestic environment
	New sites and/or sites in operation
	Air temperature Relative air humidity Air ovement speed
	ПР-СУК-02
БДС 16686 
Ordinance № RD- 07-3
 (SG № 63 / 2014)
	Ordinance № 2
/SG № 15/2007;
Ordinance № 3
/SG № 15/2007;
Ordinance № 9
/SG № 46/1994; Ordinance № 24
/ SG № 95/2003; БДС 14776 Ordinance № RD- 07-3 
/SG № 63 / 2014; Ordinance № 26
/SG № 103/2008; TC

	1.3
	Artificial lighting in a work and domestic environment
	New sites and/or sites in operation
	Illumination
	ПР-СУК-3
Methods for measurement of artificial lighting in buildings, volume
IV. National Center of Hygiene, Medical Ecology and Nutrition
	Ordinance № 2
/SG № 15/2007;
Ordinance № 3
/SG № 15/2007;
Ordinance № 9
/SG № 46/1994; Ordinance № 24
/ SG № 95/2003; Ordinance №49
/ SG № 7/1976; 
БДС EN 12464-1 Ordinance №26
/SG № 103/2008; TC

	II.
	Cosmetics

	New products and/or products in use
	
	ПР-СУК-04

	Ordinance № 14 
SG № 68/2014 Regulation (EC) 
№ 1223/2009;


	
	
	
	Appearance, color, and smell
	БДС 3741
БДС 10751
	

	
	
	
	Emulsion type
	БДС 3741
БДС 10751
	

	
	
	
	Emulsion stability
	БДС 3741
БДС 10751
	

	
	
	
	Thermal stability
	БДС 3741
БДС 10751
	

	
	
	
	pH
	БДС ISO 4316
	

	
	
	
	Total content of surfaceactive substance %
	Rulebook of the Ministry of ealth/97
	

	
	
	
	Determining anionic surface-active substance %

	Rulebook of the Ministry of Health/97
	

	
	
	
	Hydrogen Peroxide
	Ordinance N 14/ SG № 68/2014, Annex 2, VIII.B;
	

	
	
	
	Thioglycolic Acid
	Ordinance N 14/ SG № 68/2014, Annex 2, XVIII.it.5.1
	

	
	
	
	
	MR-QMS-04
	

	
	
	
	Total number of aerobic mesophilic bacteria
	БДС EN ISO 21149
	БДС EN ISO 17516

	
	
	
	Yeasts and molds
	БДС EN ISO 16212
	БДС EN ISO 17516

	
	
	
	Escherichia coli
	БДС EN ISO 21150
	БДС EN ISO 17516

	
	
	
	Candida albicans
	БДС EN ISO 18416
	БДС EN ISO 17516

	
	
	
	Pseudomonas aeruginosa

	БДС EN ISO 22717
	БДС EN ISO 17516

	
	
	
	Staphylococcus aureus
	БДС EN ISO 22718
	БДС EN ISO 17516

	III. Water

	III.1
	Water designated for potable water purposes / including spring and table water, prior to and after bottling/ for the purposes of official control
	New products and/or products in use
	
	ПР-СУК-05
	Ordinance № 9 
SG № 30/2001;



	
	
	
	Turbidity NTU
	БДС EN ISO 7027-1
	

	
	
	
	Active Reaction pH
	БДС 3424
	

	
	
	
	Permanganate oxidizability
	БДС 3413
	

	
	
	
	Ammonia ion
	ВЛМ 04/10.04.2024
	

	
	
	
	Nitrites
	ВЛМ 08/10.04.2024
	

	
	
	
	Nitrates
	ВЛМ 09/10.04.2024
	

	
	
	
	Chlorides
	БДС 3414
	

	
	
	
	Total hardness
	БДС ISO 6059
	

	
	
	
	Phosphates
	ВЛМ 10/10.04.2024
	

	
	
	
	Sulphates
	ВЛМ 11/10.04.2024
	

	
	
	
	Magnesium
	ВЛМ 01/10.04.2024
	

	
	
	
	Calcium
	БДС ISO 6058
	

	
	
	
	Iron
	ВЛМ 05/10.04.2024
	

	
	
	
	Manganese
	ВЛМ 6/10.04.2024
	

	
	
	
	Chrome
	ВЛМ 12/10.04.2024
	

	
	
	
	Specific electrical conductivity ат 20 ºС
	БДС EN 27888
	

	
	
	
	Residual free chlorine
	ВЛМ 03/10.04.2024
	

	
	
	
	Fluorides
	ВЛМ 13/10.04.2024
	

	
	
	
	Cadmium
	ВЛМ 14/10.04.2024
	

	
	
	
	
	
	Ordinance № 9 
SG № 30/2001;

	
	
	
	
	ПР-СУК-06
	

	
	
	
	Microbial count KOE
	БДС EN ISO 6222
	

	
	
	
	Coliforms KOE
Escherchia coli KOE
	
БДС EN ISO 9308-1/A1
	

	
	
	
	Enterococci KOE
	БДС EN ISO 7899-2

	

	
	
	
	Spores from sulfitereducing anaerobes KOE

	БДС EN 26461-2

	

	
	
	
	Pseudomonas aeruginosa KOE
	БДС EN ISO 16266
	

	III.2
	Water from swimming pools
	New products and/or products in use
	
	ПР-СУК-05
	Instructions 34 
SG № 82/1975;

	
	
	
	Active Reaction pH
	ВЛМ 02/10.04.2024
	

	
	
	
	Ammonia ion
	ВЛМ 04/10.04.2024
	

	
	
	
	Nitrites
	ВЛМ 08/10.04.2024
	

	
	
	
	Residual free chlorine
	ВЛМ 03/10.04.2024
	

	
	
	
	Iron
	ВЛМ 05/10.04.2024
	

	
	
	
	Manganese
	ВЛМ 06/10.04.2024
	

	
	
	
	Permanganate oxidizability
	ВЛМ 07/10.04.2024
	

	
	
	
	Turbidity
	БДС EN ISO 7027- 1
	

	
	
	
	
	ПР-СУК-06
	

	
	
	
	Microbial count
	БДС 17335, item 6
	

	
	
	
	Total coli titer
	БДС 17335, item 7
	

	
	
	
	Escherichia coli titer
	БДС 17335, item 7
	

	
	
	
	Enterococcal titer
	БДС 17335, item 8
	

	
	
	
	Staphylococcal titer
	БДС 17335, item 9
	

	III.3
	Running surface waters, designated for potable water supply for domestic purposes
	New products and/or products in use
	
	MR-QMS-06
	Ordinance № 12 
SG № 63/2002;

	
	
	
	Coliforms KOE/100
	БДС EN ISO 9308-1/A1
	

	
	
	
	Escherichia coli
	БДС EN ISO 9308- 1
	

	
	
	
	Coliforms MPN 
	БДС 17336
	

	
	
	
	Escherichia coli
	БДС 17336
	

	
	
	
	Fecal streptococci
	БДС EN ISO 7899- 2
	

	
	
	
	Salmonella
	БДС EN ISO 19250
	

	III.4
	Mineral waters prior to and after bottling (1) and swimming pools (2)
	New products and/or products in use
	
	MR-QMS-06
	Ordinance № 14 
SG № 12/1995; 

Ordinance adopted with an Ordinance of the Council of Ministers № 178 (SG № 68/2004); 




	
	
	
	Microbial count KOE
	БДС EN ISO 6222 (1)
	

	
	
	
	Coliforms MRN
	БДС 17335, item 7 (2)
	

	
	
	
	Escherichia coli
	БДС 17335 item 7 (2)
	

	
	
	
	Coliforms KOE/250
	БДС EN ISO 9308- 1/A1 (1)
	

	
	
	
	Escherichia coli KOE/250
	БДС EN ISO 9308-1/A1 (1)
	

	
	
	
	Enterococci KOE/250
	БДС EN ISO 7899-2(1)
	

	
	
	
	Enterococci MPN
	БДС 17335 item 8 (2)
	

	
	
	
	Pseudomonas aeruginosa KOE/250
	БДС EN ISO 16266 (1)
	

	
	
	
	Spores from sulfite reducing anaerobes KOE/250 (clostridia)
	БДС EN 26461-2 (1)
	

	III.5
	Bathing water
	New products and/or products in use
	
	MR-QMS-06
	

	
	
	
	Coliforms
	БДС 17335 item 7 
	

	
	
	
	Fecal coliforms
	БДС 17335 item 7 
	

	
	
	
	Coliforms
	БДС EN ISO 9308- 1
	

	
	
	
	Fecal coliforms KOE/100
	БДС EN ISO 9308-1
	

	
	
	
	Fecal streptococci KOE/100
	БДС EN ISO 7899- 2
	

	
	
	
	Salmonella species
	БДС EN ISO 19250
	





*Flexible scope: Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.
Ordinance № 2 / 05.02.2007 regarding the health requirements to the Computer and Internet clubs for public use (SG, № 15 / 2007);
Ordinance № 3 / 05.02.2007 regarding the health requirements to kindergartens (SG, № 15 / 2007. amended SG, № 90 / 2020);
Ordinance № 9 regarding the health and hygiene requirements in using personal computers in training and extracurricular activities of students (SG, № 46 / 1994);
Ordinance № 24 / 20.10.2003 regarding the sanitary and hygiene requirements to disco clubs (SG, № 95 / 2003, amended in SG, № 100 / 2003);
Ordinance № RD-07-3 / 18.07.2014 regarding the minimum requirements for the micro-climate of workplaces (SG, № 63 / 01.08.2014)
Ordinance № 26 / 18.11.2008 regarding the structure and activity of nurseries and child kitchens and health requirements to them (SG, № 103 / 02.12.2008, amended SG, № 90 / 2020)
Ordinance № 49 regarding the artificial lighting of buildings (SG, № 7 / 1976, amended SG, № 64 / 1976);
Ordinance № 7 / 23.09.1999 regarding the minimum requirements for occupational health and safety and the use of work equipment (SG, № 88 / 1999, amended SG, № 95 / 29.11.2016);
Ordinance № 6 / 15.08.2005 regarding the minimum requirements for ensuring the health and safety of workers in case of risks related to noise exposure (SG, № 70 / 2005);
Ordinance № 6 / 26.06.2006 regarding the environmental noise indicators, reporting the degree of discomfort during different times during the day, the limit value of the environmental noise indicators, in the premises of residential and public buildings, in areas and territories designation for residential construction, recreation areas, mixed designation territories and areas, methods for evaluation of the values of the noise indicators and the harmful effects of noise over the population health (SG, № 58 / 2006, amended SG, № 100 / March 29, 2021);
Ordinance № 9 / 16.03.2001 regarding the quality of water, designated for potable and household purposes (SG, № 30 / 2001. amended SG, № 6 / January 16, 2018);
Instruction № 34 regarding hygiene of sports establishments and equipment (SG, № 82 / 1975, amended SG, № 25 / 08.03.2002)
Ordinance № 12 / 18.06.2002 regarding the quality requirements to surface waters, designated for potable and household water supply (SG, № 63 / 2002, amended SG, № 15 / 21.02.2012);
Ordinance № 14 regarding the resort resources, resort areas and resorts (SG, № 12 / 1995, amended SG, № 70 / 2004);
Ordinance for the requirements to bottled mineral, spring, and table water, designated for potable purposes, adopted with Ordinance of the Council of Ministers № 178 / 23.07.2004 (SG, № 68 / 2004. amended SG, № 66 / 2008);
Ordinance of the Council of Ministers № 173 for amendment and supplement of the Ordinance for the requirements to bottled mineral, spring, and table water, designated for potable purposes, adopted with an Ordinance of the Council of Ministers № 178 / 2004 (SG, № 66 / 2008);
Ordinance № 5 / 30.05.2008 regarding bathing water quality management (SG, № 35 / 10.06.2008, amended in SG, № 5 / 18.01.2013);
Ordinance № 14 / 28.07.2014 for determining detailed rules for providing information under article 19, paragraph 4 of Regulation (EC) № 1223/2009 regarding cosmetic products, efficacy requirements of sunscreen cosmetic products and chemical methods for inspection of the composition of cosmetic products (SG, № 68 / 15.08 2014)
Regulation (EC) № 1223/2009 of the European Parliament and of the Council / 30.11.2009, regarding cosmetic products
MoH/97 - Indicators and methods for studying cosmetic, washing agents and detergents, textile, and hygiene materials.
Ordinance of the Council of Ministers № 173 for amendment and supplement of the Ordinance for the requirements to bottled mineral, spring, and table water, designated for potable purposes, adopted with an Ordinance of the Council of Ministers № 178 / 2004 (SG, № 66 / 2008);
TS - technical specification of the client
TD - Technical documents of the client
Fixed scope:
ВЛМ 01/10.04.2024- Internal laboratory metod for determining the magnesium content in water intended for drinking domestic purposes/incl. spring and table water before and after/bottling
ВЛМ 02/10.04.2024- Internal laboratory metod for determining active reaction/pH in water from swimming pools
ВЛМ 03/10.04.2024- Photometric determination of residual free chlorine in water
ВЛМ 04/10.04.2024- Photometric determination of the content of ammonium ions in water
ВЛМ 05/10.04.2024- Photometric determination on iron content in water
ВЛМ 06/10.04.2024- Photometric determination of manganese content in water
ВЛМ 07/10.04.2024- Internal laboratory metod for determining oxidizability in water from swimming pools.
ВЛМ 08/10.04.2024- Photometric determination of nitrite content in water
ВЛМ 09/10.04.2024- Photometric determination of nitrate content in water
ВЛМ 10/10.04.2024- Photometric determination of phosphate content in water
ВЛМ 11/10.04.2024- Photometric determination of sulfate content in water
ВЛМ 12/10.04.2024- Photometric determination of chromium content in water
ВЛМ 13/10.04.2024- Photometric determination of fluoride content in water
[bookmark: _GoBack]ВЛМ 14/10.04.2024- Photometric determination of cadmium content in water.
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