SCO 209 ЛИ
Sofia, 29.04.2025
MILITARY FORMATION 24510 - SOFIA, MINISTRY OF DEFENSE
LABORATORY FOR TESTING, ANALYSIS AND QUALITY CONTROL 
OF FUEL-LUBRICANTS AND SPECIAL FLUIDS
Management address: 1271, Sofia, Iliyantsi, Rozhen Blvd.
Laboratory address: 1271, Sofia, Iliyantsi, Rozhen Blvd.
To perform testing of:
	Type of the scope: fixed

	№
	Tested Products
	Type of Test/Characteristic
	Testing methods
(standardized / validated methods)

	1
	2
	3
	4

	1.
	Aviation and
automotive
gasolines
	1.1. Density
	БДС EN ISO 3675
БДС EN ISO 12185

	
	
	1.2. Distillation haracteristics
	БДС EN ISO 3405

	
	
	1.3. Acidity
	БДС 1752

	
	
	1.4. Gum content
	БДС EN ISO 6246

	
	
	1.5. Corrosiveness of copper strip
	БДС EN ISO 2160

	2.
	Jet fuels
	2.1. Density
	БДС ЕN ISO 3675
БДС EN ISO 12185

	
	
	2.2. Distillation characteristics
	БДС EN ISO 3405

	
	
	2.3. Acidity
	БДС 1752

	
	
	2.4. Gum content
	БДС EN ISO 6246

	
	
	2.5. Flash point in closed cup
	БДС EN ISO 2719

	
	
	2.6. Flash point in closed cup
	А5ТМ D56

	
	
	2.7. Ash
	БДС EN ISO 6245

	
	
	2.8. Kinematic viscosity 
	БДС EN ISO 3104, Procedure A

	
	
	2.9 Freezing Point
	АSТМ D2386

	
	
	2.10. Corrosiveness of copper strip, Class
	БДС EN ISO 2160

	3.
	Fuels for diesel engines,
Gas oils for industrial and communal purposes
	3.1. Density
	БДС EN ISO 3675
БДС EN ISO 12185

	
	
	3.2. Distillation characteristics
	БДС EN ISO 3405

	
	
	3.3. Acidity
	БДС 1752

	
	
	3.4. Ash
	БДС EN ISO 6245

	
	
	3.5. Flash point in closed cup
	БДС EN ISO 2719

	
	
	3.6. Carbon residue
	БДС ISO 6615

	
	
	3.7. Pour point
	БДС EN ISO 3016

	
	
	3.8. Cloud point
	БДС EN ISO 3015

	
	
	3.9. Cold Filter Plugging Point
	БДС EN 116
БДС EN 116/Amendment 1

	
	
	3.10. Cetane index
	БДС EN ISO 4264

	
	
	3.11. Kinematic viscosity 
	БДС EN ISO 3104,
Procedure А

	
	
	3.12. Corrosiveness of copper strip
	БДС EN ISO 2160

	
	
	3.13. Water
	БДС EN ISO 12937

	4.
	Lubricating and hydraulic oils
	4.1. Density
	БДС EN ISO 3675
БДС EN ISO 12185

	
	
	4.2. Acid number
	БДС 1752

	
	
	4.3. Kinematic viscosity 
	БДС EN ISO 3104,
Procedure A

	
	
	4.4. Viscosity index
	БДС ISO 2909

	
	
	4.5. Flash point in closed cup
	БДС EN ISO 2719

	
	
	4.6. Flash point in opencup
	БДС EN ISO 2592

	
	
	4.7. Pour point
	БДС EN ISO 3016

	
	
	4.8. Ash
	БДС EN ISO 6245

	
	
	4.9. Sulfated ash
	БДС ISO 3987

	
	
	4.10. Carbon residue
	БДС ISO 6615

	
	
	4.11. Neutralizing value
	БДС 9776

	
	
	4.12. Water
	БДС EN ISO 12937

	
	
	4.13. Corrosiveness of copper strip
	БДС EN ISO 2160

	5.
	Lubricants
	5.1. Penetration
	БДС ISO 2137

	
	
	5.2. Dropping point
	БДС ISO 2176

	
	
	5.3. Colloidal stability
	БДС 6733

	6.
	Brake fluids for automobiles
	6.1. Density
	БДС EN ISO 3675

	
	
	6.2. Kinematic viscosity 
	БДС EN ISO 3104,
Procedure А

	
	
	6.3. Flash point in open cup
	БДС EN ISO 2592

	
	
	6.4. Boiling point
	БДС 8563



Flexible Scope: Implementing a new version of standards/documents or standards / documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.
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