
INSPECTION BODY OF TYPE С
AT REIJ LTD, PIRDOP
Management Address: 1510, Sofia, Hadzhi Dimitar Residential Area, 
block 25, entrance D, flat 58
Address of the CAB: 2070, Pirdop, 2 Georgi Benkovski Street

To perform inspection:
	Type of scope: Flexible*

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	5

	1.
	Еlectrical installations and equipment up to and 
above 1000 V.




	Installed on new and/or used sites/facilities
	Insulation resistance 

	СР 7.1-6

	Ordinance №16-116, SG №26/2008;

Ordinance №3     
SG №90/2004, №91/2004; 
TS

	
	
	
	Protective grounding installation resistance 
	СР 7.1-1
	Ordinance №16-116, SG №26/2008;
Ordinance № 3 
SG № 90/2004,  
№ 91/2004; 
TS

	
	
	
	Lightning protection and grounding installation resistance
	СР 7.1-2
	Ordinance № 4    
SG № 6/2011;
Ordinance № 16-116, SG №26/2008;

TS

	2.
	Cable lines with voltage up to 20 kV.
	Installed on new and/or used sites/facilities
	Electric resistance of insulation through increased constant voltage
	НИЕМС
СР 7.1-5
	Ordinance №16-116, SG №26/2008;

Ordinance №3    
SG №90/2004, №91/2004;

НИЕМС – 1995;

TS

	3.
	Electrical installations and equipment up to and 
above 1000 V.
	Installed on new and/or used sites/facilities
	Impedance of the “phase-protective conductor” contour


	СР 7.1-3

	Ordinance №16-116, SG №26/2008;

Ordinance №3    
SG №90/2004, №91/2004;

TS

	
	
	
	Protective circuit breakers: 

Contact voltage, trigger current, shut-off time
	СР 7.1-4
	Ordinance №16-116, SG №26/2008;

Ordinance №3    
SG №90/2004, №91/2004;

TS


*Flexible scope: Introduction of new versions of standards/documents or standards/documents that replace them is allowed. An up-to-date list of standards/documents with their dated versions is provided by the CAB

Ordinance № 3 on the structure of electrical systems and power transmission lines (SG № 90/2004 and № 91/2004, amended and supplemented in the SG, № 92/2013);

Ordinance № 16-116 on the technical use of power equipment (SG № 26/2008; amended and supplemented in the SG № 4/2015);

Ordinance № 4 on the lightning protection of buildings, outdoor facilities and open spaces (SG № 6/2011);

НИЕМС-1985 Methodology instruction for measuring and evaluation of artificial illumination in buildings 40-85, Standardisation Publishing House 1985;

TS – technical specification.
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