
ORDER

№ A 36
Sofia, 29.01.2025
To perform inspection of:
	Type of the Scope: Flexible*

	№


	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, SpecificationsSchemes

	1
	2
	3
	4
	5
	6

	1
	Working environment microclimate
	new and/or operated sites facilities
	Air temperature
Relative humidity Air velocity
	БДС 16686
Ordinance № RD-07-3 

SG № 63/2014
СКК 7.1 РПК 1/1
	Ordinance № 24 

SG № 95/2003;
Ordinance № 9 

SG № 46/1994;
Ordinance № 2 

SG № 15/2007;
Ordinance № 3 

SG № 15/2007;
Ordinance № 26 

SG № 103/2008;
Ordinance № RD-07-3 

SG № 63/2014;
Ordinance № RD-02-20-3 

(SG № 5/2016, amend. 13/2016), Art. 266, clauses 1, 2, 3, 4, 5 

БДС 14776;
 TS

	2
	Working environment noise
	new and/or operated sites facilities
	Daily noise exposure level, Average weekly noise exposure level, 

Peak sound pressure level
	БДС ISO 1999
БДС EN ISO 9612
СКК 10 РПК 2/1
	Ordinance № 6 

SG № 70/2005; TS

	3
	Noise in residential and public buildings
	new and or operated sites facilities
	Noise level, Equivalent noise level in
	БДС 15471
СКК 10 РПК 3/1
	Ordinance № 6 

SG № 58/2006; 

Appendix 2, Table 1;
Ordinance № 6 

SG № 16 1977; 

Ordinance № 24 

SG № 95/2003;

Ordinance № 2 

SG № 15/2007; 

Ordinance № 9 

SG № 46/ 1994; Ordinance № 26 

SG № 103/ 2008; Ordinance № RD-02-20-3

(SG № 5 /2016), 

Art. 266, cl. 7; TS

	4
	Noise in different territories and development zone in and out of urban areas

	new and or operated sites/facilities
	Equivalent noise level
	БДС 15471
СКК 10 РПК 3/1
	Ordinance № 6 

SG № 58/2006;

Appendix 2, Table 2

	5
	Artificial lighting in a working environment
	new and or operated sites/facilities
	Illumination
	Methodological instructions for measuring artificial lighting in buildings 

40-85, issue Standardization 1985,
СКК 7.1 

РПК 4/1
	Ordinance № 49 

SG № 7/1976;
Ordinance № 24 

SG № 95/2003;
Ordinance № 9 

SG № 46/1994;
Ordinance № 2

SG № 15/2007;
Ordinance № 26 

SG № 103 2008;
Ordinance № 3

SG № 15/2007; 

Ordinance № RD-02-20-3 

(SG № 5 /2016)
art. 89, table 11; 

art. 142, para 4, Appendix 4;
Art. 207, para 1,2;
Art. 217, cl. 3; 

Art. 233;
Art. 234, para. 2; 

Art. 243, para 2, cl. D; 

Art. 266 table 15; 

БДС EN 12464-1:2011; 
TS

	6
	Ventilation installations
	new and or operated sites/facilities
	Air flow velocity. Air flow
	БДС 12.3.018
СКК 7.1 РПК 5/1
	Ordinance № 15 

SG № 68/ 2005;
Ordinance № RD-02-20-3 

(SG № 5 / 2016), 

Art. 87, Table 10; 

Art. 151 Appendix 5; 

Art. 217 cl. 6;
Art. 243 para. 2. cl. C;
Art. 266 cl. 5; 
TS

	7
	Chemical factors of the working environment
	new and or operated sites/facilities
	Concentration of chemical agents in the air of the working environment - by linear colorimetric method (indicator tubes)
	БДС EN 689+AC 

БДС EN 482 Methodological instruction for determination of toxic gases and vapours in the air of the working environment by linear-colorimetric methods book 2 Issued by the Medical Academy, Scientific Institute of Hygiene and Occupational Diseases, Association Higitest, 1987 СКК 7.1 

РПК 7/ 1:13
	Ordinance № 13 

SG № 8/ 2004; 


	
	
	
	Dust

concentration inhalable

fraction in the air

of the working environment
	БДС 2200

БДС EN 689 +АС

БДС EN 482

БДС EN 481

СКК 7.1 РПК 6/1
	Ordinance №13 

SG № 8 /2004;


	8.
	Electrical installations and equipment up to 1000V
	new and-or operated sites/facilities
	Insulation resistance
	БДС 1986 cl.
3.3 а), б), д) and е)
СКК 7.1 РПК 8/1
	Ordinance № 3  

SG № 90, 91/2004)
Ordinance № 16-116 

(SG № 26/ 2008); 
TS

	
	
	
	Resistance of protective earthing systems
	СКК 7.1 РПК 9/1
	Ordinance № 3 

(SG № 90 and 91/ 2004)
Ordinance № 16-116 

(SG № 26 /2008); 
TS

	
	
	
	Resistance of lightning protection earthing systems
	СКК 7.1 

РПК 9/1
	Ordinance № 4 

(SG № 6/2011); 
TS

	
	
	
	Phase- protective conductor circuit impedance
	СКК 7.1
РПК 10/1
	Ordinance № 3 

(SG № 90, 91/2004)
Ordinance № 16-116 

(SG № 26/ 2008)

TS

	
	
	
	Switches for protective switch-off
- trigger current - shutdown time
- touch voltage
	СКК 7.1
РПК 11/1
	Ordinance № 3 

(SG № 90, 91/ 2004)
Ordinance № 16-116 

(SG № 26/ 2008); 

TS


*Implementing of new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.

Ordinance № 2 on the health requirements for computer and Internet halls for public use (SG № 15/2007);

Ordinance No. 3 on the health requirements to the kindergartens (SG, No. 15/2007);

Ordinance № 3 on the design of electrical installations and power lines (SG № 90 and № 91/2004); 
Ordinance No. 4 regarding the lightning protection of buildings, outdoor facilities and open-air spaces (SG, No.6/2011);

Ordinance № 6 on the minimum requirements to ensure the health and safety of workers at risks related to exposure to noise (SG № 70/2005);
Ordinance № 6 to ensure a normal acoustic environment in residential and public buildings and places (SG № 16/1977);

Ordinance № 6 on the indicators of noise in the environment taking into degree of discomfort during the different parts of the day, the limit values of the indicators of noise in the environment in the premises of residential and public buildings in zones and territories intended for residential construction, reaction zones and territories and zones mixed use the methods for assessing the value of noise indicators and the harmful effects of noise on the heath of the population (SG  No 58/2006);

Ordinance № 9 on the health and hygiene requirements for the use of personal computers in the education and extracurricular activities of students (SG № 46 1994);

Ordinance № 15 on the technical rules and norms for the design. construction and operation of sites and facilities for production, transmission and distribution of heat energy (SG № 68/ 2005);

Ordinance № 26 on the structure and activity of the nurseries and children kitchens (SG № 103/2008);
Ordinance No. 24 regarding the sanitary and hygienic requirements to the disco clubs (SG, No. 95/2003);

Ordinance № 49 on artificial lighting of buildings (SG № 7/1976);\

Ordinance № 16-116 on the technical operation of energy equipment (SG № 26/ 2008);

Methodological instructions for measuring and assessment of artificial lighting in buildings 40-85, issue 1985;

Ordinance № RD-07-03 on the minimum requirements for the microclimate of the workplaces (SG № 63/2014);

Ordinance № 13 on the protection of workers from risks related to exposure to chemical agents at work (SG № 8/2004);

Ordinance № RD-02-20-3 on the design, implementation and maintenance of public service buildings in the field of education and science, healthcare, culture and arts (SG № 5/2016);

TS - Technical specification of the client.
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