ORDER 

No. A 48
Sofia, 11.02.2025
INSPECTION BODY OF TYPE C „CMC-C-CONTROL”

AT „CMC-C” EOOD, PIRDOP

Management address: 

Sofia, 3 „Academic Yordan Trifonov” str., D, fl.7, app. 39

Office address: 

2070 Pirdop, 3 „Georgi Benkovski” str.       
To perform inspection according to the following scope:
	Type of the scope: flexible*

	№
	Field of Inspection
	Type of Inspection
	Parameter of inspection/

 Characteristic
	Test and Measurement Methods Used During Inspection
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1
	Electrical installations and facilities up to and over 1000V
	At new or existing/ in operation objects/ facilities 
	Insulation resistance 
	Procedure

Attachment 5.3,

НИЕМС-1995

БДС 1986, item 3.3

a), b), e), f)
	НУЕУЕЛ № 3/2004 (State Gazette, issue 90, 91/2004)

НТЕЕ № 16-116 (State Gazette, issue 26/2008)

НИЕМС-1995

TS

	
	
	
	Resistance of protective grounding installations 
	Procedure

Attachment 5.1,


	НУЕУЕЛ № 3/2004 (State Gazette, issue 90, 91/2004)

НТЕЕ № 16-116 (State Gazette, issue 26/2008)

TS

	
	
	
	Resistance of lightning grounding installations 
	Procedure

Attachment 5.1,


	НУЕУЕЛ № 3/2004 (State Gazette, issue 90, protection 91/2004)

НТЕЕ № 16-116 (State Gazette, issue 26/2008)

Ordinance № 4 (State Gazette, issue 6/2011)

TS

	
	
	
	Apparatus for protection of electricity leakages with continuous and with preliminary control of insulation in IT networks with voltage of up to 1200V:

-Resistance of activation,

-Own time of activation and continuous current upon one-phase leakage

-Measurement current   
	Procedure

Attachment 5.7,

БДС 10880


	БДС 10880

TS

	2


	Complete switchgears of up to and over 1000 V 


	At new or existing/ in operation objects/ facilities


	Switches:

-Resistance of insulation,

-Di-electrical strength of insulation with HV, 50Hz,

-Contact resistances,

-Fast and simultaneous action upon switching on/off of contacts,

-Functional checking of drive mechanisms
	Procedure

Attachment 5.8,

НИЕМС-1995


	НИЕМС-1995

НТЕЕ №16-116

(SG, issue 26/ 2008)

БДС EN 60947-1/A1/A2

БДС EN 62271-103

TS

	
	
	
	Measurement transformers: 

-Resistance of insulation,

-Di-electrical strength of insulation with HV, 50Hz,

-Coefficient of transformation 
	Procedure

Attachment 5.8,

БДС EN 61869-2

БДС EN 61869-3
	БДС EN 61869-2

БДС EN 61869-3

НИЕМС-1995

НУЕУЕЛ № 3/2004 (SG, issue 90, 91/2004)

НТЕЕ № 16-116 
(SG, issue 26/2008)

	
	
	
	Relay protections:

-Activation current;

-Activation voltage;

-Time of activation 
	Procedure

Attachment 5.8,

SCRZINE: 2013

 (Modern digital relay protections. Selection, adjustment, operation) 
	НТЕЕ № 16-116

(SG, issue 26/ 2008)



	3
	Electrical installations and facilities of up to 1000V


	At new or existing/ in operation objects/ facilities


	Impedance of the “phase-protective conductor” circle


	Procedure

Attachment 5.2

	НУЕУЕЛ № 3/2004 (State Gazette, issue 90, 91/2004)

НТЕЕ № 16-116 (State Gazette, issue 26/2008)

TS

	
	
	
	Protective switches for currents with zero consecutiveness (Fi switches)

-Activation current,

-Time of switching off,

-Contact voltage 
	Procedure

Attachment 5.6

	НУЕУЕЛ № 3/2004 (SG, issue 90, 91/2004)

НТЕЕ № 16-116 (SG, issue 26/2008)

TS



	4
	Cables and cable conductor lines of voltage up to 20kV
	At new or existing/ in operation objects/ facilities


	Resistance of insulation 
	Procedure

Attachment 5.9,

Edition 1 date 05.04.2019

БДС 1986-82, item  3.3
 a), b), d),e)
	НИЕМС-1995

НТЕЕ № 16-116 (State Gazette, issue 26/2008)

TS

	
	
	
	Electrical strength of insulation with increased, alternating or direct current/ voltage
	БДС 2406
	НИЕМС-1995

НТЕЕ № 16-116 (State Gazette, issue 26/2008)

БДС 2581

TS


* The introduction of a new version of standards/documents or standards/documents that replace them is allowed. An updated list of standards/documents with their dated versions is provided by the CAB.
НУЕУЕЛ – Ordinance № 3 (SG, issue 90 and 91/2004) on the arrangement of electrical installations and electric conductor lines;

НТЕЕ – Ordinance № 16-116 (SG, issue 26/2008) on the technical operation of electrical furniture and equipment;

Ordinance № 4 (SG, issue 6/ 18.01.2011) on the lightning protection of buildings, outdoor facilities and open spaces;

НИЕМС – 1995 – Norms on testing of electrical machines and facilities – 1995 of the Energy Commission;
TS - Technical specification of the client.
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