
                        








 “BULAQUA STANDART” Ltd
CERTIFICATION BODY FOR CONSTRUCTION PRODUCTS 
“QUALITY MARK OF BWA”


Management and office address: 1046 Sofia, Lozenets district, 1 Hristo Smirnenski Blvd., UACEG - Rectorate, office 115

To perform certification of construction products in the voluntary (unregulated) field, according to the following scope:
	Scope type: flexible*

	No.
	PRODUCTS
	CERTIFICATION SCHEME
	STANDARD/REGULATORY DOCUMENT

	1
	2
	3
	4

	1.
	Plastic piping systems for:

	Water supply from:

	1.1
	Polyethylene PE
	CP 7.0 (A) Certification process - scheme “A”- voluntary certification,
WP 7.0-1 (A) Working procedure for certification of plastic piping systems - scheme “A”
	БДС EN 12201-1;
БДС EN 12201-1/NA;
БДС EN 12201-2+A1;
БДС EN 12201-2+A1/NA; БДС EN 12201-3+A1;
БДС EN 12201-3+A1/NA; БДС EN 12201-4;
SD CEN/TS 12201-7.

	1.2
	Thermosetting plastics (GRP)
	CP 7.0 (A) Certification process - scheme "A"- voluntary certification,
WP 7.0-1 (A) Working procedure for certification of plastic piping systems - scheme “A”
	БДС EN ISO 23856

	Drainage and sewerage:

	1.3
	Thermosetting plastics (GRP)
	CP 7.0 (A) Certification process - scheme "A"- voluntary certification,
WP 7.0-1 (A) Working procedure for certification of plastic piping systems - scheme “A”
	БДС EN ISO 23856;
БДС EN ISO 23856/NA.

	1.4
	Underground 
non-pressure;
Pipes and connecting parts made of PVC-U;
PP; PE
	CP 7.0 (A) Certification process - scheme "A"- voluntary certification,
WP 7.0-1 (A) Working procedure for certification of plastic piping systems - scheme “A”
	БДС EN 13476-1;
БДС EN 13476-2+A1;
БДС EN 13476-2+A1/NA;
БДС EN 13476-3+A1;
БДС EN 13476-3+A1/NA;
SD CEN/TS 13476-4.

	1.5
	Plastic shafts and inspection chambers
	CP 7.0 (A) Certification process - scheme "A"- voluntary certification,
WP 7.0-1 (A) Working procedure for certification of plastic piping systems - scheme “A”
	БДС EN 13598-1;
БДС EN 13598-2;
SD CEN/TS 13598-3.

	2.
	Vitrified claypiping systems for    sewerage
	CP 7.0 (A) Certification process - scheme "A"- voluntary certification,
WP 7.0-3 (A) Working procedure for certification of glass-ceramic piping systems - scheme “A”
	БДС EN 295-1;
БДС EN 295-2;
БДС EN 295-3;
БДС EN 295-4;
БДС EN 295-7.

	3.
	Piping systems made of ductile iron
	CP 7.0 (A) Certification process - scheme "A"- voluntary certification,
WP 7.0-2 (A) Working procedure for certification of ductile iron piping systems - scheme “A”
	БДС EN 545


* The introduction of a new version of the standards or standards that substitute them is permitted. An updated list of the standards with their dated versions shall be provided by CAB.
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