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To perform control, according to the following range:

	№
	Field of inspection
	Type of inspection
	Parameter / feature inspected
	Test / measurement methods used in inspection; inspection procedure
	Regulations, standards, specifications, control schemes

	[bookmark: _Hlk187658962]1
	2
	3
	4
	5
	6

	Scope type: flexible*

	




1.
	



Noise in the working environment
	



At new and/or operational sites / facilities
	Noise level,
Equivalent noise level
Daily noise exposure level,
Average weekly noise exposure level – 
Peak sound pressure level
	



БДС ISO 1999 
(БДС EN ISO 9612) 
РП ОК 10-2
	



Ordinance 6/2005, 
(SG 70/2005)
TS

	



2.
	Noise in the surrounding environmet, in different territories and development zones in urbanized territories and outside of them

 areas
	


At new and/or operational sites / facilities
	



Equivalent noise level
	


БДС 15471 
РП ОК 10-2
	


Ordinance 6/2006, 
(SG 58/06), Appendix 2 to Table 2 
TS



	3.
	Noise in premises within residential and public buildings
	At new and/or operational sites / facilities
	Noise level,
Equivalent noise level

	БДС 15471
РП ОК 10-2
	Ordinance № 6 
(SG 16/1977)
Ordinance № 6 
(SG 58/2006) - Appendix 2 to Table 1
Ordinance № 9 
(SG 46/1994)
Ordinance № 24 (SG 95/2003)
Ordinance № 2 
(SG 15/2007)
Ordinance № 26 (SG 103/2008)
TS

	4.
	Artificial lighting in work and home environments
	At new and/or operational sites / facilities
	Luminosity
	Methodological guidance on measuring artificial lighting - 1985, Standartizacia publisher
РП ОК 10-6
	Ordinance № 49 (SG 7/1976)
Ordinance № 24 (SG 95/2003)
Ordinance № 9 
(SG 46/1994)
Ordinance № 2 
(SG 15/2007)
Ordinance № 3 
(SG 15/2007)
Ordinance № 26,
(SG 103/2008)
Ordinance РД-02-20- 3/ (SG 5/ 2016]
БДС EN 12 464-1
TS

	5.
	Microclimate in work and living environment
	At new and/or operational sites / facilities
	Air temperature
Relative humidity of air
Airflow velocity
	




БДС 16 686
Ordinance № РД-07- 3, SG 63/2014
РП ОК 10-1


















	Ordinance РД-02-20- 3/ (SG 5/ 2016)
Ordinance № 3 
(SG 15/2007)
Ordinance № 9 
(SG 46/1994)
Ordinance № 2 
(SG 15/2007)
Ordinance № 24 (SG 95/2003)
Ordinance № 26, (SG 103/2008)
Ordinance № РД-07-3 (SG 63/2014)
БДС 14776
TS

	6
	Ventilation systems
	At new and/or operational sites / facilities
	Airflow velocity
Air flow
	БДС 12.3.018
РП ОК 10-8













	Ordinance № 24 (SG 95/2003)
Ordinance № 15, (SG 68/2005)
TS











	7
	Electrical installations and equipment up to 1000 V
	At new and/or operational sites / facilities
	Resistance of protective earthing systems
	РП ОК 10-3
	Ordinance № 3 
(SG 90 & 91/2004)
Ordinance № 16- 116 (SG 26/2008)
TS

	
	
	At new and/or operational sites / facilities
	Resistance of lightning protection earthing systems
	РП ОК 10-4
	Ordinance № 4 
(SG 6/2011) 
TS

	
	
	At new and/or operational sites / facilities
	Impedance of the phase-protective wire circuit
	РП ОК 10-5
	Ordinance № 3 
(SG 90 & 91/2004)
Ordinance № 16- 116 (SG 26/2008)
TS

	
	
	At new and/or operational sites / facilities
	Circuit breakers 
- Trigger current, 
- Impedance voltage 
-triggering time 
-resistance of protective earthing
	РП ОК 10-7
	Ordinance № 3 
(SG 90 & 91/2004)
Ordinance № 16- 116 (SG 26/2008)
TS

	
	
	At new and/or operational sites / facilities
	Insulation resistance
	РП ОК 10-9 
БДС 1986 - p.3.3 a), b), d), e)
	Ordinance № 3 
(SG 90 & 91/2004)
Ordinance № 16- 116 (SG 26/2008)
TS



* The introduction of a new version of standards/documents or standards/documents, which replace them, is allowed. An actual list of the standards/documents with their dated versions are given by the conformity assessment body.

Ordinance № 6 - on the minimum requirements for ensuring the health and safety of workers in case of risks related to noise exposure (SG № 70/2005);
Ordinance № 6 - on environmental noise indicators taking into account the degree of discomfort during different parts of the day, the threshold values of environmental noise indicators in the premises of residential and public buildings, zones and territories intended for residential construction, recreational zones and territories and zones with mixed purpose, methods for estimating the values of noise indicators and the harmful effects of noise on public health (SG 58/200б amendment SG 100/2021);
Ordinance № 9 - on the health and hygiene requirements for the use of personal computers in the education and extracurricular activities of students (SG 46/1994);
Ordinance № 24 - on cleaning and sanitary requirements for disco clubs (SG 95/2003);
Ordinance № 2 - on the health requirements for computer and Internet rooms for public use (SG 15/2007);
Ordinance № 26 - on the structure and operation of nurseries and children's kitchens and health requirements for them (SG 103/2008);
Ordinance № 3 - on the health requirements for kindergartens (SG № 15/2007);
Ordinance № RD-07-3 on the minimum requirements for the microclimate of workplaces (SG 63/2014);
Ordinance № 15 - on technical rules and regulations for design, construction and operation of sites and facilities for production, transmission and distribution of heat (SG 68/2005);
Ordinance № 3 - on the design of electrical installations and power lines (SG 90 and 91/2004);
Ordinance № 16-116 on technical maintenance of power equipment (SG 26/2008);
Ordinance № 4 on lightning protection of buildings, outdoor facilities and open-air spaces (SG 6/2011);
Ordinance № 49 - on artificial lighting of buildings (SG № 7/1976);
Ordinance № RD-02-20-3 for design, construction, maintenance of public maintenance buildings in the field of education and science, healthcare, culture and arts (SG 5/2016)
Ordinance № 6 - on ensuring a normal acoustic environment in residential and public buildings and places (SG № 16/1977);
TS - Technical specification.
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