


                    
[bookmark: bookmark0]ODIKO - 69 Ltd., Plovdiv
Inspection Body of Type C

Address of management and office:
4000 Plovdiv, 100 Maritsa Blvd.
To perform inspection of:
	Type of scope: flexible for part of the scope*

	№ 
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test / Measurement Methods Used During Inspection; Inspection Procedure
	Regulatory Acts, Standards, Specifications, Inspection Schemes

	1
	2
	3
	4
	5
	6

	1.
	Noise in working environment
	New and/or in-service facilities and equipment
	Daily noise exposure level;
Weekly average noise exposure level;
Peak sound pressure 
	БДС EN ISO 9612
(БДС ISO 1999) 
РПК 01
	Ordinance № 6 SG № 70/2005
TC

	1.1
	Noise in premises of residential and public buildings
	New and/or in-service facilities and equipment
	Noise level;
Equivalent noise level
	БДС 15471
РПК 01
	Ordinance № 6 SG № 58/2006 (Annex 2, Table 1)
Ordinance № 9 SG № 46/1994
Ordinance № 6 SG № 16/1977
Ordinance № 2 SG № 15/2007
Ordinance № 26 SG № 103/2008
Ordinance № 24 SG № 95/2003 
Ordinance № 7 SG № 88/1999 (Art. 138)
TC

	1.2
	Environmental noise within various territories and zoning areas in urbanized territories and outside them
	New and/or in-service facilities and equipment
	Noise level; Equivalent noise level
	БДС 15471
РПК 01
	Ordinance № 6 SG № 58/2006 (Annex 2, Table 2)
TC

	2.
	Microclimate in working and living environment
	New and/or in-service facilities and equipment
	-air temperature
-relative air humidity
-air velocity
	БДС 16686
Ordinance № РД-07-3 SG № 63/2014 
РПК 02
	Ordinance № 24 SG № 95/2003 
Ordinance № 26 SG № 103/2008 
Ordinance № 9 SG № 46/1994 
Ordinance № 2 SG № 15/2007 
Ordinance № 3 SG № 15/2007 
Ordinance № РД-07-3 SG № 63/2014 
Instruction № 34 SG № 82/1975 БДС 14776 
Ordinance № 8 SG № 74/1985
TC

	2.1
	Microclimate in working and living environment
	New and/or in-service facilities and equipment
	Radiant heat flux density
	БДС 16686
Ordinance № РД-07-3 SG № 63/2014
РПК 02
	БДС 14776 Ordinance № РД-07-3 SG № 63/2014
TC

	2.2
	Microclimate in moderate environment
	New and/or in-service facilities and equipment
	· Predicted mean vote (PMV)
· Predicted percentage of dissatisfied (PPD)
-Local thermal discomfort (PD)
	БДС EN ISO 7730
РПК 17
TC
	БДС EN ISO 7730
TC

	3
	Microclimate in hot environment using the WBGT index
	New and/or in-service sites and/or facilities
	Heat stress index WBGT determined by:
1. black globe temperature
2. natural wet-bulb temperature
3. air temperature
	БДС EN ISO 7243
БДС EN ISO 8996
Methodological guidelines for conducting measurements for determination of the WBGT index in hot environment – Collection of Methods for Hygienic Investigations, National Center of Hygiene, Medical Ecology, and Nutrition, Vol. 4/2002**
РПК 15
	БДС EN ISO 7243
БДС EN ISO 7726
TC

	4
	Artificial lighting in working and living environment
	New and/or in-service facilities and equipment
	Illumination
	Methodological guidelines on measurement of artificial lighting in buildings, 40-85,
Ed. Standardization, 1985
БДС EN 12464-2
РПК 03
	БДС EN 12464-1
БДС EN 12464-2
Ordinance № 49 SG № 7/1976
Ordinance № 2 SG № 15/2007
Ordinance № 3 SG № 15/2007
Ordinance № 9 SG № 46/1994 
Ordinance № 24 SG № 95/2003 
Ordinance № 26 SG № 103/2008 
Ordinance I3-1971 SG № 96/2009 (Art. 55 (6)) 
Ordinance РД-02-20-3 SG № 5/2016
Ordinance № 28 SG № 109/2008 
Ordinance № 19 SG № 79/2008 
Instruction № 34 SG № 82/1975
TC

	5.
	Vibrations transmitted to the hand-arm system and to the whole body
	New and/or in-service facilities and equipment
	-daily exposure value of vibrations transmitted to the hand-arm system
-daily exposure value of vibrations transmitted to the whole body
	БДС EN ISO 5349-1
БДС EN ISO 5349-2
БДС EN ISO 5349-2/A1
БДС ISO 2631-1
РПК 06
	Ordinance № 3 SG № 40/2005
TC

	5.1
	Vibrations in residential environment
	New and/or in-service facilities and equipment
	-mean square value of vibration acceleration in octave bands with mean geometric frequencies
	Ordinance № 9 SG № 17/2010
РПК 06
	Ordinance № 9 SG № 17/2010
TC

	6
	Electromagnetic fields
	New and/or in-service facilities and equipment
	Electric field intensity (5 Hz≤f≤ 400 kHz)
Magnetic flux density (magnetic induction) (5 Hz≤f≤400 kHz)
	· Methodology for investigation and assessment of electromagnetic radiation in departments for physical therapy and rehabilitation, Vol. I, Section “Working Environment – Non-ionizing Radiation”, National Center of Hygiene, Medical Ecology, and Nutrition, First Edition, Sofia, 1999 **
· Methodology for investigation and assessment of electromagnetic radiation at workplaces with visual display units – Collection of Methods of the National Center of Hygiene, Medical Ecology, and Nutrition, Vol. 1/1999 **
· Methodology for investigation and assessment of electromagnetic radiation in high-voltage substations (open and enclosed switchgear) and transformer stations, Vol. I, Section “Working Environment – Non-ionizing 
· Radiation“, National Center of 
· Hygiene, Medical Ecology, and Nutrition, First Edition, Sofia, 1999 **
· Recommended Practical Guides developed by the European Commission for the implementation of ** Ordinance № РД-07-5, dated 15/11/2016 on the minimum requirements for ensuring the health and safety of workers exposed to risks arising from electromagnetic fields (SG № 95/2016)
РПК 12
	Ordinance № РД-07-5 SG № 95/2016 (Council Recommendation 1999/519/ЕС, dated 12/07/1999) **
Ordinance № 9 SG № 46/1994
Ordinance № 2 SG № 15/2007
TC

	7
	Dust in the air of the working environment
	New and/or in-service facilities and equipment
	Dust concentration in workplace air:
-inhalable fraction
-respirable fraction
	БДС EN 689+АС;
БДС 2200;
БДС EN 482; Collection of Methods for Hygienic Investigations, National Center of Hygiene, Medical Ecology, and Nutrition, Vol. 1/1999**
РПК 04
	Ordinance № 13 SG № 8/2004
Ordinance № 10 SG № 94/2003
TC

	8
	Chemical agents in the air of the working environment
	New and/or in-service facilities and equipment
	-Concentration of chemical agents in workplace air determined by the linear colorimetric method (using indicator tubes)
	БДС EN 482;
БДС EN 689+АС;
РПК 05
	Ordinance № 13 SG № 8/2004
Ordinance № 10 SG № 94/2003
TC

	8.1
	Chemical agents in the air of premises in residential and/or public buildings
	New and/or in-service facilities and equipment
	-Indoor air quality through measurement of carbon dioxide (CO2) concentration by the linear colorimetric method (using indicator tubes)
	БДС EN ISO 16000-26
РПК 05
	БДС EN ISO 16000-26, Annex B, Table B1
TC

	9
	Physical stress
	Individuals
	Heart rate
	Method for telemetric measurement of 
	Method for telemetric measurement of heart rate during work – Collection of Methods of the National Center of Hygiene, Medical Ecology, and Nutrition, Vol. II, 2000 **
БДС EN ISO 8996

	
	
	
	
	heart rate during work – Collection of Methods of the National Center of Hygiene, Medical Ecology, and Nutrition, Vol. II, 2000 **
БДС EN ISO 9886
РПК 07
	

	10
	Electrical installations and equipment up to 1000 V
	New and/or in-service facilities and equipment
	Loop impedance “phase–protective conductor”
	Ordinance № РД-02- 20-1 (SG № 53/2018), Annex 4
РПК 08
	Ordinance № 3 SG № 90 and 91/2004 Ordinance № 16-116 SG № 26/2008 Ordinance № 1 SG № 46/2010
TC

	11
	Electrical installations and equipment up to 1000 V
	New and/or in-service facilities and equipment
	Insulation resistance
	Ordinance № РД-02- 20-1 (SG № 53/2018), Annex 2
РПК 09
	Ordinance № 16-116 SG № 26/2008 Ordinance № 3 SG № 90 and 91/2004 Ordinance № 1 SG № 46/2010 Ordinance № РД-02-20-1 (SG № 53/2018), Annex 2
TC

	12
	Electrical installations and equipment up to and above 1000 V
	New and/or in-service facilities and equipment
	-Resistance of protective earthing installations
-Resistance of earthing system for protection against static electricity
	Ordinance № РД-02- 20-1 (SG № 53/2018), Annex 3
РПК 10
	Ordinance № 3 SG № 90 and 91/2004
Ordinance № 16-116 SG № 26/2008
Ordinance № 1 SG № 46/2010 
Ordinance № 21 SG № 41/2007
БДС 15969
БДС 3820
TC

	12.1
	Electrical installations and equipment up to and above 1000 V
	New and/or in-service facilities and equipment
	-Resistance of lightning protection earthing installations
	Ordinance № РД-02- 20-1 (SG № 53/2018), Annex 3
РПК 10
	Ordinance № РД-02-20 -1 SG № 11/2017
Ordinance № 4 SG № 6/2011
Ordinance № 21 SG № 41/2007
TC

	12.2
	Electrical installations and equipment up to 1000 V
	New and/or in-service facilities and equipment
	-specific soil resistivity (4-point method)
	РПК 20
-БДС 15705/ Amendment 1

	TC

	13
	Electrical installations and equipment up to 1000 V
	New and/or in-service facilities and equipment
	Protective circuit breakers:
· touch voltage
· disconnection time of protection
· tripping current
· protective earthing resistance (contact resistance)
	Ordinance № РД-02- 20-1 (SG № 53/2018), Annex 5
РПК 11
	Ordinance № 3 SG № 90, 91/2004
Ordinance № 16-116 SG № 26/2008
Ordinance № 1 SG № 46/2010
TC

	14
	Ventilation installations
	New and/or in-service facilities and equipment
	-airflow velocity
-airflow rate
	БДС 12.3.018
РПК 13
	Ordinance № 15 SG № 68/2005
Ordinance № 24 SG № 95/2003
Instruction № 34 (SG № 82/1975)
TC

	15
	Air-conditioning installations
	New and/or in-service facilities and equipment
	· air temperature
· relative air humidity
	БДС 16686 Ordinance № РД 07-3 SG № 63/2014
РПК 14
	Ordinance № 15 SG № 68/2005
Ordinance РД 07-3 SG № 63/2014
БДС 14776
TC

	16
	Thermal radiation from appliances, apparatus, machines, equipment, cables, busbars, etc.
	New and/or in-service facilities and equipment
	-temperature of the facility/equipment measured using remote IR temperature measuring devices
	РПК 19
	Ordinance № 3 SG № 90 and 91/2004
Ordinance № 9 SG № 72/2004
-Ordinance on the structure, safe operation, and technical supervision of gas facilities and installations for liquefied hydrocarbon gases: Art. 80 (SG № 82/2004),TC

	17
	Electrochemical (cathodic) corrosion protection of underground metal structures
	New and/or in-service facilities/equipment
	-stationary potential
-total polarization potential
-polarization potential
-specific insulation transition resistance
-potential of galvanic anodes
-anode earthing resistance
-potential difference between different underground metal structures
-specific electrical soil resistivity
-stray currents in the ground
-current density
	БДС 15705/ Amendment 1
БДС EN 13509
РПК 18
	БДС 15704;
БДС 15705;
Ordinance on the structure, safe operation, and technical supervision of gas facilities and installations for liquefied hydrocarbon gases (Art. 15) (SG № 82/2004) 
-Ordinance on the structure, safe operation, and technical supervision of pressure equipment (Art. 134, 136, 137, 138, and 139) (SG № 64/2008)
-Ordinance on the structure and safe operation of transmission and distribution gas pipelines and of equipment, installations, and facilities for natural gas (SG № 67/2004)
TC



*Implementing a new version of standards/documents, or of standards/documents that replace them, is allowed. An updated list of the standards/documents with their dated versions is provided by the Conformity Assessment Body (CAB).

Ordinance № 6 on the minimum requirements for the provision of health and safety of workers against risks related to noise exposure (SG № 70/2005)
Ordinance № 9 on the hygiene requirements regarding the use of personal computers in the learning activities of pupils (SG № 46/1994)
Ordinance № 26 on the organization and activities of nurseries and children’s meal centres and the relevant health requirements (SG № 103/2008)
Ordinance № 7 on the minimum requirements for health and safety at work and for the use of work equipment (SG № 88/1999)
Ordinance № 6 on environmental noise indicators, taking into account the degree of annoyance during different parts of the day, the limit values of the environmental noise indicators, in premises of residential and public buildings, zones and areas designated for housing, recreation, and mixed use, the methods for assessment of the noise indicators’ values and the adverse effects of noise on public health (SG № 58/2006)
Ordinance № 2 on the health requirements regarding public computer rooms and Internet cafés (SG № 15/2007)
Ordinance № 24 on the sanitary and hygiene requirements regarding nightclubs (SG № 95/2003)
Ordinance № 6 on ensuring a normal acoustic environment in residential and public buildings and places (SG № 16/1977)
Ordinance № 3 on the health requirements regarding nurseries (SG № 15/2007)
Ordinance РД-07-3 on the minimum requirements for the microclimate of workplaces, dated 18/07/2014 (published in SG № 63, dated 01/08/2014)
Ordinance № 49 on artificial lighting in buildings (SG № 7/1976)
Instruction № 34 on the hygiene of sports facilities and equipment (SG № 82/1975)
Ordinance № 8 on the microclimate in underground mine facilities (SG № 74/1985)
Ordinance № 3 on the minimum requirements for the provision of health and safety of workers against risks related to vibration exposure (SG № 40/2005)
Ordinance № 9 on the maximum permissible values of vibrations in residential environment (SG № 17/2010) 
Ordinance I3-1971 on the construction and technical rules and regulations for fire safety (SG № 96/2009)
Ordinance РД-02-20-3 on the design, implementation and maintenance of public service buildings in the field of education and science, healthcare, culture, and arts (SG № 5/2016)
Ordinance № 28 on the structure, rules and organization of the activities of pharmacies and the nomenclature of medicinal products (SG № 109/2008)
Ordinance № 19 on the structure and activities of optic centres and the relevant health requirements (SG № 79/2008)
Ordinance № 13 on the protection of workers from risks related to exposure to chemical agents at work (SG № 8/2004)
Ordinance № 10 on the protection of workers from risks arising from exposure to carcinogens, mutagens or reprotoxic substances at work (SG № 94/2003) 
Ordinance № 3 on the design of electrical installations and electrical power lines (SG №s 90 and 91/2004)
Ordinance № 16-116 on the technical operation of power equipment (SG № 26/2008)
Ordinance № 1 on the design, construction, and maintenance of low-voltage electrical installations in buildings (SG № 46/2010)
Ordinance № 4 on the lightning protection of buildings, outdoor facilities, and open spaces (SG № 6/2011)
Ordinance № 21 on the rules for construction of mobile telecommunication networks and facilities (SG № 41/2007)
Ordinance РД-02-20-1 on the planning and design of construction sites designated for production, storage and trade of firearms, ammunitions, explosives, and fireworks (SG № 11/2017)
Ordinance РД-02-20-1 on the technical rules and regulations for control and approval of electrical installation works (SG № 53/2018)
Ordinance № 15 on the technical rules and regulations for design, construction, and operation of sites and facilities for production, transmission, and distribution of heating energy (SG № 68/2005)
Ordinance № 9 on the technical operation of power stations and networks (SG № 72/2004)
Ordinance № РД-07-5 on the minimum requirements for ensuring the health and safety of workers at risks related to exposure to electromagnetic fields (SG № 95/2016)
Ordinance on the structure, safe operation, and technical supervision of pressure equipment (SG № 64/2008)
Ordinance on the structure and safe operation of transmission and distribution gas pipelines and of equipment, installations, and facilities for natural gas (SG № 67/2004)
Ordinance on the structure, safe operation, and technical supervision of gas facilities and installations for liquefied hydrocarbon gases (SG № 82/2004)
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**Fixed scope
- Methodological guidelines for conducting measurements for determination of the WBGT index in hot environment – Collection of Methods for Hygienic Investigations, National Center of Hygiene, Medical Ecology, and Nutrition, Vol. 4/2002
- Methodology for investigation and assessment of electromagnetic radiation in departments for physical therapy and rehabilitation, Vol. I, Section “Working Environment – Non-ionizing Radiation”, National Center of Hygiene, Medical Ecology, and Nutrition, First Edition, Sofia, 1999
- Methodology for investigation and assessment of electromagnetic radiation at workplaces with visual display units – Collection of Methods of the National Center of Hygiene, Medical Ecology, and Nutrition, Vol. 1/1999
Methodology for investigation and assessment of electromagnetic radiation in high-voltage substations (open and enclosed switchgear) and transformer stations, Vol. I, Section “Working Environment – Non-ionizing Radiation“, National Center of Hygiene, Medical Ecology, and Nutrition, First Edition, Sofia, 1999
- Recommended Practical Guides developed by the European Commission for the implementation of ** Ordinance № РД-07-5, dated 15/11/2016 (SG № 95/2016)
- Council Recommendation 1999/519/ЕС, dated 12/07/1999
- Collection of Methods for Hygienic Investigations, National Center of Hygiene, Medical Ecology, and Nutrition, Vol. 1/1999
- Method for telemetric measurement of heart rate during work – Collection of Methods of the National Center of Hygiene, Medical Ecology, and Nutrition, Vol. II, 2000
- TС – Technical Specification
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