SCOPE 224 ЛИ
Sofia, 06.12.2025

DMV PETROL LTD
TESTING LABORATORY DMV CONTROL

Management and laboratory address:
7058 Marten, Ruse Region, Petrol Base of DMV Petrol Ltd, PI 47336.9.93

To perform testing of:
	Type of the scope: Flexible for part of the scope

	№
	Tested products
	Type of test / characteristics
	Test methods
(standard/validated method)

	1
	2
	3
	4

	1.
	Fuels for diesel engines
	1.1. Density at 15oC
	ВЛМИ-01/2021

	
	
	1.2. Kinematic viscosity at 40oC
	БДС EN ISO 3104

	
	
	1.3. Distillation characteristics
	БДС EN ISO 3405

	
	
	1.4. Flash point by closed cup
	БДС EN ISO 2719
БДС EN ISO 2719/A1

	
	
	1.5. Cold filter plugging point 
(CFPP)
	БДС EN 116
БДС EN 116/Amendment 1 

	
	
	1.6. Water 
(Karl Fisher method)
	БДС EN ISO 12937

	2.
	Gasoil for industrial and communal purposes
	2.1. Kinematic viscosity at 40oC
	БДС EN ISO 3104

	
	
	2.2. Distillation characteristics
	БДС EN ISO 3405

	
	
	2.3. Flash point by closed cup
	БДС EN ISO 2719
БДС EN ISO 2719/A1

	3.
	Biodiesel
	3.1. Density at 15oC
	ВЛМИ-01/2021

	
	
	3.2. Kinematic viscosity at 40oC
	БДС EN ISO 3104

	
	
	3.3. Flash point by closed cup
	БДС EN ISO 2719
БДС EN ISO 2719/A1

	
	
	3.4. Cold filter plugging point 
(CFPP)
	БДС EN 116
БДС EN 116/Amendment 1

	
	
	3.5. Water 
	БДС EN ISO 12937



Flexible scope: Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.

Fixed scope reference:
VLMI-01/2021 Density determination. Method by oscillation with U-pipe.
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