

ORDER

No. A 67

Sofia, 02.03.2026

INSPECTION BODY OF TYRE C for “Metal Testing” at
"TPP MARITSA EAST 2" EAD, Kovachevo village,
Stara Zagora district

Management and office address: 6265, Kovachevo village, Stara Zagora district

[bookmark: bookmark6]To perform inspection of:
	Type of range: flexible for a part of the scope*

	№
	Field of Inspection
	Type of Inspection
	Parameter of inspection/
Characteristic
	Test and Measurement Methods Used During Inspection
	Regulations, Standards, Specifications, Schemes

	1
	Pressure vessels; Gas facilities and installations; Steam and hot water pipelines; high- and low-pressure boilers; Steam turbines and their components; Machines, equipment, constructions and their components containing welded joints
	Inspection of new and operating sites and equipment
	Radiographic testing method (RT);
Type, size and
location of the
imperfections
	ПК 1-0
Procedure of performing radiographic testing of new and/or operating objects/ equipment.
BDS EN ISO 17636-1
	The Ordinance on the design, safe operation, and technical supervision of pressure equipment /State Gazette, issue 64/2008 
(Art. 19; Art. 21)
The Ordinance on the structure, safe operation and technical supervision of gas facilities and installations for liquefied hydrocarbon gases
/SG, issue 82/2004, (Art. 105);
Technical specification 
BDS EN ISO 6520-1; 
BDS EN 12952-6;
BDS EN 13480-5;
BDS EN 13445-5/А1; 
BDS EN ISO 5817; 
BDS EN ISO 17635; 
BDS EN ISO 10675-1;


	2
	Pressure vessels; Gas facilities and installations; Steam and hot water pipelines; High- and low-pressure boilers; Steam turbines and their components; Machines, equipment, constructions and their components containing: sheets, rolled products, pipes, welded joints, castings
	Inspection of new and operating sites and equipment
	Ultrasonic testing
method (UT)
Type, size and 
location of
the imperfections
	ПК 2-0
Procedure for performing
ultrasonic testing 
of new and/or operating
sites /equipment.
BDS EN ISO 16810;
BDS EN ISO 16827;
BDS EN ISO 11666;
BDS EN ISO 23279;
BDS EN ISO 17640;
BDS 9824;
BDS EN 10308; 
BDS EN 10160; 
BDS EN 10228-3; 
BDS EN 10228-4;
	The Ordinance on the design, safe operation, and technical supervision of pressure equipment  
/SG, issue 64/2008 
(Article 19);
The Ordinance on the structure, safe operation and technical supervision of gas facilities and installations for liquefied hydrocarbon gases /SG, issue 82/2004, (Art.105); 
Technical specification 
BDS EN 10160;
BDS EN ISO 11666; 
BDS EN ISO 17640; 
BDS 9824;
BDS EN 10308;
BDS EN 10228-3;
BDS EN 10228-4;
BDS EN ISO 17635; 
BDS EN ISO 5817; 
BDS EN 12952-2;
BDS EN 12952-6;
BDS EN 13480-5;
BDS EN 13445-5/А1; 
BDS 10037- repealed, without replacement;






	3
	Pressure vessels; Gas facilities and installations; Steam and hot water pipelines; High- and low-pressure boilers; Steam turbines and their components; Machines, equipment, constructions and their components containing: sheets, rolled products, pipes, welded joints, castings and forgings.

	Inspection of new and operating sites and equipment
	Magnetic particle testing method (МТ);
Type, size and 
location of indications.
	ПК 3-0
Procedure
for performing magnetic particle testing of new and/or operating sites /equipment.

BDS EN ISO 9934-1;
BDS EN ISO 17638; 
	The Ordinance on the design, safe operation, and technical supervision of pressure equipment 
/SG, (Article 19);
issue 64/2008, (Art. 20); 

Technical specification 
BDS EN ISO 23278; 
BDS EN 10228-1;
BDS EN ISO 10893-5; 
BDS EN 1369;
BDS EN ISO 17635; 
BDS EN ISO 5817; 
BDS EN 12952-6;
BDS EN 13480-5;
BDS EN 13445-5/А1;

	4
	Pressure vessels; Gas facilities and installations; Steam and hot water pipelines; High- and low-pressure boilers; Steam turbines and their components; Machines, equipment, constructions and their components containing: sheets, rolled products, pipes, welded joints, castings and forgings.
	Inspection of new and operating sites and equipment
	Liquid penetrant testing method (РТ);
Type, size and location of indications.
	ПК 4-0
Procedure for performing liquid penetrant testing 
of new and/or operating sites/equipment 

BDS EN ISO 3452-1;
	The Ordinance on the design, safe operation, and technical supervision of pressure equipment 
/SG issue 64/2008,  
(Art. 20); 
Technical specification 
BDS EN ISO 23277; 
BDS EN 10228-2;
BDS EN ISO 10893-4; 
BDS EN 1371-1;
BDS EN ISO 17635; 
BDS EN ISO 5817; 
BDS EN 12952-6;
BDS EN 13480-5;
BDS EN 13445-5/А1;

	5
	Pressure vessels; Gas facilities and installations; Steam and hot water pipelines; High- and low-pressure boilers; Steam turbines and their components; Machines, equipment,
constructions and their components containing:
sheets, rolled products, pipes, welded joints, castings and forgings.
	Inspection of new and operating sites and equipment
	Hardness testing by Leeb method; Hardness of metal materials in scales: НВ; HV and HRC, after their transformation from scales HLD or HLE 
	ПК 5-1
Procedure for performing hardness testing by Leeb method of new and/or operating sites/equipment.
BDS EN                                     ISO 16859-1;
	Technical specification 
BDS EN 12952-6; 
BDS EN 13445-5/ А1;

	6
	Pressure vessels; Gas facilities and installations; Steam and hot water pipelines; 
High- and low-pressure boilers; Steam turbines and their components; Machines, equipment, constructions and their components containing: sheets, rolled products, pipes, welded joints, castings and forgings.







	Inspection of new and operating sites and equipment
	Ultrasonic method for wall thickness measurement (UT);  
Wall thickness 
	ПК 6-0
Procedure for performing ultrasonic wall thickness measurement of new and/or operating sites/equipment

BDS EN ISO 16809
	Technical specification 


	7
	Elbows and pipes from pipelines and
heating surfaces
	Inspection of new and operating sites and equipment
	Out-of-roundness measurement 
Out-of-roundness

	ПК 7-0
Procedure for performing out-of-roundness measurement of new
and/or operating sites/equipment.
BDS EN 12952-5; BDS EN 13480-4;
	Technical specification 
BDS EN 12952-5; 
BDS EN 13480-4;

	8
	Pressure vessels; Gas facilities and installations; Steam and hot water pipelines; 
High- and low-pressure boilers;
Steam turbines and their components; Machines, equipment, constructions and their components containing: sheets, rolled products, pipes, welded joints, castings and forgings.
	Inspection of new and operating sites and equipment
	Spectral quality inspection
Presence and
type of alloying 
elements: 
Сг, Mo, V
	**ПК 8-0 
Procedure for performing spectral 
quality inspection
of new
and/or operating sites/equipment. (Revision 2, Version 4 as of 30.11.2015)

	Technical specification 


	9
	Pressure vessels; Gas facilities and installations; Steam and hot water pipelines; high- and low-pressure boilers; Steam turbines and their components; Machines, equipment, constructions and their components containing welded joints
	Inspection of new and operating equipment
	Visual testing method (VT)
Type, size and 
location of the
imperfections
	ПК 9-0
Procedure
for performing 
visual inspection
of new and/or operating sites/equipment.

BDS EN ISO 17637
	The Ordinance on the design, safe operation, and technical supervision of pressure equipment /SG issue 64/2008, (Art. 19; Art. 20; Art. 22);
 
Technical specification 
BDS EN ISO 17635; 
BDS EN ISO 5817; 
BDS EN 12952-5; 
BDS EN 12952-6; 
BDS EN 12953-5; 
BDS EN 13480-5; 
BDS EN 13445-5/А1;



*Flexible scope: Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.




References: 
* Flexible scope: The implementation of a new version of standards/documents or standards/documents, which replace them, is allowed. An up-to-date list of standards/ documents with their dated versions is provided by the CAB.
The Ordinance on the design, safe operation, and technical supervision of pressure equipment (adopted by Decree of the Council of Ministers № 164 dated 07.07.2008, State Gazette, issue 64/2008). 
The Ordinance on the structure, safe operation and technical supervision of gas facilities and installations for liquefied hydrocarbon gases (adopted by Decree of the Council of Ministers № 243, dated 10.09.2004, State Gazette, issue 82/2004).
TS - Technical specification.
** Fixed scope:
[bookmark: _GoBack]ПК 8-0 Procedure for performing spectral quality inspection of new and/or operating sites/ equipment. (Revision 2, Version 4 of 30.11.2015).
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