SCOPE 122 ЛИ
Sofia, 19.06.2026
KONTROL 94 LTD.
TESTING LABORATORY
[bookmark: bookmark8]Management address: 5100, Gorna Oryahovitsa, 2 Mladost Str. 
Laboratory address: 5100, Gorna Oryahovitsa, 2 Mladost Str

To perform testing of:
	Type of the scope: flexible*

	№
	Tested products
	Type of test / characteristic
	Testing methods
(standard/ validated method)

	1
	2
	3
	4

	1.
	Multi-firing sauna stoves fired by natural wood logs
	1.1. Temperature safety (fire safety)
	БДС EN 15821, cl. A.4.7

	
	
	1.2. Combustion products emissions (CO; O2; CO2; CO2, NOx; CxHy; OGC; mass of flue gases flow; particulate matter (PM))
	БДС EN 15821, cl. A.4.6, 
cl. A.4.4.2, cl. A.6.2.5, 
cl. A.6.2.8, cl. A.6.2.4);
CEN/TS 15883 (cl. 4, cl. 5);
БДС EN 16510-1, Annex F

	
	
	1.3. Surface temperature
	БДС EN 15821, cl. A.4.6.3

	
	
	1.4. Flue gases temperature
	БДС EN 15821, cl. A.2.3.2, 
cl. A.4.4.3

	
	
	1.5. Heat ouput (nominal heat
output)/ energy efficiency (losses)
	БДС EN 15821, cl. A.4.6 
(cl. A.6.2.2, cl. A.6.2.3)/ 
cl. A.6.2.1, (cl. A.6.2.6)

	2.
	Heating boilers for
solid fuel, manually
and automatically
stoked, nominal heat output of up to 500 kW.
	2.1. Combustion products emissions at nominal and minimum heat output (CO; O2; CO2; NOx; CxHy; OGC, mass of flue gases flow; dust)
	БДС EN 303-5, cl. 5.8, 
cl. 5.9.4;
БДС EN 13284-1

	
	
	2.2. Surface temperature at nominal and minimum heat output (losses)
	БДС EN 303-5, cl. 5.11 
(cl. 5.9.3.2)

	
	
	2.3. Flue gases temperature at
nominal and minimum heat output
	БДС EN 303-5, cl. 5.6

	
	
	2.4. Heat output/ energy efficiency (losses) at nominal and minimum heat output and determining the boiler class
	БДС EN 303-5, cl. 5.7.1, 
cl. 5.7.2, cl. 5.7.3, cl. 5.7.7, (cl. 5.9.1, cl. 5.9.2, cl. 5.10, 
cl. 5.4, cl.5.5)/ cl. 5.7.6 
(cl. 5.9.3), Annex F

	3.
	Residential solid fuel burning appliances -
Roomheaters
	БДС EN 16510-2-1

	
	
	3.1. Combustion products emissions at nominal heat output, part load heat output and slow combustion (O2; CO2; CO; mass of flue gases flow; NO; NO2; NOx; CxHy; OGC; particulate matter (PM))
	БДС EN 16510-1, cl. A.4.4.2, (cl. A.6.2.6, cl. A.6.2.9, 
cl. A6.2.5);
БДС EN 16510-1, Annex D;
БДС EN 16510-1, Annex E;
БДС EN 16510-1, Annex F

	
	
	3.2. Flue gases temperature
	БДС EN 16510-1, cl. A.2.3.2, cl. A.4.4.3; (cl. A.6.2.10)

	
	
	3.3. Surface temperature
	БДС EN 16510-1, cl. A.4.7

	
	
	3.4. Safety (load-bearing capacity; open operation; temperature safety; safety under natural draught conditions; type pressure for integral boiler; operation of thermal discharge control and safety heat exchanger; safety of roomsealed appliances)
	БДС EN 16510-1, cl. A.4.10 (cl. A.4.10.2, cl. A.4.10.3,
cl. A.4.10.4, cl. A.4.10.5, 
cl. A.6.2.8, cl. A.4.10.6, 
cl. A.4.10.7, cl. A.4.11)

	
	
	3.5. Heat output (nominal heat
output; part load of heat output; slow combustion; combustion recovery; output of the water heater; space heat output; water temperatures and flow rate)/ energv efficiencv (losses))
	БДС EN 16510-1, cl. A.4.7, 
cl. A.4.8, cl. A.4.9, 
cl. A.4.9.4, cl. A.4.5, 
(cl. A.6.2.2, cl. A.6.2.3, 
cl. A.6.2.4, cl. A.2.5)/ 
cl. A.6.2.1 (cl. A.4.4, cl. A.4.6, cl. A.6.2.7)

	4.
	Residential solid fuel burning appliances -
Inset appliances including open fires
	БДС EN 16510-2-2

	
	
	4.1.Combustion products emissions at nominal heat output, part load heat output and slow combustion (O2; CO2; CO; mass of flue gases flow; NO; NO2; NOx; CxHy; OGC; particulate matter (PM))
	БДС EN 16510-1, cl. A.4.4.2, (cl. A.6.2.6, cl. A.6.2.9, 
cl. A6.2.5);
БДС EN 16510-1, Annex D;
БДС EN 16510-1, Annex E; БДС EN 16510-1, Annex F

	
	
	4.2.Flue gases temperature
	БДС EN 16510-1, cl. A.2.3.2, (cl. A.4.4.3, (cl. A.6.2.10)

	
	
	4.3.Surface temperature
	БДС EN 16510-1, cl. A.4.7

	
	
	4.4.Safety (load-bearing capacity; open operation; temperature safety; safety during natural draught operation; type pressure for integral boiler; operation of thermal discharge control and safety heat exchanger; safety of roomsealed appliances; operation of appliances without the doors)
	БДС EN 16510-1, cl. A.4.10 (cl. A.4.10.2, cl. A.4.10.3,
cl. A.4.10.4, cl. A.4.10.5, 
cl. A.6.2.8, cl. A.4.10.6, 
cl. A.4.10.7, cl. A.4.11);
БДС EN 16510-2-2, 
cl. A.4.10.201

	
	
	4.5. Heat output (nominal heat output; part load heat output; slow combustion; combustion recovery; output of the water heater; space heat output; water temperatures and flow rate) / energy efficiency (losses))
	БДС EN 16510-1, cl. A.4.7, 
cl. A.4.8, cl. A.4.9, 
cl. A.4.9.4, cl. A.4.5, 
(cl. A.6.2.2, cl. A.6.2.3, 
cl. A.6.2.4, cl. A.2.5)/ 
cl. A.6.2.1 (cl. A.4.4, cl. A.4.6, cl. A6.2.7)

	5.
	Residential solid fuel burning appliances - Cookers
	БДС EN 16510-2-3

	
	
	5.1.Combustion products emissions at nominal heat output, part load heat output and slow combustion (O2; CO2; CO; mass of flue gases flow; NO; NO2; NOx; CxHy; OGC; particulate matter (PM))
	БДС EN 16510-1, cl. A.4.4.2, (cl. A.6.2.6, cl. A.6.2.9, 
cl. A.6.2.5);
БДС EN 16510-1, Annex D; БДС EN 16510-1, Annex E; БДС EN 16510-1, Annex F

	
	
	5.2.Flue gases temperature;
	БДС EN 16510-1, cl. A.2.3.2, cl. A.4.4.3 (cl. A.6.2.10)

	
	
	5.3. Surface temperatures;
	БДС EN 16510-1, cl. A.4.7

	
	
	5.4.Safety (load-bearing capacity; open operation; temperature safety; safety during natural draught operation; type pressure for integral boiler; operation of thermal discharge control and safety heat exchanger; safety of roomsealed appliances; operation of appliances without the doors)
	БДС EN 16510-1, cl. A.4.10 (cl. A.4.10.2, cl. A.4.10.4,
cl. A.4.10.5, cl. A.6.2.8, 
cl. A.4.10.6, cl. A.4.10.7, 
cl. A.4.11)

	
	
	5.5. Heat output (nominal heat output; part load heat output; slow combustion; combustion recovery; output of the water heater; space heat output; water temperatures and flow rate) / energy efficiency (losses)/ oven temperature; heating the hotplate; heating the oven; oven shelf and oven door)	
	БДС EN 16510-1, cl. A.4.7, 
cl. A.4.8, cl. A.4.9, cl. A.4.9.4, cl. A.4.5, (cl. A.6.2.2, 
cl. A.6.2.3, cl. A.6.2.4, 
cl. A.2.5)/ cl. A.6.2.1 
(cl. A.4.4, cl. A.4.6, 
cl. A.6.2.7);
БДС EN 16510-2-3, 
cl. A.4.301, cl. A.4.301.1, 
cl. A.4.301.2, cl. A.4.301.3,
cl. A.4.301.4, cl. A.4.301.5

	6.
	Residential solid fuel burning appliances - Mechanically by wood pellets fed roomheaters,
inset appliances and cookers
	БДС EN 16510-2-6

	
	
	6.1. Combustion products emissions at nominal heat output, part load heat output and slow combustion (O2; CO2; CO; mass of flue gases flow; NO; N02; NOx; CxHy; OGC; particulate matter (PM))
	БДС EN 16510-1, cl. A.4.4.2, (cl. A.6.2.6, cl. A.6.2.8,
cl. A.6.2.9, cl. A.6.2.5);
БДС EN 16510-1, Annex D;
БДС EN 16510-1, Annex E;
БДС EN 16510-1, Annex F

	
	
	6.2. Flue gases temperature
	БДС EN 16510-1, cl. A.2.3.2, cl. A.4.4.3 (cl. A.6.2.10)

	
	
	6.3. Surface temperatures
	БДС EN 16510-1, cl. A.4.7

	
	
	6.4. Safety (load-bearing capacity; temperature safety; type pressure for integral boiler; operation of thermal discharge control and safety heat exchanger; safety of roomsealed appliances)
	БДС EN 16510-1, cl. A.4.10 (cl. A.4.10.2, cl. A.4.10.4,
cl. A.4.10.6, cl. A.4.10.7, 
cl. A.4.11);
БДС EN 16510-2-6, 
cl. A.4.10, cl. A.4.10.4, 
cl. A.4.10.601, cl. A.4.11

	
	
	6.5. Heat output (nominal heat
output; part load heat output; output of the water heater; space heat output; water temperatures and flow rate)/ energy efficiency (losses)/ oven temperature; heating the hotplate; heating the oven; oven shelf and oven door)
	БДС EN 16510-1, cl. A.4.7, 
cl. A.4.8, cl. A.4.5, 
(cl. A.6.2.2, cl. A.6.2.3, 
cl. A.6.2.4, cl. A.2.5)/ 
cl. A.6.2.1 (cl. A.4.4, 
cl. A.4.6, cl. A.6.2.7);
БДС EN 16510-2-6, cl. A.4.6, cl. A.4.7, cl. A.4.8, A.6.2.1.4/ cl. A.4.601;
БДС EN 16510-2-3, 
cl. A.4.301



To perform sampling of:
	Type of the scope: flexible*

	№ 
	Tested products
	Sampling methods
(standard/validated method)

	1
	2
	3

	1.
	Emissions from combustion products - dust
	БДС EN 13284-1

	2.
	Emissions from combustion products - particulate matter (PM)
	БДС EN 16510-1, Annex F



*Flexible scope: Implementing a new version of standards/documents or standards/ documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by the laboratory.
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