ORDER
№ А 706  
Sofia, 01.12.2020
Inspection Body ELOT of Type C 

at COOPERATION ELOT, Sofia

Management Address: 8 Tzurnook Str, Lozenetz, 1421 Sofia
Office Address: 64 Chataldja Str, Oborishte, 1504 Sofia 
to perform inspection according to the following scope:

	Type of scope: flexible*

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Artificial lighting in work and home environments
	On new and / or operational  sites and equipment
	- Lighting
	Methodical instructions 40-85 "Methods for measurement and assessment of artificial lighting" from 1985, ed. Standardization
CWP:7.1.1.2.
	Ordinance No 49, 

SG, issue 7/1976; 

Ordinance No 9, 

SG, issue 46/1994;

Ordinance No 24, 

SG, issue 95/2003;

Ordinance No 2,

SG, issue 15/2007;

Ordinance No 3, 

SG, issue 15/2007;

Ordinance No 26,

SG, issue 103/2008;

БДС EN 12464-1; 

Instruction No 34, 

SG, issue 82/1975;

ТS.

	2.
	Microclimate in work and home environments
	On new and / or operational  sites and equipment 
	-Air temperature 

-Relative humidity 

-Air velocity
	Ordinance No RD-07-3, SG, issue  63/2014;

БДС 16686;

CWP:7.1.2.3.
	Ordinance  No 9, 

SG, issue 46/1994;
Ordinance  No 24,

SG, issue 95/2003;

Ordinance  No 2, 

SG, issue 15/2007;

Ordinance  No 3, 

SG, issue 15/2007;

Ordinance  No 26, 

SG, issue 103/2008;

BSS 14776;

Instruction No34, 

SG, issue 82/1975;

Ordinance  No RD-07-3,  SG, issue  63/2014; ТS.

	3.
	Noise in work environment
	On new and / or operational  sites and equipment
	- Daily noise exposure level 

- Average weekly noise exposure level 

- Top sound pressure level
	БДС EN ISO 9612;

(БДС ISO 1999)
CWP:7.1.3.2.
	Ordinance  No 6, 
SG, issue 70/2005;

TS.

	
	
	
	- Noise level

- Equivalent noise level
	БДС 15471;

CWP:7.1.3.2.
	Ordinance  No 7, SG, issue  88/1999;

Ordinance  No 9, 

SG, issue 46/1994;

Ordinance  No 26, 

SG, issue 103/2008;

TS.

	4.
	Noise in residential and public buildings 
	On new and / or operational  sites and equipment
	- Equivalent noise level
- Noise level
	БДС 15471;

CWP:7.1.3.2.
	Ordinance  No  6, 

Exhibit No 2, table.1, 

SG, issue 58/2006;

Ordinance  No 9, 

SG, issue 46/1994;

Ordinance  No 2, 

SG, issue 15/2007;

Ordinance  No 24,

SG, issue 95/2003;

Ordinance  No 26, 

SG, issue 103/2008;

TS.

	5.
	Ventilation installations/systems
	On new and / or operational  sites and equipment
	- Air speed flow 

- Flow of ventilation installation
	БДС 12.3.018;

CWP:7.1.4.2.


	Ordinance  No 15, 

SG, issue 68/2005;

Ordinance  No 24, 

SG, issue 95/2003;

Instruction No 34, 

SG, issue 82/1975; ТS.

	6.
	Air-conditioning installations/systems
	On new and / or operational  sites and equipment
	- Relative humidity - Air temperature
	Ordinance  No RD-07-3,  SG, issue 63/2014; БДС 16686; CWP:7.1.5.1.
	Ordinance No RD-07-3,  SG, issue  63/2014; Ordinance  No 15,  SG, issue 68/2005; БДС 14776; ТS.

	7.
	Chemical agents in the air of the working environment
	On new and / or operational  sites and equipment
	- mg / m2 Concentration of the chemical agents in the air of the working environment by linear-colorimetric method with indicator tubes
	БДС EN 482+А1;

БДС EN 689 +АС;

Methodical instructions for determination of toxic gases and vapors in the air of the working environment by linear-colorimetric methods
Vol. 2, Edition 

MA SIHOD Higitest Association, 1987; CWP:7.1.6.5.
	Ordinance  No 13, 

SG, issue 8/2004;

ТS.

	8.
	Electrical installations and equipment up to 1000V
	On new and / or operational  sites and equipment
	-Insulation resistance
	CWP:7.1.8.1.
	Ordinance  No 3,

SG, issue 90, 91/ 2004;

Ordinance  No 16-116, SG, issue 26/2008; Ordinance  No 1, SG, issue 46 /2010; ТS.

	9.
	Electrical installations and equipment up to 1000V
	On new and / or operational  sites and equipment
	-Resistance of protective earthing system
	CWP:7.1.9.1.
	Ordinance  No 3, SG, issue 90, 91/2004; Ordinance  No 16-116, SG, issue 26/2008; Ordinance  No 1, SG, issue 46/2010; TS.

	10.
	Electrical installations and equipment up to 1000V
	On new and / or operational  sites and equipment
	-Circuit impedance "phase-protective conductor ”
	CWP:7.1.10.1.
	Ordinance  No 3,

SG, issue 90, 91/2004; Ordinance  No 16-116, SG, issue 26/2008; Ordinance  No 1, SG, issue 46 /2010; ТS.

	11.
	Electrical installations and equipment up to 1000V
	On new and / or operational  sites and equipment
	Circuit breakers (SB):

- Touch voltage

- Resistance of protective earth

- Switch-off time

- Trigger current
	CWP: 7.1.11.1.
	Ordinance  No 3,

SG, issue 90, 91/2004;

Ordinance  No 16-116, SG, issue 26/2008; Ordinance  No 1, SG, issue 46/2010; ТS.

	12.
	Electrical installations and equipment up to 1000V
	On new and / or operational  sites and equipment
	-Resistance of lightning protection earthing system
	CWP: 7.1.12.1.
	Ordinance  No 4, 

SG, issue 6/2011;

Ordinance  No 16-116,  SG, issue 26/2008; ТS.

	13.
	Electrical installations and equipment up to 1000V
	On new and / or operational  sites and equipment
	- Resistance of earthing switch for protection against electrostatic charges
	CWP: 7.1.13.1.
	Ordinance  No 3, 
SG, issue 90, 91/2004; Ordinance  No 16-116, SG, issue 26/2008; Ordinance  No 4,  SG, issue 6/2011; БДС 15969; ТS.

	14.
	Electrical installations and equipment up to 1000V
	On new and / or operational  sites and equipment
	-Specific soil resistance (Ω.m)
	БДС 15705;

CWP: 7.1.14.1.
	ТS.

	15.
	Electrical installations and equipment over 1000V
	On new and / or operational  sites and equipment
	-Insulation resistance
	БДС 16654;

CWP: 7.1.15.1.
	Ordinance  No 3,

SG, issue 90, 91/2004; Ordinance  No 16-116, SG, issue 26/2008;
ТS

	16.
	Electrical installations and equipment over 1000V
	On new and / or operational  sites and equipment
	- Resistance of protective earthing systems
	CWP: 7.1.16.1.
	Ordinance  No3,

SG, issue 90, 91/2004; Ordinance  No 16-116, SG, issue 26/2008; ТS.

	17.
	Electrical installations and equipment over 1000V
	On new and / or operational  sites and equipment
	-Resistance of lightning protection earthing system
	CWP: 7.1.17.1.
	Ordinance  No 4, 

SG, issue 6/2011;

Ordinance  No 3,

SG, issue 90, 91/2004; Ordinance No 16-116, SG, issue 26/2008; ТS.

	18.
	Cathodic Protection
	On new and / or operational  sites and equipment
	-Determine the presence of stray currents in the ground

-Stationary potential (V)

-Potential difference between primary and secondary metal structures (V)

-Polarization potential (V)

-Direction and strength of protective current (mA)
	БДС 15705;

CWP: 7.1.18.1
	Ordinance on the design, safe operation and technical supervision of pressure equipment, SG, issue 64/2008. (Articles 134, 136, 136, 137, 138 and 139); 

Ordinance on the construction and safe operation of transmission and distribution pipelines and of facilities, installations and devices for natural gas; SG, issue 67/2004;

Ordinance on the design, safe operation and technical supervision of gas facilities and installations for liquefied hydrocarbon gases, SG, issue 82/2004. (Articles 15 and 30); 

БДС 15704; TS.


* The introduction of a new version of standards / documents or standards / documents that replace them is allowed. An up-to-date list of standards / documents with their dated versions is provided by the CAB.

ODSOTSPE – adopted by Council of Ministers Decree No 164/07.07.2008 – Ordinance on the design, safe operation and technical supervision of pressure equipment (SG, issue 64/2008);

OCSOTDGPFIANG – adopted by Council of Ministers Decree No 171/16.07.2004 – Ordinance on the construction, safe operation of the transmission and distribution gas pipelines and of the facilities, installations and appliances for natural gas (SG, issue 67/2004);

ODTSGFILHG – adopted by Council of Ministers Decree No 243/10.09.2004 – Ordinance on the design, safe operation and technical supervision of gas facilities and installations for liquefied hydrocarbon gases (SG, issue 82/2004);

Ordinance  No 4 on the lightning protection of buildings, outdoor facilities and open spaces (SG, issue  6/2011);

Ordinance No 3 on the design of electrical installations and power lines, SG, issue 90 and 91/2004);

Ordinance No 16-116 on the technical operation of electrical equipment (SG, issue 26/2008);

Ordinance No 1 on the design, construction and maintenance of low-voltage electrical installations in buildings (SG, issue 46/2010);

Ordinance No 13 on the protection of workers from risks related to exposure to chemical agents at work (SG, issue 8/2004);

Ordinance No RD-07-03 on the minimum requirements for the microclimate of workplaces (SG, issue 63/2014);

Ordinance No 15 on the technical rules and norms for design, construction and operation of the sites and facilities for production, transmission and distribution of heat energy (SG, issue 68/2005); 

Ordinance No 24 on the sanitary and hygienic requirements for discos (SG, issue 95/2003); 

Instruction 34 on the hygiene of sports facilities and equipment (SG, issue 82/1975); Ordinance No 6 on environmental noise indicators, taking into account the degree of discomfort during different parts of the day, the limit values ​​of environmental noise indicators, the methods for assessing the values ​​of noise indicators and the harmful effects of noise on public health (SG, issue 58/2006)

Ordinance No 9 on the hygiene requirements for the use of personal computers in the education of students (SG, issue 46/1994);

Ordinance No 2 on health requirements for computer and Internet halls for public use (SG, issue 15/2007);

Ordinance No 26 on the structure and operation of kindergartens and children's kitchens and the health requirements to them (SG, issue 103/2008);

"Methodical instructions for determination of toxic gases and vapors in the air of the working environment by linear colorimetric methods", book 2, ed. Medical Academy, Scientific Institute of Hygiene and Occupational Diseases, Hygitest Association, 1987;

Ordinance No 7 on minimum requirements for safe and healthy working conditions at workplaces and when using work equipment (SG, issue 88/1999);

Ordinance No 6 on the minimum requirements for ensuring the health and safety of workers in case of risks related to noise exposure (SG, issue 70/2005);

Ordinance No 3 on the health requirements for kindergartens (SG, issue 15/2007);

Ordinance No 49 on artificial lighting of buildings (SG, issue 7/1976);

Methodical instructions 40-85 "Methods for measurement and evaluation of artificial lighting", publishing house "Standardization", Sofia 1985;

ТS – Technical specification.
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