
ORDER

No. A 46

Sofia, 29.01.2021


INSPECTION BODY OF TYPE C 
at "IKONT-90" LTD, MONTANA  

Management address: 3400 Montana, R.D. "Mladost", bl.29, entr.2, 6th floor, ap.42. P.O. box 42
Office address: 3400 Montana, 74 Treti mart Blvd., 1st floor, office 3



To perform inspection according to the following scope:

	Type of scope: flexible*

	№
	Field of inspection
	Type of inspection
	Parameter of Inspection/
Characteristic
	Test and Measurement Methods used during inspection
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Electrical systems and facilities with rated voltage up to 1000 V
	Inspection of new and/or in-service systems / facilities 
	Resistance of protection and earthing systems
	Inspection Procedure № 16 
	Regulation № 3, (SG issue 90/2004 and issue 91/2004);
Regulation №16-116, (SG issue 26/2008);
TS

	
	
	
	Resistance of lightning protection earthing systems
	Inspection Procedure № 17
	Regulation № 4, (SG issue 6/2011);
TS

	
	
	
	Insulation resistance
	БДС 1986, item 3.3 a), b), e), f);
Inspection Procedure № 15
	Regulation № 3, (SG issue 90/2004 and issue 91/2004);
Regulation №16-116, (SG issue 26/2008);
TS

	
	
	
	Impedance of phase-protective conductor loop 
	Inspection Procedure № 14
	Regulation № 3, (SG issue 90/2004 and issue 91/2004);
Regulation №16-116, (SG issue 26/2008);
TS

	
	
	
	Protection circuit-breakers:
· Contact voltage
· Tripping time
· Tripping current
	Inspection Procedure № 24
	Regulation № 3, (SG issue 90/2004 and issue 91/2004);
Regulation №16-116, (SG issue 26/2008);
TS

	2.
	Artificial lighting systems in industrial and living environment
	Inspection of new and/or in-service systems / facilities
	Illumination
	Methodical instructions for measurement and evaluation of artificial lighting in buildings 40-85, Standardization Publishing House
Inspection Procedure № 19
	Ordinance № 9,
SG issue 46/1994; Ordinance № 24,
SG issue 95/2003; Ordinance № 2,
SG issue 15/2007; Ordinance № 49,
SG issue 7/1976; Ordinance № 26,
SG issue 103/2008; 
БДС EN 12464-1;
TS

	3.
	Microclimate in industrial and living environment
	Inspection of new and/or in-service systems / facilities
	Air temperature; 
Relative humidity; 
Air velocity.
	БДС 16686, 
Ordinance № РД-07-3, SG No. 63/2014 Inspection Procedure № 18
	Ordinance № 9,
SG issue 46/1994; Ordinance № 24,
SG issue 95/2003; Ordinance № 2,
SG issue 15/2007; Ordinance № RD-07-3, SG issue 63/2014;
TS

	4.
	Noise in industrial environment
	Inspection of new and/or in-service systems / facilities
	· Noise level;
· Daily noise exposure level;
· Average weekly noise exposure level;
· Equivalent noise level;
· Peak sound pressure level.
	БДС EN ISO 9612 
(БДС ISO 1999) 
БДС 15471 
Inspection Procedure № 20
	Ordinance № 6,
SG issue 70/2005; Ordinance № 9,
SG issue 46/1994; Ordinance № 7,
SG issue 88/1999; Ordinance № 26,
SG issue 103/2008; 
TS 

	5.
	Noise in premises in residential and public buildings
	Inspection of new and/or in-service systems / facilities
	· Noise level;
· Equivalent noise level.
	БДС 15471
Inspection Procedure № 20
	Ordinance № 6,
SG issue 58/2006; 
Annex 2, Table 1;
Ordinance № 9,
SG issue 46/1994; Ordinance № 24,
SG issue 95/2003; Ordinance № 2,
SG issue 15/2007; Ordinance № 26,
SG issue 103/2008; 
TS 

	6.
	Ventilation systems
	Inspection of new and/or in-service systems/facilities
	Air flow velocity;
Air flow rate.
	БДС 12.3.018 
Inspection Procedure № 21
	Ordinance № 15, 
SG issue 68/2005; 
TS 



* The introduction of a new version of standards/documents or standards/documents that replace them is allowed. An updated list of standards/documents with their dated versions is provided by the CAB.

Ordinance РД-07-3 on the minimum requirements for the microclimate of workplaces (SG, issue 63/2014)
Ordinance № 49 on artificial lighting of buildings (SG, issue 7/1976)
Ordinance № 6 on the minimum requirements for ensuring the health and safety of workers in case of risks related to noise exposure (SG, issue 70/2005)
Ordinance № 6 on environmental noise indicators, taking into account the degree of discomfort during different parts of the day, the limit values of environmental noise indicators, the methods for assessing the values of noise indicators and the harmful effects of noise on the health of the population (SG, issue 58/2006)
Ordinance № 7 on the minimum requirements for healthy and safe working conditions at the workplaces when using the work equipment (SG No. 88/1999)
Ordinance № 2 on the health requirements to the computer and internet halls for public use (SG, issue 15/2007)
Ordinance № 24 on the sanitary and hygienic requirements for discos (SG, issue 95/2003)
Ordinance № 9 on the hygiene requirements for the use of personal computers in the education of students (SG, issue 46/1994)
Ordinance № 26 on the structure and activity of nurseries and children's kitchens and the health requirements to them (SG, issue 103/2008)
Ordinance 3, SG issue 90 and 91/2004 on the design of electrical installations and power lines.
Ordinance 16 - 116, SG issue 26/2008 on technical operation of the energy equipment.
Ordinance 4, SG issue 6/2011 on lightning protection of buildings, outdoor facilities and open spaces.
Ordinance № 15 on the technical rules and norms for design, construction and operation of the systems and facilities for production, transmission and distribution of heat energy (SG issue 68/2005).
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