SCOPE 184 ОКС
[bookmark: _GoBack]Inspection Body of type C
At ELLATZITE MED AD – Mirkovo,

Management and Office address: 
2086 Mirkovo, Sofia-Region

To perform inspection of:
	Scope type: flexible*

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Electrical installations and equipment 
up to 1000V
	New and in operation facilities
	Impedance of the "phase protective conductor" circuit 
	NSU Control Procedure 07.1-1
	Ordinance № 3, 
SG № 90, 91/2004, 
Ordinance № 16-116, SG № 26/2008, Technical Specification

	2.
	Electrical installations and equipment 
up to 1000V
	New and in operation facilities
	Circuit breakers: actuating current and touch voltage
	NSU Control Procedure 07.1-2
	Ordinance № 3,
SG № 90, 91/2004, 
Ordinance № 16-116, SG № 26/2008, Technical Specification

	3.
	Electrical installations and equipment 
up to and above 1000 V
	New and in operation facilities
	Resistance of protective grounding installations
	NSU Control Procedure 07.1-3
	Ordinance № 3,
SG № 90, 91/2004, 
Ordinance № 16-116, SG № 26/2008,
Technical Specification

	4.
	Electrical installations and equipment 
up to and above 1000 V
	New and in operation facilities
	Resistance of lightning protection grounding systems
	NSU Control Procedure 07.1-4
	Ordinance № 3,
SG № 90, 91/2004, 
Ordinance № 16-116, SG № 26/2008,
Ordinance № 4, 
SG № 6/2011, Technical Specification

	5.
	Cable power lines for voltages up to 20kV
	New and in operation facilities
	The integrity of the cores and their phasing-in
	БДС 2374
	Ordinance № 3, SG № 90, 91/2004, 
Ordinance № 16-116, SG № 26/2008,
STEME 1995, Technical Specification

	
	
	
	Insulation resistance
	БДС 1986 - items 3.3 a), b), E) and f)
	Ordinance № 3, SG № 90, 91/2004, 
Ordinance № 16-116, SG № 26/2008,
STEME 1995, Technical Specification

	
	
	
	Insulation with increased DC voltage or voltage with industrial frequency
	БДС 2406
	Ordinance № 3, SG № 90, 91/2004,
 Ordinance № 16-116, SG № 26/2008,
STEME 1995, Technical Specification

	6.
	Electrical protection means: insulating rods, measuring rods, insulating pliers, insulating rods for portable earthing device, voltage indicators, dielectric gloves, dielectric boots and galoshes
	commissioned products
	Electric strength (leakage voltage and current)
	Ordinance № 22 SG № 45/2006 БДС 16972
	Ordinance № 22,
 SG № 45/2006, 
Technical Specification

	7.
	Transformers up to 35 kV
	New and in operation facilities
	Insulation resistance
	БДС 15320, БДС 16654
	Ordinance № 16-116, SG № 26/2008.
STEME 1995, Technical Specification

	
	
	
	Active resistance of the windings
	БДС 15320
	Ordinance № 16-116, SG № 26/2008.
STEME 1995, Technical Specification

	
	
	
	High-voltage insulation with industrial frequency
	БДС 16249
	Ordinance № 16-116, SG № 26/2008.
STEME 1995, Technical Specification

	
	
	
	Breakdown voltage of transformer oil
	БДС EN 60156
	Ordinance № 16-116, SG № 26 /2008 
STEME 1995, 
Technical Specification

	8.
	Electric motors for direct and alternating current up to and above 1000 V
	New and in operation facilities
	Insulation resistance, active winding resistance
	БДС 6949
STEME 1995
	Ordinance № 16-116, SG № 26/2008.
STEME 1995, Technical Specification

	
	
	
	High-voltage insulation with industrial frequency
	БДС 15701
	Ordinance № 16-116, SG № 26 /2008 
STEME 1995, 
Technical Specification

	9.
	Power switches and disconnectors UP TO 20 kV
	New and in operation facilities
	Insulation resistance and transient resistance of the movable contacts
	STEME 1995
	Ordinance № 16-116, SG № 26/2008, Technical Specification

	
	
	
	High-voltage insulation with industrial frequency
	БДС 15701
	Ordinance № 16-116, SG № 26/2008.
STEME 1995, Technical Specification

	10.
	Busbars, post insulators and bushing insulators 
up to and above 1000 V
	New and in operation facilities
	Insulation resistance and high-voltage insulation with industrial frequency
	БДС 3637
БДС 15701
	Ordinance № 16-116, SG, № 26/2008,
STEME 1995, Technical Specification


*Flexible scope: Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.
References:
Ordinance № 3. SG, Issue № 90 and 91/2004 - on the design of electrical installations and electric power lines
Ordinance № 16 - 116, SG № 26/2008 - on the technical operation of the energy equipment
Ordinance № 4, SG, № 6/2011 - on the lightning protection of buildings, outdoor facilities and open spaces.
in the use of personal computers in the education of students (SG, № 46/1994)
Ordinance № 22 on testing of electrical protective equipment in operation (SG, № 45/2006);
STEME-1995 - Standards for Testing of Electrical Machinery and Equipment - of the Energy Committee
TS - Technical Specification
1797 Sofia, Dr. G.M. Dimitrov Blvd. 52 A, floor 7
Tel. 02 976 6401, Fax: 02 976 6415
e-mail: office@nab-bas.bg



EA BAS						             	Page 2/2

