[bookmark: _GoBack]SCOPE 43 ОКС

Inspection Body of type C at ELIT OOD, Shumen
Management and Office address: 9700 Shumen, 49 Tsar Ivan Aleksandar Str.

To perform inspection of:
	Type of the scope: flexible*

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Electrical installations and equipment for voltages up to and above 1000 V
	Initial and/or periodic of new and/or operating sites/equipment
	Insulation resistance
	Ordinance № RD-02-20-1 
(SG № 53/2018)
Standards for testing of electrical machines and equipment (NIEMS) – 1995
БДС 13910;
БДС 2406; БДС 15089
Procedure P-1 (П-1)
	Ordinance № 3 
(SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008)
TS

	
	
	
	Electrical strength insulation of electrical equipment up to 20 kV by high voltage testing with industrial frequency
	БДС 15701; 
БДС 15235
Procedure P-1 (П-1)
	Ordinance № 3 
(SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008)
NIEMS – 1995; TS

	
	
	
	Resistance of earthing protection systems
	Ordinance № RD-02-20-1 
(SG № 53/2018)
Procedure P-1 (П-1)
	Ordinance № 3 
(SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008)
Ordinance № 21 
(SG № 41/2007
БДС 15969; TS

	
	
	
	Resistance of lightning protection earthing systems
	Procedure P-1 (П-1)
	Ordinance № 16-116
(SG № 26/2008) 
Ordinance № 4
(SG № 6/2011); TS

	2.
	Electrical installations and equipment for voltages up to 1000 V
	Initial and/or periodic of new and/or operating sites/equipment
	“Phase – protective conductor" circuit impedance
	Ordinance № RD-02-20-1 
(SG № 53/2018)
Procedure P-2 (П-2)
	Ordinance № 3 
(SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008); TS

	
	
	
	Circuit breaker for zero sequence currents (ground fault interrupters
 Fi circuit breakers): 
– Trigger current;
· Contact Voltage;
- Shutdown time.
	Ordinance № RD-02-20-1 
(SG № 53/2018)
Procedure P-2 (П-2)
	Ordinance № 3 
(SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008)
TS

	3.
	Cable power lines for voltages up to and above 1000 V 
	Initial and/or periodic of new and/or operating sites/equipment
	Insulation resistance
	Ordinance № RD-02-20-1 
(SG № 53/2018)
БДС 1986, item 3.3 а), b), e) and f)
Procedure P-3 (П-3)
	Ordinance № 3 
(SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008)
NIEMS – 1995 ; TS

	4.
	Cable power lines for voltages up to 20 kV
	Initial and/or periodic of new and/or operating sites/equipment
	Electrical insulation strength by testing with high constant voltage
	Ordinance № RD-02-20-1 
(SG № 53/2018)

БДС 2406
NIEMS – 1995
Procedure P-4 (П-4)
	Ordinance № 3 (SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008)
NIEMS – 1995; TS

	5.
	Transformers: – Power, measuring transformers.
	Initial and/or periodic of new and/or operating sites/equipment
	Insulation resistance of the windings
	БДС 16654
Procedure P-5 (П-5)
	Ordinance № 3 (SG № 90 and 91/2004)
Ordinance № 16-116 (SG № 26/2008)
NIEMS – 1995; TS

	
	
	
	Breakdown voltage of transformer oil
	БДС EN 60156
Procedure P-5 (П-5)
	

	6
	Electrical protective equipment:

	6.1
	Insulating rods of all kinds (manipulating, measuring, portable earthing rods); 
Insulating pliers;
Electric measuring pliers for voltage above 1 kV;
Devices for remote
piercing (cutting) of cables.
	Products in operation
	Electrical insulation strength by control with high voltage with industrial frequency
	Ordinance № 22 
(SG № 45/2006)
Procedure P-6 (П-6)
	Ordinance № 22 
(SG № 45/2006)
TS

	6.2
	Dielectric gloves; Dielectric ankle boots, boots and aloshes.
	Products in operation
	– Electrical insulation strength by control with high voltage with industrial frequency;
– Leakage current.
	Ordinance № 22
(SG № 45/2006)
Procedure P-6 (П-6)
	Ordinance № 22 
(SG № 45/2006)
TS

	6.3
	Voltage indicators; Voltage indicators for checking phase matching (phasing).
	Products in operation
	– Electrical insulation strength by control with high voltage with industrial frequency;
– Threshold voltage.
	Ordinance № 22 
(SG № 45/2006)
Procedure P-6 (П-6)
	Ordinance № 22 
(SG № 45/2006)
TS

	7.
	Physical environmental factors:

	7.1
	Microclimate in working and living environment
	Initial and/or periodic of new and/or operating sites/equipment
	– air temperature;
– relative humidity;
– air velocity;
	Ordinance № RD-07-3 
(SG № 63/2014)
 БДС 16686
Procedure P-7 (П-7)
	Ordinance № РД-07-3 
(SG № 63/ 2014)
Ordinance № 2
(SG № 15/2007)
Ordinance № 3
(SG № 15/2007)
Ordinance № 9
(SG № 46/1994)
Ordinance № 24 
(SG № 95/2003)
Ordinance № 26
(SG № 103/2008) :
БДС 14776; TS

	7.2
	Artificial lighting in working and living environment
	Initial and/or periodic of new and/or operating sites/equipment
	Lighting
	Methodical instructions for measurement and evaluation of artificial lighting in buildings 40–85, publishing house "Standardization", 1985.
Procedure P-8 (П-8)
	БДС EN 12464-1
Ordinance № 049 
(SG № 7/1976)
Ordinance № 2 
(SG № 15/2007)
Ordinance № 3
(SG № 15/2007)
Ordinance № 9 
(SG № 46/1994)
Ordinance № 24 
(SG № 95/2003)
Ordinance № 26 
(SG № 103/2008); TS

	7.3
	Noise in the working environment
	Initial and/or periodic of new and/or operating sites/equipment
	· Daily noise exposure leve dBA;
· Weekly avarage noise exposure level dBA;
· Noise level;
· Peak noise pressure level dBC;
	БДС EN ISO 9612
(БДС ISO 1999)
Procedure P-9 (П-9)

	Ordinance № 6
(SG № 70/2005)
TS


	7.4
	Noise in the surrounding environment
	Initial and/or periodic of new and/or operating sites/equipment
	Equivalent noise level
	БДС 15471
Procedure P-9 (П-9)
	Ordinance № 6 
(SG № 58/2006)
Annex 2 table №2); TS

	7.5
	Noise in the premises of residential or public buildings
	Initial and/or periodic of new and/or operating sites/equipment
	– Noise level;
– Equivalent noise level.
	БДС 15471
Procedure P-9 (П-9)
	Ordinance № 6
(SG № 58/2006 –
Annex №2, table № 1)
Ordinance № 2
(SG № 15/2007)
Ordinance № 9
(SG № 46/1994)
Ordinance № 24
(SG № 95/2003)
Ordinance № 26
(SG № 103/2008); TS

	8.
	Vibrations transmitted to the hand–arm system and the whole body;
	Initial and/or periodic of new and/or 
operating sites/equipment
	Daily value of vibrations transmitted to the hand–arm system
	БДС EN ISO 5349-1
БДС EN ISO 5349-2
Procedure P-10 (П-10)
	Ordinance № 3 
(SG № 40/2005)
TS

	
	
	
	Daily value of vibrations transmitted to the whole body
	БДС ISO 2631-1
Procedure P-10 (П-10)
	Ordinance № 3 
(SG № 40/2005)
TS

	9.
	Ventilation systems
	Initial and/or periodic of new and/or operating sites/equipment
	· Air flow rate;
Air flow speed;
	БДС 12.3.018
Procedure P-11 (П-11)
	Ordinance № 15 
(SG № 68/2005)
Ordinance № 24 
(SG № 95/2003)
TS

	10.
	Chemical agents in the air of the work environment
	Initial and/or periodic of new and/or operating sites/equipment
	Dust concentration in the air of the working environment: 
– Inhalable fraction;
Respirable fraction.
	БДС 2200
БДС EN 482
БДС EN 689+АС
Procedure P-12 (П-12)
	Ordinance № 13 
(SG № 8/2004)

Ordinance № 10 
(SG № 94/2003)

	
	
	
	Concentration of chemical agents in the air of the work environment by express linear colorimetric method (using indicator tubes)
	БДС EN 482
БДС EN 689+АС 

Methodical instructions for determination of toxic gases and vapours in the air of the working environment by linear-colometric methods, book 2, publishing house Medical Academy, Research Institute of Hygiene and Occupational Diseases, Hygitest Association, 1987 Procedure P-13 (П-13)
	Ordinance № 13 
(SG № 8/2004)

Ordinance № 10 
(SG № 94/2003)



*Flexible scope: Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.

References:
Ordinance № 49 – on the artificial lighting of the buildings (SG № 7/1976);
Ordinance № 2 – on the health requirements for the computers and internet halls for public use (SG № 15/2007);
Ordinance № 24, SG № 95/2003 on the sanitary and hygienic requirements for discotheques (SG № 95/2003);
Ordinance № 9 – on the health and hygiene requirements for the use of non-personal computers in the education and extracurricular activities of students (SG № 46/1994);
Ordinance № 3 – on the health requirements for the kindergartens (SG № 15/2007;
Ordinance № 26 on the structure and activity of nurseries and children's kitchens1 and health requirements for them (SG № 103/2008);
Ordinance № 6 – on the minimum requirements for ensuring the health and safety of workers in case of risks related to noise exposure (SG № 70/2005);
Ordinance № РД-07-3 – on the minimum requirements for the microclimate of the workplaces (SG № 63/2014);
Ordinance № 6 – on the indicators of noise in the environment, taking into account the degree of discomfort during the different parts of the day, the limit values of the indicators for noise and the harmful effects of noise on the health of the population (SG № 58/2006);
Ordinance № 15 on the technical rules and norms for design, construction and operation of the sites and facilities for production, transmission and distribution of heat energy (SG № 68/2005);
Ordinance № 3, SG № 40/2005 for the minimum requirements for ensuring the health and safety of the workers from the risks associated with exposure to vibration.
Ordinance № 13 – for protection of workers from risks related to the operation with chemical agents while working (SG № 8/2004);
Ordinance № 4 on the lightning protection of buildings, external facilities and open spaces (SG № 6/2011);
Methodical instructions for determination of toxic gases and vapours in the air of the working environment by linear-colometric methods, book 2, publishing house Medical Academy, Research Institute of Hygiene and Occupational Diseases, Hygitest Association, 1987;
Methodical instructions for measurement and evaluation of artificial lighting in buildings 40–85, Collection of methods of the National Centre for Hygiene, Medical Ecology and Nutrition, volume IV, publishing house “Standartization”, 1985.
NIEMS - 1995 Standards for testing of electrical machines and equipment, 1995 of the Energy Committee, Arges Publishing House;
Ordinance № 16-116 for technical operation of the energy equipment (SG № 26/2008);
Ordinance № 3 on the electrical installations design and power lines (SG № 90/2004, issue № 91/2004);
Ordinance № 22 for testing of electrical protective equipment in operation (SG № 45/2006);
Ordinance № RD-02-20-1 for technical rules and standards for inspection and acceptance of electrical and technical works;
Ordinance № 21 regulations for installation of mobile communication networks and equipment (SG № 41/2007)
Ordinance № 10 for safety of workers in case of risks related to carcinogens and mutagens exposure at work. (SG 94/2003)
TS – Technical specification of the client.
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