
ORDER 
No.  А 258 
Sofia, 29 April 2021
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PROCONTROL LTD, LOVECH
TYPE C INSPECTION BODY

Management address and office address:
7 Ivan Drasov Str., Lovech

To perform inspection of:
	Type of scope: flexible *


	№
	Field of Inspection
	Type of Inspection
	Parameter of inspection/
Characteristic
	Test and Measurement methods used for Inspection
	Regulations, Standards, Specifications, Schemes


	1
	2
	3
	4
	5
	6

	1.
	Electrical installations and equipment up to 1000 V;
	New and/ or in use  sites / facilities
	Electrical insulation resistance
	Ordinance No. RD-02-20-1,
SG no. 53/2018
БДС 1986 it.3.3 a), b), e) and f)
ПК 01

	Ordinance No. RD-02-20-1, SG No. 53/2018;
Ordinance No.3, SG no. 90/2004 and 91/2004; Ordinance No.16-116, SG No. 26/2008;

	2.
	Electrical installations and equipment up to and over 1000 V;
	New and/ or in use  sites / facilities
	Resistance of protective earthing systems
	Ordinance No. RD-02-20-1,
SG no. 53/2018
ПК 02
	Ordinance No.3, SG no. 90/2004 and 91/2004; Ordinance No.16-116, SG No. 26/2008;
Technical specifications

	3.
	Electrical installations and equipment up to and over 1000 V;
	New and/ or in use  sites / facilities
	Resistance of lightning protection earthing systems
	Ordinance RD-02-20-1, SG no. 53/2018
ПК 02
	SG no. 90/2004 and 91/2004; Ordinance No.16-116, SG No. 26/2008;
Ordinance No. 4, SG No. 6/2011
Technical specifications

	4.
	Electrical installations and equipment up to 1000 V;
	New and/ or in use  sites / facilities
	Impedance of the circuit “phase - protective conductor” or “phase – con-ductor PEN”
	Ordinance RD-02-20-1, SG no. 53/2018

ПК 03
	Ordinance No.3, SG no. 90/2004 and 91/2004;
Ordinance No. 16-116 (SG, 26/2008); Technical specifications

	5.
	Electrical installations and equipment up to 1000 V;
	New and/ or in use  sites / facilities
	Functionality of circuit breakers for currents with zero
sequence (RCD) in TN and TT circuits:
- Contact voltage (V);
- Shutdown time (ms);
- Actuation current (mA);
	Ordinance No. RD-02-20-1, SG no. 53/2018

ПК 08
	Ordinance No.3, SG no. 90, 91/2004;
Ordinance No. 16-116 (SG, 26/2008); Technical specifications

	
	
	
	- Contact voltage (V);
- Shutdown time (ms);
- Switch-off current (mA);
Non-tripping current
	Ordinance No. RD-02-20-1, SG no. 53/2018

ПК 08
	Ordinance No. RD-02-20-1, SG no. 53/2018



	6.
	Artificial lighting 

	New and/ or in use  sites / facilities
	illumination

	Methodical instructions for measurement and assessment of artificial lighting in buildings, 1985;
ПК 04
	Ordinance No. 49 (SG, 7/1976); Ordinance No. 24 (SG, 95/2003); Ordinance No. 9 (SG, 46/1994);
Ordinance No. 2 (SG, 15/2007);
Ordinance No. 3 (SG, 15/2007);
Ordinance No. 26 (SG, 103/2008);
 BDS 12464-1;
Technical specifications

	7.
	Microclimate
	New and/ or in use  sites / facilities
	1. Air tempera-ture; ° С 
2. Relative humidity of air, %;
3. Air velocity, m/s 

	Ordinance No. RD-07-3,
SG No. 63/2014 
БДС 16686;
ПК 06 

	Ordinance No.3,
SG No. 15/2007; Ordinance No.9,
SG No. 46/1994; Ordinance No.2,
SG no. 15/2007; Ordinance No.24,
SG No. 95/2003 Ordinance No.RD-07-3, SG No. 63/2014; Ordinance No. 26 SG, no. 103/2008;
БДС 14776;
Technical specifications

	8.
	Ventilation
installations
	New and/ or in use  sites / facilities
	1. Air flow rate, m/s;
2. Flow rate of the installation, m3/h 
	БДС 12.3.018; 
ПК 07
	Ordinance No. 15, SG No. 68/2005; Ordinance No. 24, SG No. 95/2003; 
Technical specifications

	9.
	Air conditioning installations
	New and/ or in use  sites / facilities
	1. Relative air humidity, %;
2. Air temperature °С 
	Ordinance No. RD-07-3, SG No. 63/2014 
БДС 16686;
ПК 05 
	Ordinance No. 15, SG No. 68/2005; Ordinance No. RD-07-3, SG No. 63/2014; 
БДС 14776;
Technical specifications


* The introduction of a new version of standards/documents or standards/documents that replace them is allowed. An updated list of standards/documents with their dated versions is provided by the conformity assessment bodies.

Ordinance No. 3 of 9 June, 2004 on the structure of electrical installations and power lines /OSEIPL/ - Issued by the Minister of Energy and Energy Resources, Promulgated SG No. 90 of 13 October, 2004, SG No. 91 of 14 October, 2004;
Ordinance No. 4 of 22 December 2010 on the lightning protection of buildings, outdoor facilities and open spaces was issued by the Ministry of Regional Development and Public Works and promulgated in the SG No. 6 of 18 January, 2011;
Ordinance No. 16-116 of 8 February 2008 on technical operation of energy equipment (Promulgated, SG No. 26 of 07.03.2008;
Ordinance No. 49 on the artificial lighting of buildings /OALB/ - Promulgated SG No. 7/1976;
Ordinance No. 24 of 20.10.2003 on the sanitary and hygienic requirements for discos, Promulgated SG No. 95/2003;
Ordinance No. 9 of 28.05.1994 on the health and hygiene requirements for the use of personal computers in the education and extracurricular activities of students, Promulgated SG No. 46/1994;
Ordinance No. 2 of 5.02.2007 on the health requirements to the computer and internet halls for public use, Promulgated SG No. 15/2007;
Ordinance No. 3 on the health requirements for kindergartens, Promulgated SG no. 15/2007;
Ordinance No.RD-07-3 of 18.07.2014 on the minimum requirements for the microclimate of workplaces, Promulgated SG No. 63/2014;
Ordinance No.15 on the technical rules and regulations for design, construction and operation of sites and facilities for heat generation, transmission and distribution, Promulgated SG No. 68/2005;
Methodical instructions for measurement and evaluation of artificial lighting in buildings, 40-85, ed. Standardization, 1985;
Ordinance No. RD-02-20-1 of 12 June 2018 on the technical rules and regulations for control and acceptance of electrical works, Promulgated SG No. 53/2018




