

ORDER

№ A 742

Sofia, 30.11.2021


Inspection Body of type C, SLAY,
At  Occupational Medicine Service ― SLAY 2008 Ltd, Sofia

Management and Office address: 
1836 Sofia,”Levski-Zone B”, Residential District, 95 Stanislav Dospevski Str. Bl.44, office 1


To perform inspection of:
	Type of the scope: flexible*

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Work environment microclimate
	Control over new and operational units and facilities
	Air temperature, air relative humidity and velocity of air movement
	БДС 16686
Ordinance № PD-07-3, 
SG  63 /01.08.2014 Control Procedure (CP) 01
	Ordinance № PD-07-З/ 
SG  63/ 01.08.2014 Ordinance № 9, 
SG, 46/ 1994
Ordinance № 24, 
SG, 95/ 2003
Ordinance № 2, 
SG, 15/ 2007
Ordinance № 3, 
SG, 15/2007
Instruction № 34 of the Ministry of Public Health, SG, 82/ 1975
Ordinance № 26, 
SG, 103/ 2008; 
CTS

	2
	Artificial lighting in work and household environment
	Control over new and operational units and facilities
	Illumination
	Methodological guidance on the measurement and assessment of artificial lighting of buildings, 40-85 ‘Standardization’ Publishing House, 1985
CP 02
	Ordinance № 49, 
SG, 7/ 1976
БДС EN 12464-1
Ordinance № 9, 
SG, 46/ 1994
Ordinance № 24, 
SG, 95/ 2003
Ordinance № 2,
 SG, 15/ 2007
Ordinance № 3, 
SG, 15/ 2007
Instruction № 34 of the Ministry of Public Health, SG, 82/ 1975
Ordinance № 26, 
SG, 103/ 2008; 
CTS

	3
	Noise
	
	
	
	

	3.1
	Work environment noise
	Control over new and operational units and facilities
	Daily level of exposure to noise, average weekly exposure to noise, peak level of sound pressure
	БДС ISO 1999 
(БДС EN ISO 9612) 
CP 09 CP 10
	Ordinance № 6, 
SG, 70/ 2005; 
CTS

	B)
	Noise in the premises of residential and public buildings
	Control over new and operational units and facilities
	Level of noise, equivalent level of noise
	БДС 15471
CP 03
	Ordinance № 6,
SG, 58/ 2006, Supplement № 2, 
table 1 
Ordinance № 9, 
SG, 46/ 1994 
Ordinance № 24, 
SG, 95/ 2003
Ordinance № 2, 
SG, 15/ 2007
Ordinance № 26, 
SG, 103/ 2008; 
CTS


	C)
	Environmental noise - various territories and structural zones in urbanized territories and outside them
	Control over new and operational units and facilities
	Level of noise, equivalent level of noise
	БДС 15471
CP 03
	Ordinance № 6, 
SG, 58/ 2006, Supplement № 2, 
table 2; 
CTS

	4.
	Electrical installations and facilities up to 1000 V
	Control over new and operational units and facilities
	4.1. Resistance of the ‘phase - protected conductor’ loop impedance Zs
	Ordinance № PD- 02-20-1
(SG, 53/ 2018)
CP 04
	Ordinance № 16-116
(SG, 26/ 2008)
Ordinance № 3
(SG, s 90 and 91/ 2004); 
CTS


	
	
	
	4.2. Resistance of protective earthing installation
	Ordinance № PD- 02-20-1
(SG, 53/ 2018) 
CP 05
	Ordinance № 16-116
(SG, 26/ 2008)
Ordinance № 3
(SG, 90 and 91/ 2004)
CTS

	
	
	
	4.3. Resistance of lightning-protective earthing installation
	Ordinance № PD- 02-20-1 
(SG, 53/ 2018) 
CP 06
	Ordinance № 4, 
SG, 6/ 2011; 
CTS


	
	
	
	Resistance of insulation
	Ordinance № PD- 02-20-1 
(SG, 53/ 2018) 
БДС 1986 item 3.3, a), b), e) and f) 
CP 11
	Ordinance № 16-116 (SG, 26/ 2008)
Ordinance № 3 
(SG, 90 and 91/ 2004)
CTS

	
	
	
	Protective breakers for currents of zero sequence - actuating current; - contact voltage
	Ordinance № PD- 02-20-1
(SG, 53/ 2018)
 CP 12
	Ordinance № 16-116 (SG, 26/ 2008)
Ordinance № 3 
(SG, s 90 and 91/ 2004);
CTS

	5.
	Ventilation installations
	Control over new and operational units and facilities
	Airflow velocity
Airflow rate
	БДС 12.3.018
CP 07
	Ordinance № 15, 
SG, 68/ 2005
Ordinance № 24, 
SG, 95/ 2003; 
CTS



*Flexible scope: Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.

References:
Ordinance № PD-07-03 on the minimum requirements for the microclimate of workplaces (SG № 63 / 2014);
Ordinance № 9 on hygiene requirements regarding the use of personal computers in school training (SG № 46/1994); 
 Ordinance № 24 on sanitary and hygienic requirements for discotheques (SG № 95/2003);
Ordinance № 2 on the health requirements for computer and internet halls for public use (SG № 15/2007);
Ordinance № 3 on the health requirements for kindergartens (SG № 15/2007);
Ordinance № 26 on the structure and activity of nurseries and children's takeaway food outlets and the health requirements to them (SG № 103/2008); 
Ordinance № 49 on artificial lighting in buildings (SG № 7/1976);
Ordinance № 6 on the environmental noise indicators measuring the level of discomfort during different parts of the day, the limit values of the environmental noise indicators, the methods for assessing the values of the noise indicators and the harmful effects of noise on the health of the population (SG № 58 / 18 July 2006);
Ordinance № 6 - on the minimum requirements for ensuring the health and safety of workers at risks related to noise exposure (SG № 70/2005); 
Ordinance № 3 (SG № 90 and № 91/2004) on the structure of electrical appliances and power lines;
Ordinance № 16-116 (SG № 26/2008) on the technical operation of energy equipment;
Ordinance № 4 (SG № 6/2011) on the lighting protection of buildings, outdoor ifacilities and open spaces;
Ordinance № PD-02-20-1 on technical rules and norms regarding the control and acceptance of electric installation work (SG № 53/2018)
Ordinance № 15 on technical rules and norms for the design, realisation and operation of facilities for production, transmission and distribution of heat energy(SG № 68/2005);
Instruction № 34 of the ministry of Public Health on sports facilities and equipment hygiene (G № 84/1975);
CTS - Client's Technical Specification.


Methodological guidelines for the measurement of artificial lighting in buildings, 40-85, Standardization Publishing House 1985.
Ordinance № 7 on the minimum requirements for health and safety at work and in the use of work equipment (SG № 88/1999).
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