SCOPE 31 ОКА
[bookmark: bookmark1]of Inspection Body of type A
at Regional Health Inspectorate, Kardzhali

Management and office address: 
6600 Kardzhali, Residential area Baykal, 2 Gen. Vladimir Stoychev Str.

To perform inspection of:
	Type of the scope: flexible *

	№
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Microclimate in the working and living environment
	Initial and/or periodic of new sites/facilities or sites/facilities in use/in operation
	Air temperature; 
Relative air 
humidity;
Air velocity.
	БДС 16686
Ordinance РД-07 3, SG № 63/2014

Inspection procedure
OKA 7.1 ПК 1

	Ordinance № 2,
SG № 15/2007
Ordinance № 3, 
SG № 15/2007 
Ordinance № 9, 
SG № 46/1994
Ordinance № 24, 
G № 95/2003
Ordinance РД-07-3,
SG № 64/2015
БДС 14776
TS

	2.
	Artificial lightning in the working and living environment
	Initial and/or periodic of new sites/facilities or sites/facilities in use/in operation
	Illumination
	Methodology for measuring the artificial lighting of buildings. Collection of methods of the
 National Center for Hygiene, Medical Ecology and Nutrition, Vol. 4, 2002

Inspection procedure
OKA 7.1 ПК 2
	Ordinance № 2, 
SG № 15/2007
Ordinance № 3, 
SG № 15/2007 
Ordinance № 9, 
SG № 46/1994
Ordinance № 24, 
SG № 95/2003
Ordinance 49,
SG № 7/1976
БДС 12464-1
TS

	3.
	Noise in the working environment
	Initial and/or periodic of new sites/facilities or sites/facilities in use/in operation
	Daily level of noise exposure;
Average weekly level of noise exposure
Peak level of noise pressure.
Equivalent noise level;
Noise level.
	БДС EN ISO 9612 (БДС ISO 1999)


БДС 15471

Inspection procedure
OKA 7.1 ПК 3
	Ordinance № 6, 
SG №70/2005

Ordinance № 9, 
SG № 46/1994

TS

	4.
	Noise in the premises of residential and public buildings
	Initial and/or periodic of new sites/facilities or sites/facilities in use/in operation
	Equivalent noise level;
Noise level.
	БДС 15471

Inspection procedure
OKA 7.1 ПК 6
	Ordinance № 6, Appendix 2, Table 1, 
SG № 58/2006
Ordinance № 6, 
SG № 16/1977
Ordinance № 9, 
SG № 46/1944
TS

	5.
	Noise in the environment
	Initial and/or periodic of new sites/facilities or sites/facilities in use/in operation
	Equivalent noise level
	БДС 15471

Inspection procedure
OKA 7.1 ПК 6
	Ordinance № 6, Appendix 2, Table 2, 
SG № 58/2006
TS

	6.
	Vibrations transmitted to the arm-shoulder system
	Initial and/or periodic of new sites/facilities or sites/facilities in use/in operation
	Daily value of expose to vibrations.
	БДС EN ISO 5349-2
БДС EN ISO
5349-1
Inspection procedure
OKA 7.1 ПК 4
	Ordinance № 3, 
SG № 40/2005
TS

	7.
	Ventilation installations
	Initial and/or periodic of new sites/facilities or sites/facilities in use/in operation
	Velocity of air current;
Air debit
	БДС 12.3.018

Inspection procedure
OKA 7.1 ПК 5
	Ordinance № 15, 
SG № 68/2005
TS



*Flexible scope: Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.
References:
Ordinance № 2 - on health requirements for computer and internet room for public use (SG № 15/2007);
Ordinance № 3 - on health requirements for kindergartens (SG № 15/2007);
Ordinance № 24 - on sanitary and hygienic requirements for discotheques (SG № 95/2003);
Ordinance № 9 - on sanitary and hygienic requirements for personal computer use in curricular and extracurricular activities of students (SG № 46/1994);
Ordinance № РД-07-3 - on the minimal requirements for microclimate at workplaces (SG № 63/2014);
Ordinance № 49 - on the artificial lightning of buildings (SG № 7/1976);
Ordinance № 6 - on the minimal requirements for securing the health and safety of people working at risks related to exposure to noise (SG № 70/2005);
Ordinance № 6 - on the indicators of noise in the environment, identifying the level of discomfort during different parts of the day, the threshold values of the indicators of noise in the environment, the methods for assessment of the values of indicators of noise in the environment and of the damaging effects on public health (SG № 58/2006);
Ordinance № 6 - on providing normal acoustic environment at residential and public buildings and places (SG № 16/1977);
Ordinance № 3 - on the minimal requirements for securing the health and safety of people working at risks related to exposure to vibrations (SG № 40/2005);
Ordinance № 15 - on the technical guidelines and regulations for design, construction and operation of sites and facilities for production, transmission and distribution of heat energy (SG № 68/2005);
TS - technical specification of the client.
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