 SCOPE 240 ЛИ
SVILOCELL EAD

Testing Laboratory 

Management address: 5250 Svishtov, West Industrial Area
Laboratory address: 5250 Svishtov, West Industrial Area, Voden Blok, floor 2
To perform testing of:
	Type of the scope: Fixed
	

	№ 
	Tested products
	Type of test / characteristic
	Testing methods
(standard / validated method)

	1
	2
	3
	4

	1.
	Waste water
	1.1. Active reaction (рН)
	БДС EN ISO 10523:2012

	
	
	1.2. Suspended substances / undissolved substances
	БДС EN 872:2006

	
	
	1.3. Chemical Oxygen Demand (COD)
	VLM № 01:2016

	
	
	1.4. Biochemical Oxygen Demand (BOD 5)
	БДС EN ISO 5815-1:2019

	
	
	1.5. Total Phosphorus
	VLM № 02:2016

	
	
	1.6. Total Nitrogen
	VLM № 03:2016


To perform sampling of:
	Type of the scope: Fixed

	№
	Product
	Methods of sampling/ extracting

(standardized/ validated)

	1
	2
	3

	1.
	Waste water
	БДС ISO 5667-10:2020


References:

VLM № 01:2016 Spectrophotometric method for determination of the Chemical Oxygen Demand (COD) in Waste water

VLM № 02:2016 Spectrophotometric method for determination of the total Phosphorus in Waste water

VLM № 03:2016 Spectrophotometric method for determination of the total Nitrogen in Waste water
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