ORDER
№ A 298
Sofia, 29.09.2025

the Inspection Body of Type C
at “LOT-CONSULT” EOOD, Sofia

Management address: 1612 Sofia, Lagera Residential Area, Bl. 36, Fl. 11, Apt. 83
Office address: 1612 Sofia, Lagera Residential Area, 16 Troyanski Prohod Str., Fl. 2, Office 1
[bookmark: _GoBack]

To perform inspection of:

	Type of scope: flexible

	№
	Area of control
	Type of control
	Controlled
parameter/
characteristic
	Test/measurement methods used in control
	Normative acts, standards,
specifications, diagrams

	1
	2
	3
	4
	5
	6n

	1.
	Microclimate in working and living environment
	New and/or in operation sites/facilities
	-Air temperature;
-Relative air humidity;
-Air velocity.
	БДС 16686 
Ordinance № РД-07-3   (SG № 63/2014)
	Ordinance  № 9 
(SG № 46/1994) 
Ordinance № 24 
(SG № 95/2003) 
Ordinance № 2 
(SG № 15/2007) 
Ordinance № 3 
(SG № 15/2007) 
Ordinance № 26 
(SG № 103/2008) 
BSS 14776 
Ordinance № RD-07-3 
(SG № 63/2014) 
Instruction 34                 (SG № 82/1975)
Ordinance RD-02-20-3 (SG № 5/2016)
TC




	2.
	Ventilation​
installations
	New and/or in operation; sites/facilities
	- Air flow velocity;
- Air mass flow.
	БДС 12.3.018
	Ordinance № 15 
(SG № 68/2005)    Ordinance № 24 
(SG № 95/2003), Instruction 34 
(SG № 82/1975) Ordinance RD-02-20-3 
(SG № 5/2016)
TC

	3.
	Noise in
working
environment
	New and/or in operation sites/facilities
	- Daily noise exposure level;
- Average weekly noise exposure level;
- Peak sound pressure level;
	БДС EN ISO 9612 
(БДС ISO 1999)
	Ordinance № 6 
(SG № 70/2005) 
TC

	4.
	Noise in residential and public buildings
	New and/or in operation sites/facilities
	- Equivalent noise level;
- Noise level;
	БДС 15471
	Ordinance № 6,
Appendix № 2, 
Table № 1 
(SG № 58/2006)   Ordinance № 24 
(SG № 95/2003) Ordinance № 6 
(SG № 16/1977) Ordinance № 2 
(SG № 15/2007) Ordinance № 26 
(SG № 103/2008) Ordinance RD-02-20-3 
(SG № 5/2016) 
Ordinance № 7 
(SG № 88/1999) 
Ordinance № 9 
(SG № 46/1994) 
TC


	5.
	Environmental noise - in the various territories and development zones in and 
outside the urbanized territories
	New and/or in operation sites/facilities
	Equivalent noise level


















	БДС 15471
	Regulation № 6, 
Annex № 2, 
Table № 2 
(SG № 58/2006) 
TC

	6.
	Artificial lighting in work and living environment
	New and/or in operation sites/facilities
	Illumination
	Methodological guidelines 40-85 "Methods for measuring and evaluation of artificial lighting in buildings", ed. Standardization 1985
БДС EN 12464-2
	Ordinance № 49 
(SG № 7/1976) 
Ordinance № 24 
(SG № 95/2003)  Ordinance № 9 
(SG № 46/1994)  Ordinance № 2 
(SG № 15/2007)  Ordinance № 3 
(SG № 15/2007)  Ordinance № 26 
(SG № 103/2008) 
BSS EN 12464-1 
Ordinance RD-02-20-3 
(SG № 5/2016) 
Ordinance № 28/ 
(SG № 109/2008) Ordinance № 19 
(SG № 79/2008)  Instruction 34 
(SG № 82/1975)
BSS EN 12464-2 
TC

	7.
	Dust -
inhalable fraction in workplace air
	New and/or in operation sites/facilities
	Concentration
	БДС 2200 
БДС EN 689+AS 
БДС EN 482
	Ordinance № 13
 (SG № 8/2004)   Ordinance № 10
 (SG № 94/2003) 
TC

	8.
	Dust -
respirable fraction in workplace air
	New and/or in operation
sites/facilities
	Concentration
	БДС 2200 
БДС EN 689+AS 
БДС EN 482
	Ordinance № 13 
(SG № 8/2004) 
Ordinance № 10 
(SG № 94/2003) 
TC

	9.
	Chemical agents in the air of the working environment
	New and/or in operation sites/facilities
	Concentration, by linear colorimetric method
	БДС EN 689+AS 
БДС EN 482
	Ordinance № 13 
(SG № 8/2004) 
Ordinance № 10 
(SG № 94/2003) 
TC

	10.
	Electrical installations and equipment up to and above 1000 V
	New and/or in operation sites/facilities
	Resistance of protective earthing systems
	PK 09
	Ordinance № 3,
(SG № 90 and 91/2004) Ordinance № 16-116, 
(SG № 26/2008)  Ordinance № 21 
(SG № 41/2007)
TC

	11.
	Electrical installations and equipment up to 1000 V
	New and/or in operation sites/facilities
	Insulation resistance
	БДС 1986 item 3.3 a), b), e), f)
PK 10
	Ordinance № 16-116, 
(SG № 26/2008); Ordinance №. 3,
(SG № 90 and 91/2004)
TC

	12

	Electrical installations and equipment up to and above 1000 V
	New and/or in operation sites/facilities
	Resistance of lightning protection earthing systems
	PK 11
	Ordinance № 4 
(SG № 6/2011) 
Ordinance № 21 
(SG № 41/2007)
TC

	13.
	Electrical installations and equipment up to 1000 V
	New and/or in operation sites/facilities
	Impedance of the "phase-protective conductor" loop
	PK 12
	Ordinance No. 3
 (SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008) 
TC

	14.
	Electrical installations and equipment up to 1000 V
(Protective
circuit breakers
(ZP)
	New and/or in operation sites/facilities
	- Protective earth resistance;
- Trigger current;
- Shutdown time.
	PK 13
	Ordinance № 3 
(SG № 90 and 91/2004)
Ordinance № 16-116 
(SG № 26/2008) 
TC

















	15.

	Electro
magnetic
fields
	New and/or in operation sites/facilities
	Electric field intensity (10 Hz ≤ f ≤ 400 kHz);
(3 MHz ≤ f ≤ 18 GHz);

Magnetic flux density (magnetic induction) 
0 Hz (5 Hz ≤ f ≤ 400 kHz)

Magnetic field intensity (100 kHz ≤ f ≤ 18 GHz);

Power density (energy flux density)
(300 MHz ≤  f ≤ 18  GHz)
	Methodology for measuring and evaluation of the electromagnetic field in the populated area of transmitting antennas for mobile communication systems.
Collection of methods for hygiene research NCEMEH, volume IV
PK 14
	Ordinance 
№ RD-07-5, 
(SG № 95/2016)
(Council Recommendation 1999/519/EC of 12.07.1999) 
Ordinance № 9
 (SG № 46/1994) Ordinance № 2 
(SG № 15/2007) Ordinance № 9 
(SG № 35/1991) 
TC

	16.
	Physical workload
	Physical
persons
	Dynamic physical activity by heart rate
	Collection of methods for hygiene measurements of the NCEMEH, Vol. II - "Method for telemetric measurement of heart rate during work", 2000.
	Collection of methods for hygiene measurements of the NCEMEH, Vol. II - "Method for telemetric measurement of heart rate during work", 2000.


* The introduction of new version of standards/documents, or standards/documents that supersede them, is permitted. An up-to-date list of standards/documents with their dated versions is provided by the CAB.

Reference: 
Ordinance № 9 on health and hygiene requirements for the use of personal computers in teaching and extracurricular activities of students (SG № 46/1994);
Ordinance № 24 on sanitary and hygiene requirements for disco clubs (SG № 95/2003);
Ordinance № 2 on health requirements for computer and Internet rooms for public use (SG № 15/2007);
Ordinance № 3 on health requirements for kindergartens (SG № 15/2007);
Ordinance № 26 on the organization and operation of nurseries and children's kitchens (SG № 103/2008);
Ordinance RD-07-3 on the microclimate of workplaces (SG № 63/2014);
Ordinance № 15 of 28 July 2005 on technical rules and standards for the design, construction, and operation of facilities and installations for the production, transmission, and distribution of thermal energy (SG № 68/2005);
Ordinance № 7 of 23 September 1999 on the minimum requirements for healthy and safe working conditions at workplaces and the use of work equipment (SG № 88 of 8 October 1999);
Ordinance № 6 on minimum requirements to ensure the health and safety of workers from risks related to noise exposure (SG № 70/2005);
Ordinance № 6 of 26 June 2006 on environmental noise indicators reflecting discomfort level during different parts of the day, limit values of noise indicators in the enviroment, assessment methods of the noise indicators and harmful effects of noise on human health (SG № 58 of 18 July 2006);
Ordinance № 6 on ensuring normal acoustic conditions in residential and public buildings and areas (SG № 16 of 25 February 1977);
Ordinance № 49 on artificial lighting of buildings (SG № 7 of 23 January 1976, amended SG № 64 of 10 August 1976);
Ordinance № 13 of 30 December 2003 on the protection of workers from risks related to exposure to chemical agents at work (SG № 8 of 30 January 2004);
Ordinance № 3 of 9 June 2004 on the arrangement of electrical installations and power lines (SG № 90 of 13 October 2004);
Ordinance № 16-116 of 8 February 2008 on technical operation of energy equipment (SG № 26 of 7 March 2008);
Ordinance № 4 of 22 December 2010 on lightning protection of buildings, external installations and open areas (SG № 6 of 18 January 2011);
Ordinance RD-07-5 of 15 November 2016 on minimum requirements to ensure the health and safety of workers from risks related to exposure to electromagnetic fields (SG № 95 of 29 November 2016);
Ordinance № 9 of 14 March 1991 on maximum permissible levels of electromagnetic fields in populated areas and the determination of sanitary-protective zones around emitting sources (SG № 35 of 3 May 1991);
Collection of Methods for Hygienic Research, NCEMEH, Vol. II – “Method for Telemetric Measurement of Heart Rate During Work,” 2000;
Methodology for Measurement and Assessment of Electromagnetic Fields in the Vicinity of Mobile Communication Antenna Systems, Collection of Methods for Hygienic Research, NCEMEH, Vol. IV;
Methodological Guidelines 40-85 "Methods for Measurement and Assessment of Artificial Lighting in Buildings," Standards Publishing, 1985;
Ordinance RD-02-20-3 of 21 December 2015 on the design, execution, and maintenance of public service buildings in the fields of education and science, healthcare, culture and arts (SG № 5 of 19 January 2016);
Ordinance № 28 of 9 December 2008 on the organization, operation, and nomenclature of pharmacies and medicinal products (SG No. 109 of 23 December 2008);
Ordinance № 19 of 27 August 2008 on the organization and operation of optician services and health requirements (amended title – SG No. 103 of 2011), (SG № 79 of 9 September 2008);
Instruction 34 on hygiene of sports facilities and equipment (SG № 82 of 24 October 1975);
Ordinance № 21 of 11 May 2007 on rules for the construction of mobile telecommunication networks and installations (SG No. 41 of 22 May 2007);
Ordinance № 10 of 26 September 2003 on the protection of workers from risks related to exposure to carcinogens and mutagens at work (SG № 94 of 24 October 2003);
TC – Technical Specification.
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