


ORDER 
No. A 751
Sofia, 07.12.2021
[bookmark: _GoBack]
“PREVENTA CONTROL” LTD, town of Stara Zagora
Inspection body for safety and health control at work of type A

Management address: town of Stara Zagora 6000, 90 „G. S. Rakovski“ Str., 1st floor, apt. 12
Office address: town of Stara Zagora 6000, 90 “G. S. Rakovski” Str., 1st floor, apt. 3

To perform inspection of:
	Scope type: Flexible*

	№

	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	




1




	Electro-
magnetic
fields
	Inspection of new or objects in operation
	Electric field intensity
(20 Hz ≤ f ≤ 400 kHz)

Magnetic flux density 
(magnetic induction)
(0 Hz, B ≤ 2.4 T)
(20 Hz ≤ f ≤ 200 kHz)
	"Methodology for research and evaluation of electromagnetic radiation from video displays"; "Methodology for EMF research in physiotherapy rooms"; "Methodology for research and evaluation of electromagnetic radiation in high voltage substations (ORU and ZRU) and transformer substations"; Collection of Methods for Hygienic Research of the National Center for Hygiene, Medical Ecology and Nutrition, Volume 1 and Volume 4, Section “Non- Ionizing Radiation, Sofia, 1999;  Methodology for measurement and hygienic assessment of permanent magnetic field in a working environment / Collection of methods for hygienic research of the National Center for Hygiene, Medical Ecology and Nutrition, Volume 1, Section "Non-ionizing radiation", Sofia, 1999
БДС EN 50413;
Procedure EMP.1
	Ordinance No. 2, SG, issue 15, 2007;

Ordinance No. 9 SG, issue 46, 1994;

Ordinance RD-07-5,
SG, issue 95, 2016;

COUNCIL RECOMMENDATION
of 12 July 1999 on the limitation of exposure of the general public to electromagnetic fields
(0 Hz to 300 GHz)
(1999/519 / EO); 
Technical Specification

	2.
	Electrical installations and equipment for voltages up to 1000V
	Inspection of new or objects in operation
	Impedance of the phase-protective conductor circuit
	Ordinance
No. RD-02-20-1,
SG, issue 53, 2018;

Procedure E.2
	Ordinance No. 3,
SG, issue 90 and 91, 2004;
Ordinance 
No. 16-116, SG, issue 26, 2008;
Ordinance No. 1,
SG, issue 46, 2010;
Technical Specification

	3.
	Electrical installations and equipment for voltages up to 1000V: Safety switches
	Inspection of new or objects in operation
	Actuation current;

Touch voltage
	Procedure E.3
	Ordinance No. 3,
SG, issue 90 and 91, 2004;
Ordinance 
No. 16-116, SG, issue 26, 2008;
Ordinance No. 1,
SG, issue 46, 2010;
Technical Specification

	4.
	Electrical installations and equipment for voltages up to and over 1000V
	Inspection of new or objects in operation
	Resistance of protective earthing system;

Continuity of conductors and resistance of connections
	Ordinance
No. RD-02-20-1,
SG, issue 53, 2018;

Procedure E.4
	Ordinance No. 3,
SG, issue 90 and 91, 2004;
Ordinance 
No. 16-116, SG, issue 26, 2008;
Ordinance No. 1,
SG, issue 46, 2010;
Ordinance
No. RD-02-20-1,
SG, issue 53, 2018;
PBZREN up to 1000 V, SG, issue 21, 2005;
Technical Specification

	5.
	Electrical installations and equipment for voltages up to and over 1000 V
	Inspection of new or objects in operation
	Resistance of lightning protection earthing system
	Ordinance
No. RD-02-20-1,
SG, issue 53, 2018;

Procedure E.5
	Ordinance No. 4,
SG, issue 6, 2011;
Ordinance 
No. 16-116, SG, issue 26, 2008;
Technical Specification

	6.
	Electrical installations and equipment for voltages up to and over 1000 V
	Inspection of new or objects in operation
	Insulation resistance
	Ordinance
No. RD-02-20-1,
SG, issue 53, 2018;
NIEMS, 1995;
БДС 1986, items 3.3a), b), d) and e);

Procedure E.6
	Ordinance 
No. 16-116, SG, issue 26, 2008;
Ordinance No. 3,
SG, issue 90 and 91, 2004;
Ordinance
No. RD-02-20-1,
SG, issue 53, 2018;
NIEMS, 1995;
Technical Specification

	7.
	Electrical installations and equipment for voltages up to and over 1000 V
	Inspection of new or objects in operation
	Electrical strength of the insulation by increased test voltage up to 50 kV alternating and up to 60 kV constant
	NIEMS, 1995;
БДС 15235;

Procedure E.7
	Ordinance 
No. 16-116, SG, issue 26, 2008;
Ordinance No. 9, SG, issue 72, 2004;
Ordinance No. 3,
SG, issue 90 and 91, 2004;
NIEMS, 1995;
Technical Specification

	8.
	Ventilation installations
	Inspection of new or objects in operation
	Air flow rate;

Air flow
	Guidelines for technical testing of ventilation systems and air heating - NIOTE, Sofia, 1985;
БДС 12.3.018;
Procedure V.8
	Ordinance No. 15, SG, issue 68, 2005;
Ordinance No. 24, SG, issue 95, 2003;
Ordinance
No. RD-02-20-3,
SG, issue 5, 2016;
Technical Specification

	9.
	Noise in the work environment
	Inspection of new or objects in operation
	Daily noise exposure level; Average weekly noise exposure level; 
Noise level; Equivalent noise level;
Peak sound pressure
	БДС EN ISO 9612 (БДС ISO 1999);
БДС 15471;

Procedure SH.9
	Ordinance No. 7, SG, issue 88, 1999, Art. 138;
Ordinance No. 6, SG, issue 70, 2005;
Ordinance No. 9, SG, issue 46, 1994;
Technical Specification

	10.
	Noise in the environment
	Inspection of new or objects in operation
	Noise level; Equivalent noise level
	БДС 15471;

Procedure SH.10
	Ordinance No. 6, SG, issue 58, 2006, Annex No. 2, 
Table No. 2;
Technical Specification

	11.
	Noise in the premises of residential and public buildings
	Inspection of new or objects in operation
	Noise level; Equivalent noise level
	БДС 15471;

Procedure SH.11
	Ordinance No. 6, SG, issue 58, 2006, 
Annex No.2, Table No.1;
Ordinance No. 9, SG, issue 46, 1994;
Ordinance No. 24, SG, issue 95, 2003;
Ordinance No. 2, SG, issue 15, 2007;
Ordinance No. 6, SG, issue 16, 1977;
Technical Specification

	12.
	Vibrations transmitted by the arm-shoulder system
	Inspection of new or objects in operation
	Daily value of vibration exposure
	БДС EN ISO 5349-1;
БДС EN ISO 5349-2;

Procedure В.12
	Ordinance No. 3, SG, issue 40, 2005;
Technical Specification

	13.
	Vibrations transmitted to the whole body

	Inspection of new or objects in operation
	Daily value of vibration exposure
	БДС EN ISO 2631-1;

Procedure В.13
	Ordinance No. 3, SG, issue 40, 2005;
Technical Specification

	14.
	Vibration in living quarters
	Inspection of new or objects in operation
	Vibration acceleration
	Ordinance No. 9, SG, issue 17, 2010;

Procedure В.14
	Ordinance No. 9, SG, issue 17, 2010;
Technical Specification

	15.
	Microclimate in work and living environment
	Inspection of new or objects in operation
	Air temperature;

Relative humidity of the air;

Air velocity
	БДС 16686;
Ordinance
No. RD-07-3,
SG, issue 63, 2014;

Procedure М.15
	Ordinance No. 9, SG, issue 46, 1994;
Ordinance No. 24, SG, issue 95, 2003;
Ordinance No. 2, SG, issue 15, 2007;
Ordinance No. 3, SG, issue 15, 2007;
Ordinance No. 26, SG, issue 103, 2008;
Ordinance
No. RD-07-3,
SG, issue 63, 2014;
Ordinance
No. RD-02-20-3,
SG, issue 5, 2016;
БДС 14776;
Technical Specification

	16.
	Artificial lighting in work and living environment
	Inspection of new or objects in operation
	Illumination
	Methodical instructions
40-85 "Methods for measuring and evaluating artificial lighting", 1985;

Procedure О.16
	Ordinance No. 049, SG, issue 7, 1976;
Ordinance No. 9, SG, issue 46, 1994;
Ordinance No. 24, SG, issue 95, 2003;
Ordinance No. 2, SG, issue 15, 2007;
Ordinance No. 3, SG, issue 15, 2007;
Ordinance No. 26, SG, issue 103, 2008;
Ordinance No. 28, SG, issue 109, 2008;
Ordinance
No. RD-02-20-3,
SG, issue 5, 2016;
БДС EN 12 464-1;
Technical Specification

	17.
	Chemical agents in the air at the workplace
	Inspection of new or objects in operation
	Concentration
of chemical agents in the air of the working environment by linear - colorimetric express method (indicator tubes)
	БДС EN 689+AC;
БДС EN 482

Procedure ХА.17
	Ordinance No. 13, SG, issue 8, 2004;
Ordinance No. 10, SG, issue 94, 2003;
Technical Specification

	18.
	Chemical agents in the air at the workplace
	Inspection of new or objects in operation
	Concentration
powder in the air of the working environment - inhalable fraction
	БДС EN 689+AC;
БДС EN 482;
БДС 2200

Procedure ХА.18
	Ordinance No. 13, SG, issue 8, 2004;
Ordinance No. 10, SG, issue 94, 2003;
Technical Specification



* Introduction of new versions of standards/documents or superseding standards/documents is allowed. An updated list of standards/documents with their dated versions is maintained by the Conformity Assessment Body.


Ordinance No. RD-07-3, SG, issue 63, 2014 for the minimum requirements regarding microclimate at the workplace;
Ordinance No. 2, SG, issue 15, 2007 for the health requirements to the computer and internet halls for public use;
Ordinance No. 3, SG, issue 15, 2007 for the health requirements to the kindergartens;
Ordinance No. 9, SG, issue 46, 1994 for the health and hygiene requirements for the use of personal computers in the teaching and extracurricular activities of students;
Ordinance No. 24, SG, issue 95, 2003 for the sanitary and hygienic requirements to the discos;
Ordinance No. 26, SG, issue 103, 2008 for the structure and activity of nurseries and children's kitchens and the health requirements to them;
Methodical instructions 40-85 "Methods for measuring and evaluating artificial lighting", 1985;
Ordinance No. 049, SG, issue 7, 1976 for artificial lighting of buildings;
Ordinance No. 6, SG, issue 70, 2005 on minimum requirements for ensuring the health and safety of workers from the risks related to noise exposure;
Ordinance No. 6, SG, issue 58, 2006 on environmental noise indicators, taking into account the degree of discomfort during the different parts of the day, the limit values of environmental noise indicators, the methods for estimating the values of noise indicators and the harmful effects of noise on public health;
Ordinance No. 6, SG, issue 16, 1977 to ensure a normal acoustic environment in residential and public buildings and places;
Ordinance No. 7, SG, issue 88, 1999 on the minimum requirements for healthy and safe working conditions at workplaces and when using work equipment;
Ordinance No. 16-116, SG, issue 26, 2008 for technical operation of energy equipment;
Ordinance No. 3, SG, issue 90 and 91, 2004 for the device of electrical installations and power lines;
Ordinance No. 4, SG, issue 6, 2011 for lightning protection of buildings, outdoor facilities and open spaces;
Ordinance No. 1, SG, issue 46, 2010 for design, construction and maintenance of low voltage electrical installations in buildings;
Ordinance No. 9, SG, issue 72, 2004 for the technical operation of power plants and networks;
Ordinance No. 15, SG, issue 68, 2005 for design, construction and operation of sites and facilities for production, transmission and distribution of heat;
Ordinance No. RD-02-20-3, SG, issue 5, 2016 for design, implementation and maintenance of public service buildings in the field of education and science, healthcare, culture and arts;
Ordinance No. 3, SG, issue 40, 2005 on minimum requirements for ensuring the health and safety of workers from the risks related to exposure to vibration;
Ordinance No. 9, SG, issue 17, 2010 for the maximum permissible values of vibrations in residential premises;
Ordinance No. 28, SG, issue 109, 2008 for the structure, order and organization of the work of pharmacies and the nomenclature of medicinal products;
Ordinance RD-07-5, SG, issue 95, 2016 on minimum requirements for ensuring the health and safety of workers from the risks related to exposure to electromagnetic fields;
Ordinance No. 13, SG, issue 8, 2004 to protect workers from risks related to exposure to chemical agents at work;
Ordinance No. 10, SG, issue 94, 2003 to protect workers from risks related to exposure to carcinogens and mutagens at work;
Ordinance No. RD-02-20-1, SG, issue 53, 2018 for technical rules and norms for control and acceptance of electrical installation works;
PBZREN- Regulations for safety and health when working on electrical equipment with voltage up to 1000 V, SG, issue 21, 2005;
NIEMS- Norms for testing electrical machinery and equipment, 1995.




 
