SCOPE 220 ЛИ
Coal testing laboratory at TPP Maritsa East 2 EAD 
Management and Laboratory address: 6265, Kovachevo, Stara Zagora Region
To perform testing of:
	Type of the scope: Flexible

	№ 
	Tested products
	Type of test / characteristic
	Testing methods
(standard / validated method)

	1
	2
	3
	4

	1.
	Lignite /1/
Brown coal /2/
	1.1
Ash
· of dry condition /1,2/
· of operational condition /1,2/
	БДС ISO 1171
БДС ISO 1170

	
	
	1.2 Total moisture /1,2/
	БДС ISO 5068-1

	
	
	1.3 Moisture in a sample for analysis /1,2/
	БДС ISO 5068-2

	
	
	1.4 High calorific value
· of dry condition /1,2/
· of operational condition /1,2/
	БДС ISO 1928

	
	
	1.4 Low calorific value
· of dry condition /1,2/
· of operational condition /1,2/
	БДС ISO 1928

	
	
	1.6 Volatile Matter
· of dry condition /1,2/
· of dry ashless conditionh /1,2/
	БДС ISO 5071-1
БДС ISO 1170

	
	
	1.7 Total sulfur
· of dry condition /1,2/
· of operational condition /12/
	БДС ISO 334
БДС ISO 1170


Flexible scope: Implementing a new version of standards/documents or standards / documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by laboratory.
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