
 ORDER 
№ А 617
  Inspections body "EFFECT CONTROL" of type A at ANGEL LTD, Montana
                                          Registered offICe address:

                                     3400, Montana, 2, Hristo Botev street
                                                    OffICe address:

                                   1225, Sofia, district Orlandovci, 20, Saznanie street

To perform inspection, according to the following scope:

	Scope type: flexible*

	№
	Field of Inspection





	Type of Inspection
	Parameter of Inspection / Characteristic 
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes 

	1
	2
	3
	4
	
	5
	6

	1.
	Electric installations and devices up to and above 1000 V
	Initial /periodic on new and/or in

operation objects and facilities
	Resistance of protective earthing installations
	Ordinance No РД-02-20-1,

SG issue 53/2018 Attachment No 3

ПК-RPEI
	Ordinance No 3, SG issues 90 and 91/2004

Ordinance 16-116, SG issue 26/2008

БДС 3820

TС

	2.
	Electric installations and devices up to and above 1000 V
	Initial /periodic on new and/or in

operation objects and facilities
	Resistance of lightning protection grounding systems


	Ordinance No РД-02-20-1,

SG issue 53/2018 Attachment No 3

ПК-RLPG 


	Ordinance No 4, SG issue 6/2011

Ordinance No 3, SG issues 90 and 91/2004

Ordinance 16-116, SG issue 26/2008

TС

	3
	Electric installations and devices up to 1000 V
	Initial /periodic on new and/or in

operation objects and facilities
	Insulation resistance
	Ordinance No РД-02-20-1,

SG issue 53/2018 Attachment No 2

 БДС 1986

(item 3.3 –a,b,d,e)

ПК-IR
	Ordinance No 3, SG issues 90 and 91/2004

Ordinance 16-116, SG issue 26/2008

Ordinance No1, SG issue 46/2010

Ordinance No РД-02-20-1, SG issue 53/2018, Attachment No 5

Art.13, para 2

TС

	4
	Electric installations and devices up to 1000 V
	Initial /periodic on new and/or in

operation objects and facilities
	Impedance of the phase-protective conductor loop
	Ordinance No РД-02-20-1,

SG issue 53/2018 Attachment No 4

ПК-IPPCL
	Ordinance No 3, SG issues 90 and 91/2004

Ordinance 16-116, SG issue 26/2008

TС

	5
	Electric installations and devices up to 1000 V
	Initial /periodic on new and/or in

operation objects and facilities
	Circuit breakers for protective disconnection, contact voltage, resistance of earthing device, triggering current, break time 
	Ordinance No РД-02-20-1,

SG issue 53/2018 Attachment No 5

ПК - PD
	Ordinance No 3, SG issues 90 and 91/2004

Ordinance 16-116, SG issue 26/2008

Ordinance No1, SG issue 46/2010

Ordinance No РД-02-20-1, SG issue 53/2018, Attachment No 5

TС

	6
	Artificial lighting in work environmentpremises of residential and public buildings
	Initial /periodic on new and/or in

operation objects and facilities
	Illumination
	Methodological guidelines for measurement and evaluation of artificial lighting in buildings 40-85, ed. Standardization, 1985

ПК-I
	Ordinance N9 49, SG no. 7 of 1976 

Ordinance No. 9, SG no. 46 of 1994 

Ordinance No. 24, SG No. 95 of 2003 

Ordinance N°. 2 SG no. 15 of 2007 Ordinance No. 3, SG no. 15 of 2007 Ordinance N9 26, SG no. 103 of 2008 

БДС EN 12 464-1 Ordinance No. Iz -1971, SG no. 96/2009, Art.55 (6)1

Ordinance N9 RD-02-20-3,

SG no. 5/2016, Art.89,

Art.142 (5) (7),

Art.142-Appendix 4;

Art.206, para 4;

Art.207, para s 1 and 2;

Art.217, item 3;

Art.223, Para 4;

Art.231, para 3
Art.233;
Art.234, para 2;
Art.243, para 2 , item Г;

Art.259, art 260
Art.260,

TС

	7
	Microclimate in working environment, premises of residential and public buildings
	Initial /periodic on new and/or in

operation objects and facilities
	Air temperature

Relative air humidity

Air movement speed
	Ordinance No. RD-07-3, SG no. 63 of 2014

БДС 16686

ПК-MC
	Ordinance No 9, SG no 46 of 1994

Ordinance No 24, SG no 95 of 2003

Ordinance No 2, SG no 15 of 2007

Ordinance No 3, SG no 15 of 2007

Ordinance No 26, SG no 103 of 2008

Ordinance No РД-07-3, SG no 63 of 2014

БДС 14776

Ordinance No РД-02-20-3, SG no 5/2016, art.151, item 1- attachment 5; para 10; art 266 item 1, 2, 4, 5

TС

	8
	Noise in

working

environment
	Initial /periodic on new and/or in

operation objects and facilities
	Daily noise exposure level

Average weekly noise exposure level

Peak sound pressure level
	БДС EN ISO 9612 / БДС ISO 1999/

ПК-NWE
	Ordinance No. 6, SG no. 70 of 2006
TС

	9
	Noise in the environment - differences in territories and development zones in urbanized territories and outside them
	Initial /periodic on new and/or in

operation objects and facilities
	Noise level

Equivalent noise level
	БДС 15471
ПК-NE
	Ordinance No. 6

SG No. 58 of 2006, Appendix 2, table 2

TС

	10
	Noise in the premises of residential and public buildings
	Initial /periodic on new and/or in

operation objects and facilities
	Noise level

Equivalent noise level
	БДС 15471

ПК-NRPB
	Ordinance No. 6,

SG no. 58 of 2006, app. 2, tab. 1

Ordinance No. 9,

SG no. 46 of 1994

Ordinance No. 24,

SG no. 95 of 2003

Ordinance N 2

State Gazette, no. 15 of 2007

Ordinance No. 26, SG No. 103 of 2008

Ordinance N9 7, SG no. 88 of 1999

TС

	11
	Ventilation installations
	Initial /periodic on new and/or in

operation objects and facilities
	Velocity of air flow

Air flow rate
	БДС 12.3.018 

ПК-VI


	Ordinance No. 15, SG No. 68 of 2005 

Ordinance No. RD-02-20-3, SG no. 5/2016 

Art.79-table 10; 

Art.87-table 10; 

Art.148 para 2; 

Art.150 item 1; 

Art.151 - Appendix 5; 

Art.153, Item 2 (Appendix 6) 

Art.217-item 6; 

Art.243-para 2, item 1 c; Art.266

Ordinance No 13, SG. 103 of 2016, art.14, para. 1

TС

	12
	Staircases, elevator shafts, fire-protection vestibules, premises with a requirement for increased pressure
	Initial /periodic on new and/or in

operation objects and facilities
	Pressure (elevated, gauge)
	БДС 12.3.018

 ПК-P


	Ordinance No. Iz -1971, SG No. 96/2009, Art.25 (1), Art.50 (2), item 3, Art.79; Art.97; Art.98; Art.291 (1), item 4,  Art.326 (1);

TС

	13
	Air conditioning installations
	Initial /periodic on new and/or in

operation objects and facilities
	Air temperature

Relative air humidity
	Ordinance No. RD-07-3, SG no. 63/2014

БДС 16686

ПК-ACI
	Ordinance No. 15, SG No. 68 of 2005 Ordinance No. RD-07-3, SG no. 63 of 2014 БДС 14776 

TС

	14
	Chemical agents in the air of working environment
	Initial /periodic on new and/or in

operation objects and facilities
	Concentration of chemical agents by linear-colorimetric method /indicator tubes/
	БДС EN 689+АС БДС EN 482 

ПК-ChA
	Ordinance No. 13 SG No. 8/2004 

TС

	15
	Dust
	Initial /periodic on new and/or in

operation objects and facilities
	Dust concentration:

inhalable fraction; respirable fraction
	БДС EN 689+AS БДС EN 482 БДС 2200 

ПК-D
	Ordinance No. 13 SG No. 8/2004

TС

	16
	Electromagnetic fields
	Initial /periodic on new and/or in

operation objects and facilities
	Electric field intensity, V/m; 5Hz≤f≤6GHz

MagnetIC flux density (magnetic induction) T; 5Hz≤f≤ 400kHz

Magnetic field intensity, A/m;

5Hz≤f≤400kHz

Power density µW/cm2

100 kHz≤f≤6 GHz


	Methodology for determining the Hygienic-Protection Zone around objects with EMF, Sb. methods, volume I, NCHMEN, 1999

Methodology for EMF research in physiotherapy offICes, Sb. methods, volume I, NCHMEN, 1999

Methodology for the study of EMF in outdoor switchgear, indoor switchgear and substations, Sb. methods, volume I, NCHMEN, 1999

EMF research methodology from

video displays, Sb. methods, volume I, NCHMEN, 1999

Methodology for measurement and evaluation of the electromagnetIC field in the populated vicinity of transmission antennas to mobile connection systems", Compendium of methods for hygiene studies, NCHMEN Volume IV, 2002, Residential Environment,

Non-Ionizing Radiations, pp. 3-5

БДС EN 50413

БДС EN 62232

(6.3; 6.4; 7;

8.2.2; 9; A.3.3;

A. 3.4; C.2; V.3;

B. 4; E.7; F.5; F.6; F.7) ПК-EMF
	Ordinance РД-07-5,

SG no.95/2016

(Recommendation

1999/519/EU of the Council of 12.07.1999; Assessment and Control of Personnel Exposure to Radio Frequency Fields 3 KHZ-300 GHZ STANAG 234, NATO 13 Feb.l993)

Ordinance No. 2, SG No. 15/2007. 

Ordinance No. 9, SG No. 46/1994. 

Ordinance No. 9 SG No. 35/1991

TС


*Flexible scope: Implementing a new version of standards/documents or standards/documents replacing them is allowed. An updated list of standards/documents and their dated versions is provided by CAB.
Ordinance No. 16-116, SG No. 26/2008 on technical operation of energy equipment 

Ordinance No. 3, SG No. 90 and No. 91/2004 on the design of electrical installations and power transmission lines

Ordinance No. 4, SG No. 6/2011 on the lightning protection of buildings, outdoor facilities and open spaces 
Ordinance No. 1, SG No. 46/2010 on design, construction and maintenance of low voltage electrical installations in buildings.

Ordinance No. 49, SG No. 7/1976 on artificial lighting of buildings 

Ordinance no 9, SG no 46/1994 on the health and hygiene requirements for the use of personal computers in students' learning and extracurricular activities

Ordinance no 24, SG no 95/2003 on sanitary and hygienic requirements for discotheques
Ordinance no 2, SG no 15/2007 about health requirements for computer and internet rooms for public use

Ordinance no 3 SG no 15/2007 about the health requirements for kindergartens

Ordinance no 26, SG no 103/2008 on the organization and activities of nurseries and children’s kitchens

Ordinance no РД-07-3, SG no 63/2014 on the microclimate of workplaces

Ordinance no 6, SG no 70/2005 on the minimum requirements for ensuring health and the safety of workers at risks related to noise exposure
Ordinance no 6, SG no 58/2006г - for environmental noise metrics reporting the extent of discomfort during different parts of the day, the limit values of noise indicators in the environment, in the premises of residential and public buildings, in zones and territories pre-designated for residential construction, recreational zones and territories and zones with mixed use, the methods for assessing the values of noise indicators and the harmful effects of noise on the health of the population

Ordinance no 7, SG no 88/1999 on the minimum requirements for health and safety working conditions at the workplaces and when using the work equipment

Ordinance no 15, SG no 68/2005 on technical rules and regulations for the design, construction and operation of the objects and facilities for the production, transmission and distribution of thermal energy

Ordinance no 13, SG no 8/2004 on protection of workers from risks associated with exposure to chemical agents at work

Ordinance РД-07-5, SG no 95/2016 on the minimum requirements for ensuring the health and safety of workers at risks associated with exposure to electromagnetic fields

Ordinance no 9, SG no 35/1991 on maximum permissible levels of electromagnetic fields in populated areas and determination of hygienic protection zones around emitting objects 

Ordinance no РД-02-20-3 – on the design, implementation and maintenance of buildings for public service in the fields of education and science, health care, culture and the arts (SG no 5/2016);

Ordinance no 1з-1971 – on building and technical rules and norms for ensuring safety in case of fire (SG no 96/2009)

Ordinance no РД-02-20-1 – on technical rules and regulations for control and acceptance of electrical installation works (SG no 53 /2018); 

TС – Technical Specification


