


ORDER

No. A 701

Sofia, 19.12.2022

[bookmark: _GoBack]ELMARK KONTROL INSPECTION BODY – TYPE C
at ELMARK EOOD,  Dobrich

Management address:
9300, city of Dobrich, 4 Dimitar Spisarevski St., entrance A, apartment 6

Office address:
9300, city of Dobrich, 51 25 Septemvri Blvd.

To perform inspection of:

	 Scope type: flexible*

	

No. in order
	

Field of inspection
	

Inspection type
	
Inspected parameter/
characteristic
	Methods of testing/ measurement used for inspection
	Provisions, standards, specifications, inspection schemes

	1
	2
	3
	4
	5
	6

	1.
	Electrical installations and equipment of up to 1000V
	initial and/or periodic inspection; new and/or in use/operation sites/facilities
	Impedance of the “phase - protective conductor” circuit
	ПК 7.1.1-1
	Ordinance No. 3
State Gazette, issue 90 and 91/2004; Ordinance No. 16-116 State Gazette, issue 26/2008);
 TS

	2.
	Electrical installations and equipment of up to 1000 V
	initial and/or periodic inspection; new and/or in use/operation sites/ facilities
	Circuit breakers for zero sequence currenTehnikcal specification, protective earth resistance, actuating current
	ПК 7.1.1-2
	Ordinance No. 3 State Gazette, issue 90 and 91/2004); Ordinance No. 16-116 State Gazette, issue 26/2008; 
TS

	   3.
	Electrical installations and equipment of up to 1000 V
Cable lines
	initial and/or periodic inspection; new and/or in use/operation sites/facilities
	Insulation resistance
	БДС 1986 item 3.3 а), b), е) and f);
ПК 7.1.1-3
	Ordinance No. 3 State Gazette, issue 90 and 91/2004; Ordinance No. 16-116 State Gazette, issue 26/2008; Electrical machinery and equipment testing standards; 
TS

	4.
	Electrical installations and equipment of up to and above 1000 V
	initial and/or periodic inspection; new and/or in use/operation sites/ facilities
	Resistance of an earthing switch of a protective earthing system
	ПК 7.1.1-4
	Ordinance No. 3 State Gazette, issue 90 and 91/2004; Ordinance No. 16-116 State Gazette, issue 26/2008); Rules for safety and health when working on electrical equipment with voltage of up to 1000 V State Gazette, issue 21/2005;  
TS

	5.
	Electrical installations and equipment of up to and above 1000 V



	initial and/or periodic inspection; new and/or in use/operation sites/ facilities
	Resistance of an earthing switch of a lightning protection earthing system
	ПК 7.1.1-5
	Ordinance No. 4 State Gazette, issue 6/2011;
Ordinance No. 3
State Gazette, issue 90 and 91/2004; Ordinance No. 16-116 State Gazette, issue 26/2008; 
TS

	6.
	Electrical installations and equipment of above 1000 V

Cable lines of up to 20kV
	initial and/or periodic inspection; new and/or in use/operation sites/facilities
	Electrical insulation strength with increased DC voltage of up to 60 kV
	БДС 2406;
ПК 7.1.1-6
	Ordinance No. 3 State Gazette, issue 90 and 91/2004; Ordinance No. 16-116 State Gazette, issue 26/2008; Electrical machinery and equipment testing standards; 
TS

	7.
	Electrical protective equipment:

	7.1
	Insulating rods; measuring rods; insulating pliers; current measuring pliers; insulating rods for portable earthing switches
	Periodic inspection; in operation producTehnikcal specification
	Electrical strength of insulation with increased alternating voltage
	Ordinance No. 22
State Gazette, issue 45/2006;
ПК 7.1.1-7
	Ordinance No. 22
State Gazette, issue 45/2006; 
TS

	7.2
	Voltage detectors
	Periodic inspection; in operation producTehnikcal specification
	Electrical strength of insulation with increased alternating voltage; voltage indication threshold /voltage threshold/
	Ordinance No. 22 State Gazette, issue 45/2006;
ПК 7.1.1-7
	Ordinance No. 22 State Gazette, issue 45/2006;
TS

	7.3
	Dielectric gloves, booTehnikcal specification and overshoes
	Periodic inspection; in operation producTehnikcal specification
	Electrical strength of insulation with increased alternating voltage, leakage current
	Ordinance No. 22 State Gazette, issue 45/2006); ПК 7.1.1-7
	Ordinance No. 22 State Gazette, issue 45/2006;
TS

	7.4
	Dielectric maTehnikcal specification
	Periodic inspection; in operation producTehnikcal specification
	Electrical strength of insulation with increased alternating voltage, leakage current
	БДС 9914;
ПК cedure 7.1.1-7
	Ordinance No. 22 State Gazette, issue 45/2006); 
БДС 9914; 
TS



* The introduction of a new version of standards/documents or standards/documents which replace them is allowed. An up-to-date list of the standards/documents with their dated versions is provided by the conformity assessment body.

Ordinance No. 16-116 on the technical operation of energy equipment (State Gazette, issue 26/2008);
Ordinance No. 3 on the design of electrical installations and power lines (State Gazette, issue 90 and issue 91/2004);
Ordinance No. 4 on lightning protection of buildings, outdoor facilities and open spaces (State Gazette, issue 6/2011);
Ordinance No. 22 on the testing of electrical protective equipment in operation (State Gazette, issue 45/2006);
Electrical machinery and equipment testing standards - 1995 - Electrical machinery and equipment testing standards;
TS - Technical specification



