


ORDER

№ A 116

Sofia, 27.02.2023

[bookmark: _Hlk96347950]
INSPECTION BODY OF TYPE C „AS CONTROL”, at „AS CLUB” OOD, city of Sofia

Management and office address:
1202 Sofia, 42 Stefan Stambolov Blvd., apt. 1


To perform inspection of:
	Tyre of scope: flexible*

	№ 
	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic



	Test and Measurement Methods Used                          During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Electrical installations and equipment up to 1000 V
	New and / or in operation sites / facilities
	Resistance of protective earthing systems
	Inspection procedure 7.01
	Ordinance № 3
(SG № 90 and 91/2004)
Ordinance №16-1 16
(SG № 26/2008)
TS

	2.
	Electrical installations and equipment up to 1000 V
	New and / or in operation sites / facilities
	Resistance of lightning protection earthing systems
	Inspection procedure PC 7.02 
	Ordinance № 4 (SG №
6/201 1)
Ordinance №16-1 16 (SG № 26/2008)
TS

	3.
	Electrical installations and equipment up to 1000 V
	New and / or in operation sites / facilities
	Impedance of the "phase- protective conductor" circuit
	Inspection procedure PC 7.03








	Ordinance № 3 (SG № 90 and 91/2004) 
Ordinance № 16-116 (SG 26/2008) 
TS





TS











	4.
	Electrical installations and equipment up to 1000 V
	New and / or in operation sites / facilities
	Circuit breakers:
Trigger current;
Earthing resistance;
Time of shutdown; Tangential voltage.
	Inspection procedure 7.04




	Ordinance № 3
(SG № 90 and 91/2004)
Ordinance № 16-116
(SG No 26/2008)
TS

	5.
	Electrical installations and equipment up to 1000 V
	New and / or in operation sites / facilities
	Insulation resistance
	Inspection procedure 7.05 БДС 1986;
items 3.3 a), b), e) and f)



	Ordinance № 3
(SG № 90 and 91/2004)
Ordinance № 16-116
(SG № 26/2008)
TS

	6.
	Microclimate in work and living environment
	New and / or in operation sites / facilities
	Air temperature;
Relative humidity;
Air velocity.
	БДС 16686;
Ordinance № RD-07- 3 (SG № 63/2014) PC Inspection procedure 7.06 
	БДС 14776; 
Ordinance № 2 (SG № 15/2007)
Ordinance № 3 (SG № 15/2007) 
Ordinance № 9 (SG № 46/1994) 
Ordinance № 24 (SG № 95/2003) 
Ordinance № 26 (SG № 103/2008) 
Ordinance № RD-07-3 (SG № 63/2014) 
TS


	7.
	Artificial lighting in working and household environment
	New and / or in operation sites / facilities
	Stage of lighting
	Methodical instructions for measurement and evaluation of artificial lighting in buildings 40-85, 
Standardization Edition 1985,
Inspection procedure 7.07 
	Ordinance № 49 (SG № 7/1976) 
Ordinance № 9 (SG № 46/1994) 
Ordinance № 24 (SG № 95/2003) 
Ordinance № 2 (SG № 15/2007) 
Ordinance № 3 (SG № 15/2007);
Ordinance № 26 (SG № 103/2008); 
Ordinance № 19 (SG №27/2008);
БДС EN 12464-1;
TS























 
TS

	8.







	Noise in operational environment
	New and / or in operation sites / facilities
	Daily noise exposure level, dBA; 
Average weekly noise exposure level, dBA; 
Peak sound pressure level, dBC 











	БДС EN  ISO 9612;
(БДС ISO 1999)

Inspection procedure 7.08

	Ordinance № 6 (SG № 70/2005);

TS













	9.
	Noise in premises of residential and public buildings
	New and / or in operation sites / facilities
	Noise level, dBA; Equivalent noise level, dBA.

	БДС 15471;  Inspection procedure 7.09









	Ordinance № 6 (SG № 16/1977)
Ordinance № 6, Annex № 2, Table №1 (SG, issue 58/2006)
Ordinance № 7 (SG № 88/1999/art. 138)
Ordinance № 2 (SG № 15/2007)
Ordinance № 9 (SG №
46/1994)
Ordinance № 24 (SG №
95/2003)
Ordinance № 26 (SG № 103/2008) TS





Ordinance № 6 (SG № 16/1977)
Ordinance № 6, Annex № 2, Table №1 (SG, issue 58/2006) Ordinance № 2 (SG № 15/2007)
Ordinance № 9 (SG №
46/1994)
Ordinance № 24 (SG №
95/2003)
Ordinance № 26 (SG № 103/2008) TS
Ordinance № 9 (SG №
46/1994)
Ordinance № 24 (SG №
95/2003)
Ordinance № 26 (SG № 103/2008) TS


	10.
	Noise in the environment – various territories and development zones in urbanized territories and outside them
	New and / or in operation sites / facilities
	Equivalent noise level, dBA;
	БДС 15471;
Inspection procedure 7.10

	Ordinance № 6, Annex № 2, Table № 2 (SG № 58/2006)

	11.
	Ventilation installations
	New and / or in operation sites/ facilities.
	Air flow speed;
Air flow rate
	БДС 12.3.018; Inspection procedure 7.11
	Ordinance № 15 (SG № 68/2005)






Ordinance № 16-116 - For technical operation of the energy equipment (SG № 26/2008);
Ordinance № 3 - On the structure of electrical installations and power lines (SG, issue 90 and 91/2004);
Ordinance № 4 on the lightning protection of buildings, external facilities and open spaces (SG № 6/2011);
Ordinance № 49 - For artificial lighting of the buildings (SG, issue 7/1976);
Ordinance № 2 - on the health requirements for computers and Internet halls for public use (SG № 15/2007);
Ordinance № 24 - on the sanitary and hygienic requirements for discos (SG № 95/2003);
Ordinance № 9 - on the health and hygiene requirements for the use of personal computers in the education and extracurricular activities of students (SG № 46/1994);
Ordinance № 3 - On the health requirements for kindergartens (SG № 15/2007);
Ordinance № 26 - On the structure and activity of nurseries and children's kitchens and the health requirements to them (SG № 103/2008);
Ordinance № RD-07-3 - on the minimum requirements for the microclimate of the workplaces (SG № 63/2014);
Ordinance № 6 on the minimum requirements for ensuring the health and safety of workers in case of risks related to noise exposure (SG № 70/2005);
Ordinance № 6 - For the indicators for environmental noise, taking into account the degree of discomfort during the different parts of the day, the limit values of the environmental noise indicators, the methods for assessment of the values of the noise indicators and the harmful effects of noise on the health of the population (SG № 58/2006);
Ordinance № 15 - On technical rules and norms for design, constructjon and operation of sites
and facilities for production, transmission apd distribution of hear energy (SG № 68/2005);
Ordinance № 6 for ensuring a normal acoustic environment in residential and public buildings and places (SG № 16/1977);
Ordinance № 7 on the minimum requirements for healthy and safe working conditions at workplaces and when using work equipment (SG № 88/1999);
Ordinance № 19 on the organization and operation of opticians, health requirements  for them and the procedure for keeping a register of opticians (SG №27/2008); 
MU 40-85 - Methodical instructions for measurement and evaluation of artificial lighting in buildings 40-85. ed. Standardization, 1985;
TS - technical specification of the customer.
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